(footprint "ESP32_C3_Super_Mini"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
	(tags "Arduino Nano")
	(property "Reference" "U1"
		(at 7.62 -5.08 0)
		(layer "F.SilkS")
		(uuid "38959e10-bc40-4d07-9240-7bb04123c473")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "ESP32_C3_Super_Mini"
		(at 2.54 8.89 90)
		(layer "F.Fab")
		(uuid "ea094d67-e6cb-4c30-b8ee-e63c08d463b2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "f56b765c-2a5f-4d29-b1ba-77014b7d8575")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "ESP32-C3-MINI-1 family is an ultra-low-power MCU-based SoC solution that supports 2.4 GHz Wi-Fi and Bluetooth®Low Energy (Bluetooth LE)."
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8c8631ba-5be3-47aa-b399-de485643363b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.4 -1.27)
		(end -1.27 20.32)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e3801fd6-c87d-4a7a-a2ae-b81c0c749da5")
	)
	(fp_line
		(start -1.27 20.32)
		(end 16.64 20.32)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e55294b4-d9bf-44fc-bc3f-a7205d464d14")
	)
	(fp_line
		(start 1.27 -1.27)
		(end -1.4 -1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5e5f9965-a866-4351-a1a5-3a3552f44fa8")
	)
	(fp_line
		(start 1.27 -1.27)
		(end 1.27 19.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a52bcb08-96ec-4d89-8df3-cbd716c6b8bf")
	)
	(fp_line
		(start 1.27 19.05)
		(end -1.4 19.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "91c389df-33a4-4a32-a5fe-aacc3fd749aa")
	)
	(fp_line
		(start 3.68 -3.94)
		(end 11.56 -3.94)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "73f058cb-b77f-4df3-b8f9-ddec9c8e377f")
	)
	(fp_line
		(start 3.68 5.08)
		(end 3.68 -3.94)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e8d8eb43-12b4-4a4a-95ce-6f9428d5d395")
	)
	(fp_line
		(start 11.56 -3.94)
		(end 11.56 5.08)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2ab94d09-3a8c-4ca4-a297-37bae56a7531")
	)
	(fp_line
		(start 11.56 5.08)
		(end 3.68 5.08)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c3da1926-9137-4680-aabc-a775cca595e9")
	)
	(fp_line
		(start 13.905 -1.27)
		(end 13.97 19.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "16da93c4-a347-474e-aa5a-0aa94df929ad")
	)
	(fp_line
		(start 13.905 -1.27)
		(end 16.575 -1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "141589a9-f89e-4547-b02a-dc48baf9b0fc")
	)
	(fp_line
		(start 13.97 19.05)
		(end 16.64 19.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ea1cb801-311a-40a1-9285-ea8affdbae70")
	)
	(fp_line
		(start 16.64 -1.27)
		(end -1.4 -1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3ff77fd2-8bfc-4c70-a410-c2090c3f130a")
	)
	(fp_line
		(start 16.64 20.32)
		(end 16.575 -1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "845a8d6b-decd-47dc-bd78-74b678a251ce")
	)
	(fp_line
		(start -1.52 -1.27)
		(end -1.53 20.32)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ff08506e-5e76-4b7b-a279-1a663885f11e")
	)
	(fp_line
		(start -1.52 -1.27)
		(end 3.81 -1.27)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2a569fc4-ac68-4f48-bc55-7e9f76088d31")
	)
	(fp_line
		(start 16.75 20.32)
		(end -1.53 20.32)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e71abb04-8281-4024-8ad8-c9556f8b3ad0")
	)
	(fp_line
		(start 16.75 20.32)
		(end 16.76 -1.27)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4f317956-6ecc-410b-9c84-b4ab293a1921")
	)
	(fp_line
		(start -1.27 -1.27)
		(end 16.51 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "99efbf23-359b-44d9-b618-8fe70a5738eb")
	)
	(fp_line
		(start -1.27 20.32)
		(end -1.27 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6d89306e-8d39-4ac8-9175-226b963b1d38")
	)
	(fp_line
		(start 3.81 -3.81)
		(end 11.43 -3.81)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "35d5846c-cdf6-4b8d-8c02-3a72bbdfc6c4")
	)
	(fp_line
		(start 3.81 5.08)
		(end 3.81 -3.81)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b8e975e8-6a60-4156-8354-1db2cdfb866b")
	)
	(fp_line
		(start 11.43 -3.81)
		(end 11.43 5.08)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9a4dda7f-dc1a-4d6f-bde0-e8d43a3d7dfe")
	)
	(fp_line
		(start 11.43 5.08)
		(end 3.81 5.08)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5892b675-6cd2-4dee-84e1-70758daedaf4")
	)
	(fp_line
		(start 16.51 -1.27)
		(end 16.51 20.32)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "945d34ef-6f43-42f6-828f-e8f1e063de82")
	)
	(fp_line
		(start 16.51 20.32)
		(end -1.27 20.32)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "08f28974-415e-471d-af5b-09539cb7200e")
	)
	(fp_text user "USB"
		(at 7.62 1.27 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "aca452ce-688f-4dd7-99a4-9cba7a63a770")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at -3.81 8.89 90)
		(layer "F.Fab")
		(uuid "a3ade212-31dd-46ba-bb8e-a46703a507b8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "-1" thru_hole oval
		(at 15.24 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4882c682-0274-4d6b-8a9b-4b5d096bfce5")
	)
	(pad "-2" thru_hole oval
		(at 15.24 2.54)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ceb15fa3-a8b6-4d0f-a1b5-a4aec2dc2c0f")
	)
	(pad "-3" thru_hole oval
		(at 15.24 5.08)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c4b3235e-7483-47b3-8339-ca221af3eb18")
	)
	(pad "0" thru_hole oval
		(at 15.24 17.78)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "37f33c9e-8298-4531-83ea-3cf95f29cee6")
	)
	(pad "1" thru_hole oval
		(at 15.24 15.24)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ed0c51ef-1dc8-45e9-90fa-d6408d9998fa")
	)
	(pad "2" thru_hole oval
		(at 15.24 12.7)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9194bb4a-3b5f-47cd-a313-878797483842")
	)
	(pad "3" thru_hole oval
		(at 15.24 10.16)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "02d320c1-22c5-435e-be9b-3b46b9d5623a")
	)
	(pad "4" thru_hole oval
		(at 15.24 7.62)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4a99551f-e8a5-417f-b7bd-ea2a220af128")
	)
	(pad "5" thru_hole rect
		(at 0 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "57389eac-5d93-49d5-aa7e-a2c568b9c9c0")
	)
	(pad "6" thru_hole oval
		(at 0 2.54)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0921bf4a-c5d9-44b7-b854-f160aceef955")
	)
	(pad "7" thru_hole oval
		(at 0 5.08)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ab8fb3d7-5e17-47d9-8806-f62c8ac3b273")
	)
	(pad "8" thru_hole oval
		(at 0 7.62)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0017e8f5-9504-4a35-9b2c-0c15feeb6b07")
	)
	(pad "9" thru_hole oval
		(at 0 10.16)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "434b5d4e-c9b0-4a9d-aa8d-179ad9846f91")
	)
	(pad "10" thru_hole oval
		(at 0 12.7)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4b6f47e3-a1f9-4fe5-a993-e036ff2d4a67")
	)
	(pad "20" thru_hole oval
		(at 0 15.24)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d7b50d02-a79c-4de9-9ab1-f83f2d5d1f1c")
	)
	(pad "21" thru_hole oval
		(at 0 17.78)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "94d64a69-eb9f-4359-bf88-13714282b9dd")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/Blender/ESP32 C3 Super Mini.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
