
(footprint SOP65P640X120-14N (layer F.Cu) (tedit 65346025)
  (descr "")
  (attr smd)
  (fp_text reference REF** (at -0.595 -3.435 0) (layer F.SilkS)
    (effects (font (size 1.0 1.0) (thickness 0.15)))
  )
  (fp_text value SOP65P640X120-14N (at 7.025 3.435 0) (layer F.Fab)
    (effects (font (size 1.0 1.0) (thickness 0.15)))
  )
  (pad 1 smd roundrect (roundrect_rratio 0.05) (at -2.87 -1.95) (size 1.57 0.41) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 2 smd roundrect (roundrect_rratio 0.05) (at -2.87 -1.3) (size 1.57 0.41) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 3 smd roundrect (roundrect_rratio 0.05) (at -2.87 -0.65) (size 1.57 0.41) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 4 smd roundrect (roundrect_rratio 0.05) (at -2.87 0.0) (size 1.57 0.41) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 5 smd roundrect (roundrect_rratio 0.05) (at -2.87 0.65) (size 1.57 0.41) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 6 smd roundrect (roundrect_rratio 0.05) (at -2.87 1.3) (size 1.57 0.41) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 7 smd roundrect (roundrect_rratio 0.05) (at -2.87 1.95) (size 1.57 0.41) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 8 smd roundrect (roundrect_rratio 0.05) (at 2.87 1.95) (size 1.57 0.41) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 9 smd roundrect (roundrect_rratio 0.05) (at 2.87 1.3) (size 1.57 0.41) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 10 smd roundrect (roundrect_rratio 0.05) (at 2.87 0.65) (size 1.57 0.41) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 11 smd roundrect (roundrect_rratio 0.05) (at 2.87 0.0) (size 1.57 0.41) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 12 smd roundrect (roundrect_rratio 0.05) (at 2.87 -0.65) (size 1.57 0.41) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 13 smd roundrect (roundrect_rratio 0.05) (at 2.87 -1.3) (size 1.57 0.41) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 14 smd roundrect (roundrect_rratio 0.05) (at 2.87 -1.95) (size 1.57 0.41) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (fp_circle (center -4.24 -2.26) (end -4.14 -2.26) (layer F.SilkS) (width 0.2))
  (fp_circle (center -4.24 -2.26) (end -4.14 -2.26) (layer F.Fab) (width 0.2))
  (fp_line (start -2.2 -2.5) (end 2.2 -2.5) (layer F.Fab) (width 0.127))
  (fp_line (start -2.2 2.5) (end 2.2 2.5) (layer F.Fab) (width 0.127))
  (fp_line (start -2.2 -2.5) (end 2.2 -2.5) (layer F.SilkS) (width 0.127))
  (fp_line (start -2.2 2.5) (end 2.2 2.5) (layer F.SilkS) (width 0.127))
  (fp_line (start -2.2 -2.5) (end -2.2 2.5) (layer F.Fab) (width 0.127))
  (fp_line (start 2.2 -2.5) (end 2.2 2.5) (layer F.Fab) (width 0.127))
  (fp_line (start -3.905 -2.75) (end 3.905 -2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.905 2.75) (end 3.905 2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.905 -2.75) (end -3.905 2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.905 -2.75) (end 3.905 2.75) (layer F.CrtYd) (width 0.05))
)