(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "ESP32-DEVKITC-32D" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -15.2654 26.0604 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "ESP32-DEVKITC-32D" (at -15.2654 -27.9654 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "MODULE_ESP32-DEVKITC-32D" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "4" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Field4" "Espressif Systems" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "ESP32-DEVKITC-32D_0_0"
      (polyline
        (pts
          (xy -15.24 -25.4)
          (xy -15.24 25.4)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -15.24 25.4)
          (xy 15.24 25.4)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 15.24 -25.4)
          (xy -15.24 -25.4)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 15.24 25.4)
          (xy 15.24 -25.4)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (pin power_in line (at -20.32 22.86 0) (length 5.08)
        (name "3V3" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 0 0) (length 5.08)
        (name "IO26" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 -2.54 0) (length 5.08)
        (name "IO27" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 -5.08 0) (length 5.08)
        (name "IO14" (effects (font (size 1.016 1.016))))
        (number "12" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 -7.62 0) (length 5.08)
        (name "IO12" (effects (font (size 1.016 1.016))))
        (number "13" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -20.32 -10.16 0) (length 5.08)
        (name "GND1" (effects (font (size 1.016 1.016))))
        (number "14" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 -12.7 0) (length 5.08)
        (name "IO13" (effects (font (size 1.016 1.016))))
        (number "15" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 -15.24 0) (length 5.08)
        (name "SD2" (effects (font (size 1.016 1.016))))
        (number "16" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 -17.78 0) (length 5.08)
        (name "SD3" (effects (font (size 1.016 1.016))))
        (number "17" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 -20.32 0) (length 5.08)
        (name "CMD" (effects (font (size 1.016 1.016))))
        (number "18" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -20.32 -22.86 0) (length 5.08)
        (name "EXT_5V" (effects (font (size 1.016 1.016))))
        (number "19" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 20.32 0) (length 5.08)
        (name "EN" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 22.86 180) (length 5.08)
        (name "GND3" (effects (font (size 1.016 1.016))))
        (number "20" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 20.32 180) (length 5.08)
        (name "IO23" (effects (font (size 1.016 1.016))))
        (number "21" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 17.78 180) (length 5.08)
        (name "IO22" (effects (font (size 1.016 1.016))))
        (number "22" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 20.32 15.24 180) (length 5.08)
        (name "TXD0" (effects (font (size 1.016 1.016))))
        (number "23" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at 20.32 12.7 180) (length 5.08)
        (name "RXD0" (effects (font (size 1.016 1.016))))
        (number "24" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 10.16 180) (length 5.08)
        (name "IO21" (effects (font (size 1.016 1.016))))
        (number "25" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 7.62 180) (length 5.08)
        (name "GND2" (effects (font (size 1.016 1.016))))
        (number "26" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 5.08 180) (length 5.08)
        (name "IO19" (effects (font (size 1.016 1.016))))
        (number "27" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 2.54 180) (length 5.08)
        (name "IO18" (effects (font (size 1.016 1.016))))
        (number "28" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 0 180) (length 5.08)
        (name "IO5" (effects (font (size 1.016 1.016))))
        (number "29" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 17.78 0) (length 5.08)
        (name "SENSOR_VP" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -2.54 180) (length 5.08)
        (name "IO17" (effects (font (size 1.016 1.016))))
        (number "30" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -5.08 180) (length 5.08)
        (name "IO16" (effects (font (size 1.016 1.016))))
        (number "31" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -7.62 180) (length 5.08)
        (name "IO4" (effects (font (size 1.016 1.016))))
        (number "32" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -10.16 180) (length 5.08)
        (name "IO0" (effects (font (size 1.016 1.016))))
        (number "33" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -12.7 180) (length 5.08)
        (name "IO2" (effects (font (size 1.016 1.016))))
        (number "34" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -15.24 180) (length 5.08)
        (name "IO15" (effects (font (size 1.016 1.016))))
        (number "35" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -17.78 180) (length 5.08)
        (name "SD1" (effects (font (size 1.016 1.016))))
        (number "36" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -20.32 180) (length 5.08)
        (name "SD0" (effects (font (size 1.016 1.016))))
        (number "37" (effects (font (size 1.016 1.016))))
      )
      (pin input clock (at 20.32 -22.86 180) (length 5.08)
        (name "CLK" (effects (font (size 1.016 1.016))))
        (number "38" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 15.24 0) (length 5.08)
        (name "SENSOR_VN" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 12.7 0) (length 5.08)
        (name "IO34" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 10.16 0) (length 5.08)
        (name "IO35" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 7.62 0) (length 5.08)
        (name "IO32" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 5.08 0) (length 5.08)
        (name "IO33" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 2.54 0) (length 5.08)
        (name "IO25" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
    )
  )
  (symbol "SL2300" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "Q" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SL2300" (at 7.62 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SL2300_1_1"
      (polyline
        (pts
          (xy -1.016 0)
          (xy -3.81 0)
        )
        (stroke (width 0) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.016 1.905)
          (xy -1.016 -1.905)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.508 -1.27)
          (xy -0.508 -2.286)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.508 0.508)
          (xy -0.508 -0.508)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.508 2.286)
          (xy -0.508 1.27)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 2.54)
          (xy 1.27 1.778)
        )
        (stroke (width 0) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 -2.54)
          (xy 1.27 0)
          (xy -0.508 0)
        )
        (stroke (width 0) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.508 -1.778)
          (xy 2.032 -1.778)
          (xy 2.032 1.778)
          (xy -0.508 1.778)
        )
        (stroke (width 0) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.254 0)
          (xy 0.762 0.381)
          (xy 0.762 -0.381)
          (xy -0.254 0)
        )
        (stroke (width 0) (type solid))
        (fill (type outline))
      )
      (polyline
        (pts
          (xy 1.524 0.508)
          (xy 1.651 0.381)
          (xy 2.413 0.381)
          (xy 2.54 0.254)
        )
        (stroke (width 0) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.032 0.381)
          (xy 1.651 -0.254)
          (xy 2.413 -0.254)
          (xy 2.032 0.381)
        )
        (stroke (width 0) (type solid))
        (fill (type none))
      )
      (circle (center 0.381 0) (radius 2.794)
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (circle (center 1.27 -1.778) (radius 0.254)
        (stroke (width 0) (type solid))
        (fill (type outline))
      )
      (circle (center 1.27 1.778) (radius 0.254)
        (stroke (width 0) (type solid))
        (fill (type outline))
      )
      (pin input line (at -6.35 0 0) (length 2.54)
        (name "G" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 1.27 -5.08 90) (length 2.54)
        (name "S" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 1.27 5.08 270) (length 2.54)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SR04M-2" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "H" (at 6.35 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SR04M-2" (at 7.62 -21.59 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SR04M-2_0_1"
      (rectangle (start -22.86 26.67) (end 41.91 -20.32)
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
    )
  )
  (symbol "SR04M-2-HeaderConn_01x04_Female" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 5.08 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SR04M-2-HeaderConn_01x04_Female" (at 0 -7.62 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "ESP32:SR04M-2PinHeader_1x04_P2.54mm_Vertical" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "connector" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Connector*:*_1x??_*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SR04M-2-HeaderConn_01x04_Female_1_1"
      (arc (start 0 -4.572) (mid -0.5058 -5.08) (end 0 -5.588)
        (stroke (width 0.1524) (type solid))
        (fill (type none))
      )
      (arc (start 0 -2.032) (mid -0.5058 -2.54) (end 0 -3.048)
        (stroke (width 0.1524) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 -5.08)
          (xy -0.508 -5.08)
        )
        (stroke (width 0.1524) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 -2.54)
          (xy -0.508 -2.54)
        )
        (stroke (width 0.1524) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 0)
          (xy -0.508 0)
        )
        (stroke (width 0.1524) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 2.54)
          (xy -0.508 2.54)
        )
        (stroke (width 0.1524) (type solid))
        (fill (type none))
      )
      (arc (start 0 0.508) (mid -0.5058 0) (end 0 -0.508)
        (stroke (width 0.1524) (type solid))
        (fill (type none))
      )
      (arc (start 0 3.048) (mid -0.5058 2.54) (end 0 2.032)
        (stroke (width 0.1524) (type solid))
        (fill (type none))
      )
      (pin power_in line (at -5.08 2.54 0) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 0 0) (length 3.81)
        (name "RX" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -5.08 -2.54 0) (length 3.81)
        (name "TX" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -5.08 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
