(module N95_battery_connector (layer F.Cu) (tedit 569FD4EC)
  (fp_text reference CON** (at -0.5 6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value N95_battery_connector (at 0.5 -6) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.5 -4.5) (end -3 -4.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 -4.5) (end -3 4.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 4.5) (end 2.5 4.5) (layer F.SilkS) (width 0.15))
  (pad 2 smd rect (at 0 0) (size 5.5 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0 -3.5) (size 5.5 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 0 3.5) (size 5.5 1.5) (layers F.Cu F.Paste F.Mask))
)
