(footprint "R_Shunt_Vishay_WSK2512_6332Metric_T1.19mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Shunt Resistor SMD 2512 (6332 Metric), 2.6mm thick, Vishay WKS2512, Terminal length (T) 1.19mm, 5 to 200 milli Ohm (http://http://www.vishay.com/docs/30108/wsk.pdf)")
  (tags "resistor shunt WSK2512")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e64357ee-67ea-437d-842c-edd4e9b0e817)
  )
  (fp_text value "R_Shunt_Vishay_WSK2512_6332Metric_T1.19mm" (at 0 2.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6d43eee8-d677-4710-a5b6-ed0a393d7e86)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7af73258-6848-4c90-ada6-9916b21e0d54)
  )
  (fp_line (start -2.5 1.7) (end 1.67 1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 686b0a9f-f303-4b9c-97bc-13b268071b2a))
  (fp_line (start -1.67 -1.7) (end 2.53 -1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8ff3cd0c-2e69-49a7-948e-62e2af1cdeaf))
  (fp_line (start -4.38 -1.9) (end 4.38 -1.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 97453d6f-90a6-4d0b-9533-4b9de0e70d67))
  (fp_line (start -4.38 1.9) (end -4.38 -1.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8d751a64-d963-4d3e-b652-c6367d221a4c))
  (fp_line (start 4.38 -1.9) (end 4.38 1.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5fc8cbbe-390d-45f2-b9e2-001b3b36ad53))
  (fp_line (start 4.38 1.9) (end -4.38 1.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 85ea9322-734e-4f57-b7f4-e08d8559c109))
  (fp_line (start -3.175 -1.59) (end 3.175 -1.59)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a616017c-8c30-4c24-8988-6ebc65a5a14c))
  (fp_line (start -3.175 0.32) (end -3.175 -1.59)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 007035a4-df14-4627-b9dd-16c0816e9fc4))
  (fp_line (start -3.175 0.32) (end -2.795 0.32)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7a92ebc4-86fb-494b-8925-1512bf4598dd))
  (fp_line (start -3.175 0.94) (end -3.175 1.59)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8d1ed9db-8b9e-4c9a-b026-a147d8ba5a89))
  (fp_line (start -3.175 0.94) (end -2.795 0.94)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3238b0a3-1bbc-4ecd-9eca-d39a4563f46a))
  (fp_line (start -2.795 0.94) (end -2.795 0.32)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 56e7214e-7e65-4896-9919-6dfa6ad242a1))
  (fp_line (start 2.79 -0.94) (end 3.17 -0.94)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bf2fd8b5-dc07-4d36-93f4-c05d760e4ae8))
  (fp_line (start 2.79 -0.32) (end 2.79 -0.94)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2732ea3b-0a68-4014-9f1f-147b192cb827))
  (fp_line (start 2.79 -0.32) (end 3.17 -0.32)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7597632e-0fab-4537-9ef5-3d955ee8fe04))
  (fp_line (start 3.175 -0.94) (end 3.175 -1.59)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp be78e59b-9296-4843-849b-9aeaddf3ec90))
  (fp_line (start 3.175 -0.32) (end 3.175 1.59)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f0529fdf-6a96-4afa-ae66-3987676f8cc1))
  (fp_line (start 3.175 1.59) (end -3.175 1.59)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5494f1f1-9934-4901-ae11-4f45356840a6))
  (pad "1" smd roundrect (at -2.985 0.635) (size 2.29 2.03) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.12) (tstamp 7d665233-6376-4fd3-9d23-184556b0630c))
  (pad "2" smd roundrect (at -3.43 -1.27) (size 1.4 0.76) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.12) (tstamp a060266a-0c38-4364-b2df-6f7cf4c69f0d))
  (pad "3" smd roundrect (at 3.43 -1.27) (size 1.4 0.76) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a1e31646-49e8-4836-bd67-1b6bed652414))
  (pad "4" smd roundrect (at 2.985 0.635) (size 2.29 2.03) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.12) (tstamp 3f532dd2-fd5a-4fe7-9636-aa84f769e3b2))
  (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Vishay_WSK2512_6332Metric_T1.19mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
