
(footprint XCVR_ESP32-C6-WROOM-1-N8 (layer F.Cu) (tedit 66216AE3)
  (descr "")
  (attr smd)
  (fp_text reference REF** (at -5.825 -13.885 0) (layer F.SilkS)
    (effects (font (size 1.0 1.0) (thickness 0.15)))
  )
  (fp_text value XCVR_ESP32-C6-WROOM-1-N8 (at 6.24 13.865 0) (layer F.Fab)
    (effects (font (size 1.0 1.0) (thickness 0.15)))
  )
  (pad 1 smd rect (at -8.75 -5.26) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 2 smd rect (at -8.75 -3.99) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 3 smd rect (at -8.75 -2.72) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 4 smd rect (at -8.75 -1.45) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 5 smd rect (at -8.75 -0.18) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 6 smd rect (at -8.75 1.09) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 7 smd rect (at -8.75 2.36) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 8 smd rect (at -8.75 3.63) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 9 smd rect (at -8.75 4.9) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 10 smd rect (at -8.75 6.17) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 11 smd rect (at -8.75 7.44) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 12 smd rect (at -8.75 8.71) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 13 smd rect (at -8.75 9.98) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 14 smd rect (at -8.75 11.25) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 15 smd rect (at 8.75 11.25) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 16 smd rect (at 8.75 9.98) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 17 smd rect (at 8.75 8.71) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 18 smd rect (at 8.75 7.44) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 19 smd rect (at 8.75 6.17) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 20 smd rect (at 8.75 4.9) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 21 smd rect (at 8.75 3.63) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 22 smd rect (at 8.75 2.36) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 23 smd rect (at 8.75 1.09) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 24 smd rect (at 8.75 -0.18) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 25 smd rect (at 8.75 -1.45) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 26 smd rect (at 8.75 -2.72) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 27 smd rect (at 8.75 -3.99) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 28 smd rect (at 8.75 -5.26) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 29_5 smd rect (at -1.505 0.46) (size 0.8 0.8) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 29_1 smd rect (at -2.755 -0.79) (size 0.8 0.8) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 29_2 smd rect (at -1.505 -0.79) (size 0.8 0.8) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 29_3 smd rect (at -0.255 -0.79) (size 0.8 0.8) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 29_4 smd rect (at -2.755 0.46) (size 0.8 0.8) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 29_6 smd rect (at -0.255 0.46) (size 0.8 0.8) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 29_7 smd rect (at -2.755 1.71) (size 0.8 0.8) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 29_8 smd rect (at -1.505 1.71) (size 0.8 0.8) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 29_9 smd rect (at -0.255 1.71) (size 0.8 0.8) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 30_1 thru_hole circle (at -2.13 -0.79) (size 0.35 0.35) (drill 0.25) (layers *.Cu))
  (pad 30_2 thru_hole circle (at -0.88 -0.79) (size 0.35 0.35) (drill 0.25) (layers *.Cu))
  (pad 30_3 thru_hole circle (at -2.755 -0.165) (size 0.35 0.35) (drill 0.25) (layers *.Cu))
  (pad 30_4 thru_hole circle (at -1.505 -0.165) (size 0.35 0.35) (drill 0.25) (layers *.Cu))
  (pad 30_5 thru_hole circle (at -0.255 -0.165) (size 0.35 0.35) (drill 0.25) (layers *.Cu))
  (pad 30_6 thru_hole circle (at -2.13 0.46) (size 0.35 0.35) (drill 0.25) (layers *.Cu))
  (pad 30_7 thru_hole circle (at -0.88 0.46) (size 0.35 0.35) (drill 0.25) (layers *.Cu))
  (pad 30_8 thru_hole circle (at -2.755 1.085) (size 0.35 0.35) (drill 0.25) (layers *.Cu))
  (pad 30_9 thru_hole circle (at -1.505 1.085) (size 0.35 0.35) (drill 0.25) (layers *.Cu))
  (pad 30_10 thru_hole circle (at -0.255 1.085) (size 0.35 0.35) (drill 0.25) (layers *.Cu))
  (pad 30_11 thru_hole circle (at -2.13 1.71) (size 0.35 0.35) (drill 0.25) (layers *.Cu))
  (pad 30_12 thru_hole circle (at -0.88 1.71) (size 0.35 0.35) (drill 0.25) (layers *.Cu))
  (fp_line (start -9.0 12.75) (end 9.0 12.75) (layer F.Fab) (width 0.127))
  (fp_line (start -9.0 -12.75) (end 9.0 -12.75) (layer F.Fab) (width 0.127))
  (fp_line (start 9.0 -12.75) (end 9.0 12.75) (layer F.Fab) (width 0.127))
  (fp_line (start -9.0 12.75) (end 9.0 12.75) (layer F.SilkS) (width 0.127))
  (fp_line (start -9.0 12.75) (end -9.0 12.02) (layer F.SilkS) (width 0.127))
  (fp_line (start 9.0 12.02) (end 9.0 12.75) (layer F.SilkS) (width 0.127))
  (fp_line (start -9.0 -6.03) (end -9.0 -12.75) (layer F.SilkS) (width 0.127))
  (fp_line (start -9.0 -12.75) (end 9.0 -12.75) (layer F.SilkS) (width 0.127))
  (fp_line (start 9.0 -12.75) (end 9.0 -6.03) (layer F.SilkS) (width 0.127))
  (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks allowed) (vias not_allowed) (pads allowed ) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -9.0 -12.75)
        (xy 9.0 -12.75)
        (xy 9.0 -6.75)
        (xy -9.0 -6.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -9.0 -12.75)
        (xy 9.0 -12.75)
        (xy 9.0 -6.75)
        (xy -9.0 -6.75)
      )
    )
  )
  (fp_line (start -9.75 -13.0) (end -9.75 13.0) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.75 13.0) (end 9.75 13.0) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.75 13.0) (end 9.75 -13.0) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.75 -13.0) (end -9.75 -13.0) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.0 12.75) (end -9.0 -12.75) (layer F.Fab) (width 0.127))
  (fp_circle (center -10.0 -5.25) (end -9.9 -5.25) (layer F.SilkS) (width 0.2))
  (fp_circle (center -10.0 -5.25) (end -9.9 -5.25) (layer F.Fab) (width 0.2))
)