(module MT3608_module_SMT (layer F.Cu) (tedit 569D6C5F)
  (fp_text reference M2 (at 0.25 6 180) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value DC_DC_boost_module (at 0 -1 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VOUT- (at -16 6.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VIN+ (at 14 -6.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VIN- (at 14 6.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VOUT+ (at -16 -6.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -8 -7) (end -8 -4) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.5 -7) (end -4.5 -4) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.5 -4) (end -8 -5.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -8 -5.5) (end -4.5 -7) (layer F.SilkS) (width 0.15))
  (fp_arc (start -17 -6) (end -19.5 -6) (angle 90) (layer F.SilkS) (width 0.15))
  (fp_arc (start 14 -6) (end 14 -8.5) (angle 90) (layer F.SilkS) (width 0.15))
  (fp_arc (start 14 6) (end 16.5 6) (angle 90) (layer F.SilkS) (width 0.15))
  (fp_arc (start -17 6) (end -17 8.5) (angle 90) (layer F.SilkS) (width 0.15))
  (fp_line (start -17 8.5) (end 14 8.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 14 -8.5) (end -17 -8.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 16.5 6) (end 16.5 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start -19.5 -6) (end -19.5 6) (layer F.SilkS) (width 0.15))
  (pad "" thru_hole circle (at -7.75 5) (size 2.1 2.1) (drill 2) (layers *.Cu *.Mask F.SilkS))
  (pad "" thru_hole circle (at -5.5 2.5) (size 2.1 2.1) (drill 2) (layers *.Cu *.Mask F.SilkS))
  (pad "" thru_hole circle (at -10.5 2.5) (size 2.1 2.1) (drill 2) (layers *.Cu *.Mask F.SilkS))
  (pad 1 smd rect (at 14 -3.2 180) (size 5 3.5) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 14 3.25 180) (size 5 3.5) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -17 3.25 180) (size 5 3.5) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -17 -3.25 180) (size 5 3.5) (layers F.Cu F.Paste F.Mask))
)
