(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)

  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 891)
    (zones 0)
    (modules 141)
    (nets 83)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 1)
    (user_trace_width 0.2)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 4 3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 68.58 26.67)
    (grid_origin 68.58 26.67)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x3ffff_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )

  (net 0 "")
  (net 1 PLANT1_PUMP)
  (net 2 PLANT2_PUMP)
  (net 3 PLANT3_PUMP)
  (net 4 PLANT4_PUMP)
  (net 5 PLANT5_PUMP)
  (net 6 PLANT6_PUMP)
  (net 7 GND)
  (net 8 PLANT6_MOIST)
  (net 9 PLANT5_MOIST)
  (net 10 PLANT4_MOIST)
  (net 11 PLANT3_MOIST)
  (net 12 PLANT2_MOIST)
  (net 13 PLANT1_MOIST)
  (net 14 PLANT_CTRL_PUMP_0)
  (net 15 LIPO+)
  (net 16 SOLAR_IN)
  (net 17 PUMP_PWR)
  (net 18 PWR_PUMP_CONVERTER)
  (net 19 "Net-(J5-Pad3)")
  (net 20 3_3V)
  (net 21 Temp)
  (net 22 PLANT0_PUMP)
  (net 23 CUSTOM_GPIO)
  (net 24 PWR_SENSORS)
  (net 25 PLANT0_MOIST)
  (net 26 "Net-(C1-Pad2)")
  (net 27 "Net-(C2-Pad2)")
  (net 28 "Net-(R35-Pad1)")
  (net 29 PLANT_CTRL_PUMP_1)
  (net 30 "Net-(R37-Pad1)")
  (net 31 PLANT_CTRL_PUMP_2)
  (net 32 "Net-(R39-Pad1)")
  (net 33 PLANT_CTRL_PUMP_3)
  (net 34 "Net-(R41-Pad1)")
  (net 35 PLANT_CTRL_PUMP_4)
  (net 36 "Net-(R43-Pad1)")
  (net 37 PLANT_CTRL_PUMP_5)
  (net 38 "Net-(R45-Pad1)")
  (net 39 PLANT_CTRL_PUMP_6)
  (net 40 "Net-(R49-Pad1)")
  (net 41 PUMP_ENABLE)
  (net 42 SENSORS_ENABLE)
  (net 43 GND_BATT)
  (net 44 "Net-(C10-Pad2)")
  (net 45 VCC_BATT)
  (net 46 LIPO_OD)
  (net 47 LIPO_OC)
  (net 48 "Net-(Q11-Pad3)")
  (net 49 "Net-(D8-Pad2)")
  (net 50 "Net-(D18-Pad3)")
  (net 51 "Net-(Hall1-Pad3)")
  (net 52 "Net-(Hall1-Pad2)")
  (net 53 "Net-(IC1-Pad2)")
  (net 54 "Net-(JP3-Pad1)")
  (net 55 "Net-(JP4-Pad1)")
  (net 56 "Net-(JP5-Pad1)")
  (net 57 "Net-(R20-Pad2)")
  (net 58 "Net-(R21-Pad2)")
  (net 59 "Net-(D1-Pad2)")
  (net 60 "Net-(D2-Pad2)")
  (net 61 "Net-(D3-Pad2)")
  (net 62 "Net-(D4-Pad2)")
  (net 63 "Net-(D5-Pad2)")
  (net 64 "Net-(D6-Pad2)")
  (net 65 "Net-(D7-Pad2)")
  (net 66 "Net-(Pumps1-Pad2)")
  (net 67 "Net-(Q1-Pad1)")
  (net 68 "Net-(Q2-Pad1)")
  (net 69 "Net-(Q3-Pad1)")
  (net 70 "Net-(Q4-Pad1)")
  (net 71 "Net-(Q5-Pad1)")
  (net 72 "Net-(Q6-Pad1)")
  (net 73 "Net-(Q7-Pad1)")
  (net 74 "Net-(Q8-Pad1)")
  (net 75 "Net-(Q9-Pad3)")
  (net 76 "Net-(Q9-Pad1)")
  (net 77 "Net-(Q10-Pad3)")
  (net 78 "Net-(Q10-Pad1)")
  (net 79 "Net-(Q_PWR1-Pad1)")
  (net 80 "Net-(Q_PWR2-Pad1)")
  (net 81 "Net-(R31-Pad1)")
  (net 82 "Net-(J5-Pad2)")

  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 1.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3_3V)
    (add_net CUSTOM_GPIO)
    (add_net GND)
    (add_net GND_BATT)
    (add_net LIPO+)
    (add_net LIPO_OC)
    (add_net LIPO_OD)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D18-Pad3)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(Hall1-Pad2)")
    (add_net "Net-(Hall1-Pad3)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(JP3-Pad1)")
    (add_net "Net-(JP4-Pad1)")
    (add_net "Net-(JP5-Pad1)")
    (add_net "Net-(Pumps1-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q10-Pad1)")
    (add_net "Net-(Q10-Pad3)")
    (add_net "Net-(Q11-Pad3)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(Q7-Pad1)")
    (add_net "Net-(Q8-Pad1)")
    (add_net "Net-(Q9-Pad1)")
    (add_net "Net-(Q9-Pad3)")
    (add_net "Net-(Q_PWR1-Pad1)")
    (add_net "Net-(Q_PWR2-Pad1)")
    (add_net "Net-(R20-Pad2)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(R31-Pad1)")
    (add_net "Net-(R35-Pad1)")
    (add_net "Net-(R37-Pad1)")
    (add_net "Net-(R39-Pad1)")
    (add_net "Net-(R41-Pad1)")
    (add_net "Net-(R43-Pad1)")
    (add_net "Net-(R45-Pad1)")
    (add_net "Net-(R49-Pad1)")
    (add_net PLANT0_MOIST)
    (add_net PLANT0_PUMP)
    (add_net PLANT1_MOIST)
    (add_net PLANT1_PUMP)
    (add_net PLANT2_MOIST)
    (add_net PLANT2_PUMP)
    (add_net PLANT3_MOIST)
    (add_net PLANT3_PUMP)
    (add_net PLANT4_MOIST)
    (add_net PLANT4_PUMP)
    (add_net PLANT5_MOIST)
    (add_net PLANT5_PUMP)
    (add_net PLANT6_MOIST)
    (add_net PLANT6_PUMP)
    (add_net PLANT_CTRL_PUMP_0)
    (add_net PLANT_CTRL_PUMP_1)
    (add_net PLANT_CTRL_PUMP_2)
    (add_net PLANT_CTRL_PUMP_3)
    (add_net PLANT_CTRL_PUMP_4)
    (add_net PLANT_CTRL_PUMP_5)
    (add_net PLANT_CTRL_PUMP_6)
    (add_net PUMP_ENABLE)
    (add_net PUMP_PWR)
    (add_net PWR_PUMP_CONVERTER)
    (add_net PWR_SENSORS)
    (add_net SENSORS_ENABLE)
    (add_net SOLAR_IN)
    (add_net Temp)
    (add_net VCC_BATT)
  )

  (net_class 5V ""
    (clearance 0.2)
    (trace_width 1.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (net_class Mini ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (net_class Power ""
    (clearance 0.2)
    (trace_width 1.7)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (module ESP32:MODULE_ESP32-DEVKITC-32D (layer F.Cu) (tedit 5F565126) (tstamp 5F61C0F7)
    (at 192.405 94.615)
    (path /5F5A25C2)
    (fp_text reference U2 (at -10.829175 -28.446045) (layer F.SilkS)
      (effects (font (size 1.000386 1.000386) (thickness 0.015)))
    )
    (fp_text value ESP32-DEVKITC-32D (at 1.24136 28.294535) (layer F.Fab)
      (effects (font (size 1.001047 1.001047) (thickness 0.015)))
    )
    (fp_circle (center -14.6 -19.9) (end -14.46 -19.9) (layer F.Fab) (width 0.28))
    (fp_circle (center -14.6 -19.9) (end -14.46 -19.9) (layer F.Fab) (width 0.28))
    (fp_line (start -14.2 27.5) (end -14.2 -27.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 14.2 27.5) (end -14.2 27.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 14.2 -27.4) (end 14.2 27.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -14.2 -27.4) (end 14.2 -27.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.95 27.25) (end -13.95 27.25) (layer F.SilkS) (width 0.127))
    (fp_line (start 13.95 -27.15) (end 13.95 27.25) (layer F.SilkS) (width 0.127))
    (fp_line (start -13.95 -27.15) (end 13.95 -27.15) (layer F.SilkS) (width 0.127))
    (fp_line (start -13.95 27.25) (end -13.95 -27.15) (layer F.SilkS) (width 0.127))
    (fp_line (start -13.95 27.25) (end -13.95 -27.15) (layer F.Fab) (width 0.127))
    (fp_line (start 13.95 27.25) (end -13.95 27.25) (layer F.Fab) (width 0.127))
    (fp_line (start 13.95 -27.15) (end 13.95 27.25) (layer F.Fab) (width 0.127))
    (fp_line (start -13.95 -27.15) (end 13.95 -27.15) (layer F.Fab) (width 0.127))
    (pad 38 thru_hole circle (at 12.7 25.96) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask))
    (pad 37 thru_hole circle (at 12.7 23.42) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask))
    (pad 36 thru_hole circle (at 12.7 20.88) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at 12.7 18.34) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 14 PLANT_CTRL_PUMP_0))
    (pad 34 thru_hole circle (at 12.7 15.8) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 21 Temp))
    (pad 33 thru_hole circle (at 12.7 13.26) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at 12.7 10.72) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 23 CUSTOM_GPIO))
    (pad 31 thru_hole circle (at 12.7 8.18) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 42 SENSORS_ENABLE))
    (pad 30 thru_hole circle (at 12.7 5.64) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 50 "Net-(D18-Pad3)"))
    (pad 29 thru_hole circle (at 12.7 3.1) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 29 PLANT_CTRL_PUMP_1))
    (pad 28 thru_hole circle (at 12.7 0.56) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 31 PLANT_CTRL_PUMP_2))
    (pad 27 thru_hole circle (at 12.7 -1.98) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 33 PLANT_CTRL_PUMP_3))
    (pad 26 thru_hole circle (at 12.7 -4.52) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 25 thru_hole circle (at 12.7 -7.06) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 35 PLANT_CTRL_PUMP_4))
    (pad 24 thru_hole circle (at 12.7 -9.6) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 57 "Net-(R20-Pad2)"))
    (pad 23 thru_hole circle (at 12.7 -12.14) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 56 "Net-(JP5-Pad1)"))
    (pad 22 thru_hole circle (at 12.7 -14.68) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 37 PLANT_CTRL_PUMP_5))
    (pad 21 thru_hole circle (at 12.7 -17.22) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 39 PLANT_CTRL_PUMP_6))
    (pad 20 thru_hole circle (at 12.7 -19.76) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 18 thru_hole circle (at -12.7 23.42) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at -12.7 20.88) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at -12.7 18.34) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at -12.7 15.8) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 41 PUMP_ENABLE))
    (pad 14 thru_hole circle (at -12.7 13.26) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 13 thru_hole circle (at -12.7 10.72) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 25 PLANT0_MOIST))
    (pad 12 thru_hole circle (at -12.7 8.18) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 13 PLANT1_MOIST))
    (pad 11 thru_hole circle (at -12.7 5.64) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 12 PLANT2_MOIST))
    (pad 10 thru_hole circle (at -12.7 3.1) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 11 PLANT3_MOIST))
    (pad 9 thru_hole circle (at -12.7 0.56) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 10 PLANT4_MOIST))
    (pad 8 thru_hole circle (at -12.7 -1.98) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 9 PLANT5_MOIST))
    (pad 7 thru_hole circle (at -12.7 -4.52) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 8 PLANT6_MOIST))
    (pad 6 thru_hole circle (at -12.7 -7.06) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 26 "Net-(C1-Pad2)"))
    (pad 5 thru_hole circle (at -12.7 -9.6) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 27 "Net-(C2-Pad2)"))
    (pad 4 thru_hole circle (at -12.7 -12.14) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -12.7 -14.68) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at -12.7 25.96) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -12.7 -17.22) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at -12.7 -19.76) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 20 3_3V))
    (model ${KIPRJMOD}/kicad-stuff/ESP32-DEVKITC-32D--3DModel-STEP-56544.STEP
      (offset (xyz 0 -3 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9) (tstamp 5FC21506)
    (at 211.074 127.508 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (path /5F8539DC)
    (attr smd)
    (fp_text reference Sensor1 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_green (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1 -0.6) (end -0.7 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.6) (end -1 -0.3) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.3) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.96) (end -1.86 -0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 -0.96) (end -1.86 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 0.96) (end 1 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 81 "Net-(R31-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 55 "Net-(JP4-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9) (tstamp 5FC20E39)
    (at 210.82 111.506 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (path /5F834AFA)
    (attr smd)
    (fp_text reference Pumps1 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_red (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1 -0.6) (end -0.7 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.6) (end -1 -0.3) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.3) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.96) (end -1.86 -0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 -0.96) (end -1.86 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 0.96) (end 1 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 66 "Net-(Pumps1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9) (tstamp 5FC20711)
    (at 262.636 104.902 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (path /5F7DC6AB)
    (attr smd)
    (fp_text reference D7 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_Blue (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1 -0.6) (end -0.7 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.6) (end -1 -0.3) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.3) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.96) (end -1.86 -0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 -0.96) (end -1.86 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 0.96) (end 1 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 65 "Net-(D7-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 PLANT6_PUMP))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9) (tstamp 5FC206FE)
    (at 239.776 104.8655 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (path /5F81F9E9)
    (attr smd)
    (fp_text reference D6 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1 -0.6) (end -0.7 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.6) (end -1 -0.3) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.3) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.96) (end -1.86 -0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 -0.96) (end -1.86 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 0.96) (end 1 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 64 "Net-(D6-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 PLANT3_PUMP))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9) (tstamp 5FC206EB)
    (at 255.27 104.902 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (path /5F795029)
    (attr smd)
    (fp_text reference D5 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1 -0.6) (end -0.7 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.6) (end -1 -0.3) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.3) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.96) (end -1.86 -0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 -0.96) (end -1.86 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 0.96) (end 1 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 63 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 PLANT5_PUMP))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9) (tstamp 5FC206D8)
    (at 231.902 104.8655 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (path /5F811E9A)
    (attr smd)
    (fp_text reference D4 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_Blue (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1 -0.6) (end -0.7 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.6) (end -1 -0.3) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.3) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.96) (end -1.86 -0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 -0.96) (end -1.86 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 0.96) (end 1 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 62 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 PLANT2_PUMP))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9) (tstamp 5FC206C5)
    (at 247.396 104.902 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (path /5F7D93FF)
    (attr smd)
    (fp_text reference D3 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_Blue (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1 -0.6) (end -0.7 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.6) (end -1 -0.3) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.3) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.96) (end -1.86 -0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 -0.96) (end -1.86 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 0.96) (end 1 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 61 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 PLANT4_PUMP))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9) (tstamp 5FC206B2)
    (at 224.282 104.8655 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (path /5F7FA2EA)
    (attr smd)
    (fp_text reference D2 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1 -0.6) (end -0.7 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.6) (end -1 -0.3) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.3) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.96) (end -1.86 -0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 -0.96) (end -1.86 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 0.96) (end 1 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 60 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 PLANT1_PUMP))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9) (tstamp 5FC2069F)
    (at 216.916 104.902 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (path /5F7E5EE6)
    (attr smd)
    (fp_text reference D1 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_Blue (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1 -0.6) (end -0.7 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.6) (end -1 -0.3) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.3) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.96) (end -1.86 -0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 -0.96) (end -1.86 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.86 0.96) (end 1 0.96) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 59 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 22 PLANT0_PUMP))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B) (tstamp 5FC18632)
    (at 186.182 73.66 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /603684C2)
    (attr smd)
    (fp_text reference C13 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22uf (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.6) (end -1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -0.261252 -0.71) (end 0.261252 -0.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.261252 0.71) (end 0.261252 0.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 3_3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B) (tstamp 5FC18621)
    (at 245.11 75.438 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /6007356D)
    (attr smd)
    (fp_text reference C12 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22uf (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.6) (end -1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -0.261252 -0.71) (end 0.261252 -0.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.261252 0.71) (end 0.261252 0.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 17 PUMP_PWR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B) (tstamp 5FC18610)
    (at 240.03 71.882)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /5FF0BD1A)
    (attr smd)
    (fp_text reference C11 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22uf (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.6) (end -1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -0.261252 -0.71) (end 0.261252 -0.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.261252 0.71) (end 0.261252 0.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 PWR_PUMP_CONVERTER))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC35D10)
    (at 234.061 76.581 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5FC8E1C3)
    (attr smd)
    (fp_text reference D25 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 PWR_SENSORS))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 LIPO+))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm (layer F.Cu) (tedit 5C756AB2) (tstamp 5FC18BB1)
    (at 210.678 131.684)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (path /6017FFC5)
    (attr virtual)
    (fp_text reference JP4 (at 0 -1.8) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SolderJumper_2_Open (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_poly (pts (xy -0.25 -0.3) (xy 0.25 -0.3) (xy 0.25 0.3) (xy -0.25 0.3)) (layer F.Cu) (width 0))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 1) (end -1.4 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 1) (end -1.4 -1) (layer F.SilkS) (width 0.12))
    (pad 2 smd rect (at 0.65 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.65 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 55 "Net-(JP4-Pad1)"))
  )

  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 5FC543C6)
    (at 183.134 87.9055 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /5FB48503)
    (attr smd)
    (fp_text reference C1 (at 0 -1.68 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1u (at 0 1.68 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 26 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A429) (tstamp 5FC3CD2F)
    (at 259.842 71.374)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (path /5F7E5709)
    (fp_text reference J2 (at 0 -2.77) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 0 10.39) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.8 9.4) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 9.4) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.8) (end 1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 8.89) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -0.635) (end 1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 SOLAR_IN))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 LIPO+))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module ESP32:SR04M-2PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5FC1448F) (tstamp 5FC285C1)
    (at 193.675 133.985 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (path /5F9D6D22)
    (fp_text reference Hall1 (at 0 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 0 9.95 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_poly (pts (xy 8.81 6.27) (xy 3.81 6.27) (xy 3.81 1.27) (xy 8.81 1.27)) (layer F.Fab) (width 0.1))
    (fp_line (start -10 -17.5) (end 0.5 -17.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -10 23.5) (end -10 -17.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 10 23.5) (end -10 23.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 10 -17.5) (end 10 23.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -17.5) (end 10 -17.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 PWR_SENSORS))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(Hall1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(Hall1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module ESP32:DPAK457P991X255-3N (layer F.Cu) (tedit 5F5CEF39) (tstamp 5FC215BA)
    (at 191.262 73.914 90)
    (path /5F84FA14)
    (attr smd)
    (fp_text reference U3 (at -2.825 -4.635 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.015)))
    )
    (fp_text value LP38690DT-3.3 (at 5.43 5.365 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.015)))
    )
    (fp_poly (pts (xy -0.265 -2.555) (xy 0.855 -2.555) (xy 0.855 -1.405) (xy -0.265 -1.405)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy 1.085 -2.555) (xy 2.205 -2.555) (xy 2.205 -1.405) (xy 1.085 -1.405)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy 2.435 -2.555) (xy 3.555 -2.555) (xy 3.555 -1.405) (xy 2.435 -1.405)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy 3.785 -2.555) (xy 4.905 -2.555) (xy 4.905 -1.405) (xy 3.785 -1.405)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy 3.785 -1.235) (xy 4.905 -1.235) (xy 4.905 -0.085) (xy 3.785 -0.085)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy 3.785 0.085) (xy 4.905 0.085) (xy 4.905 1.235) (xy 3.785 1.235)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy 3.785 1.405) (xy 4.905 1.405) (xy 4.905 2.555) (xy 3.785 2.555)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy 2.435 -1.235) (xy 3.555 -1.235) (xy 3.555 -0.085) (xy 2.435 -0.085)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy 2.435 0.085) (xy 3.555 0.085) (xy 3.555 1.235) (xy 2.435 1.235)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy 2.435 1.405) (xy 3.555 1.405) (xy 3.555 2.555) (xy 2.435 2.555)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy 1.085 -1.235) (xy 2.205 -1.235) (xy 2.205 -0.085) (xy 1.085 -0.085)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy 1.085 0.085) (xy 2.205 0.085) (xy 2.205 1.235) (xy 1.085 1.235)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy 1.085 1.405) (xy 2.205 1.405) (xy 2.205 2.555) (xy 1.085 2.555)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy -0.265 -1.235) (xy 0.855 -1.235) (xy 0.855 -0.085) (xy -0.265 -0.085)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy -0.265 0.085) (xy 0.855 0.085) (xy 0.855 1.235) (xy -0.265 1.235)) (layer F.Paste) (width 0.01))
    (fp_poly (pts (xy -0.265 1.405) (xy 0.855 1.405) (xy 0.855 2.555) (xy -0.265 2.555)) (layer F.Paste) (width 0.01))
    (fp_line (start 3.875 -3.365) (end -2.345 -3.365) (layer F.SilkS) (width 0.127))
    (fp_line (start -2.345 -3.365) (end -2.345 3.365) (layer F.SilkS) (width 0.127))
    (fp_line (start -2.345 3.365) (end 3.875 3.365) (layer F.SilkS) (width 0.127))
    (fp_line (start 3.875 3.365) (end 3.875 -3.365) (layer F.Fab) (width 0.127))
    (fp_line (start 3.875 -3.365) (end -2.345 -3.365) (layer F.Fab) (width 0.127))
    (fp_line (start -2.345 -3.365) (end -2.345 3.365) (layer F.Fab) (width 0.127))
    (fp_line (start -2.345 3.365) (end 3.875 3.365) (layer F.Fab) (width 0.127))
    (fp_circle (center -6.015 -2.285) (end -5.915 -2.285) (layer F.SilkS) (width 0.2))
    (fp_circle (center -6.015 -2.285) (end -5.915 -2.285) (layer F.Fab) (width 0.2))
    (fp_line (start -5.815 -3.615) (end 5.815 -3.615) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.815 -3.615) (end 5.815 3.615) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.815 3.615) (end -5.815 3.615) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.815 3.615) (end -5.815 -3.615) (layer F.CrtYd) (width 0.05))
    (pad 4 smd rect (at 2.32 0 90) (size 6.49 5.63) (layers F.Cu F.Mask)
      (net 7 GND))
    (pad 3 smd rect (at -4.45 2.285 90) (size 2.22 0.96) (layers F.Cu F.Paste F.Mask)
      (net 15 LIPO+))
    (pad 1 smd rect (at -4.45 -2.285 90) (size 2.22 0.96) (layers F.Cu F.Paste F.Mask)
      (net 20 3_3V))
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC212F3)
    (at 229.87 74.93 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5FBB5E39)
    (attr smd)
    (fp_text reference R51 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 42 SENSORS_ENABLE))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 78 "Net-(Q10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC212E2)
    (at 182.896 110.236 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5FBA9B4B)
    (attr smd)
    (fp_text reference R50 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 41 PUMP_ENABLE))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 76 "Net-(Q9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC212D1)
    (at 264.287 126.238 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F99CEF5)
    (attr smd)
    (fp_text reference R49 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 8 PLANT6_MOIST))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 40 "Net-(R49-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC212C0)
    (at 192.278 92.71 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F9D1DC9)
    (attr smd)
    (fp_text reference R48 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 20 3_3V))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 54 "Net-(JP3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC212AF)
    (at 262.636 95.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5FB647E5)
    (attr smd)
    (fp_text reference R47 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 74 "Net-(Q8-Pad1)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 39 PLANT_CTRL_PUMP_6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC5A078)
    (at 198.374 96.774 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5FC58F54)
    (attr smd)
    (fp_text reference R46 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 23 CUSTOM_GPIO))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 72 "Net-(Q6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC2128D)
    (at 256.794 126.365 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F99CBD3)
    (attr smd)
    (fp_text reference R45 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 9 PLANT5_MOIST))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 38 "Net-(R45-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC2127C)
    (at 255.27 95.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5FB64320)
    (attr smd)
    (fp_text reference R44 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 71 "Net-(Q5-Pad1)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 37 PLANT_CTRL_PUMP_5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC2126B)
    (at 249.174 126.365 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F99C828)
    (attr smd)
    (fp_text reference R43 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 10 PLANT4_MOIST))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 36 "Net-(R43-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC2125A)
    (at 247.396 95.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5FB634A6)
    (attr smd)
    (fp_text reference R42 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 69 "Net-(Q3-Pad1)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 35 PLANT_CTRL_PUMP_4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC21249)
    (at 241.554 126.365 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F99C5A6)
    (attr smd)
    (fp_text reference R41 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 11 PLANT3_MOIST))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 34 "Net-(R41-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC21238)
    (at 239.776 95.266 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5FB62F27)
    (attr smd)
    (fp_text reference R40 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 73 "Net-(Q7-Pad1)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 33 PLANT_CTRL_PUMP_3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC21227)
    (at 234.061 126.365 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F99C2BC)
    (attr smd)
    (fp_text reference R39 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 12 PLANT2_MOIST))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 32 "Net-(R39-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC21216)
    (at 231.902 95.266 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5FB62A85)
    (attr smd)
    (fp_text reference R38 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 70 "Net-(Q4-Pad1)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 31 PLANT_CTRL_PUMP_2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC21205)
    (at 226.441 126.349 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F99BE26)
    (attr smd)
    (fp_text reference R37 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 13 PLANT1_MOIST))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 30 "Net-(R37-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC211F4)
    (at 224.282 95.266 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5FB62566)
    (attr smd)
    (fp_text reference R36 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 68 "Net-(Q2-Pad1)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 29 PLANT_CTRL_PUMP_1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC211E3)
    (at 218.694 126.349 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F993C00)
    (attr smd)
    (fp_text reference R35 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 25 PLANT0_MOIST))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 28 "Net-(R35-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC211D2)
    (at 216.916 95.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5FB60540)
    (attr smd)
    (fp_text reference R34 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 67 "Net-(Q1-Pad1)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 14 PLANT_CTRL_PUMP_0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC211C1)
    (at 208.788 127.762 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F8539E2)
    (attr smd)
    (fp_text reference R31 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 270 (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 24 PWR_SENSORS))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 81 "Net-(R31-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC211B0)
    (at 210.82 106.934 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F834B00)
    (attr smd)
    (fp_text reference R30 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 270 (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 66 "Net-(Pumps1-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 18 PWR_PUMP_CONVERTER))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC2117F)
    (at 233.934 85.598)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F819B5B)
    (attr smd)
    (fp_text reference R28 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 15 LIPO+))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 80 "Net-(Q_PWR2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC2116E)
    (at 238.252 87.122)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F7BEED8)
    (attr smd)
    (fp_text reference R27 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 15 LIPO+))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 79 "Net-(Q_PWR1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC2115D)
    (at 204.47 127)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5EE03137)
    (attr smd)
    (fp_text reference R26 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4k7 (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 24 PWR_SENSORS))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 21 Temp))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC2114C)
    (at 229.87 85.598 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F819B52)
    (attr smd)
    (fp_text reference R25 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 77 "Net-(Q10-Pad3)"))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 80 "Net-(Q_PWR2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC2113B)
    (at 242.316 81.534)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F7B97DA)
    (attr smd)
    (fp_text reference R24 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 75 "Net-(Q9-Pad3)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 79 "Net-(Q_PWR1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC2112A)
    (at 229.87 77.216 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F819B42)
    (attr smd)
    (fp_text reference R23 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 GND))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 78 "Net-(Q10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC21119)
    (at 242.316 84.836 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F7A8C30)
    (attr smd)
    (fp_text reference R22 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 GND))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 76 "Net-(Q9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC325E6)
    (at 259.572 96.266 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F79B18E)
    (attr smd)
    (fp_text reference R19 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 GND))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 74 "Net-(Q8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC210B7)
    (at 262.636 100.314 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F7DC6B1)
    (attr smd)
    (fp_text reference R18 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 270 (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 65 "Net-(D7-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 15 LIPO+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC210A6)
    (at 236.712 96.266 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F7960A3)
    (attr smd)
    (fp_text reference R17 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 47k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 GND))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 73 "Net-(Q7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC21095)
    (at 200.66 92.71 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F8849CF)
    (attr smd)
    (fp_text reference R16 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 72 "Net-(Q6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC21084)
    (at 239.776 100.346 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F81F9EF)
    (attr smd)
    (fp_text reference R15 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 270 (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 64 "Net-(D6-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 15 LIPO+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC21073)
    (at 252.222 96.266 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F79ABE6)
    (attr smd)
    (fp_text reference R14 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 GND))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 71 "Net-(Q5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC21062)
    (at 255.27 100.33 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F79751F)
    (attr smd)
    (fp_text reference R13 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 270 (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 63 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 15 LIPO+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC21051)
    (at 228.838 96.266 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F79593C)
    (attr smd)
    (fp_text reference R12 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 GND))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 70 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC21040)
    (at 231.902 100.346 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F811EA0)
    (attr smd)
    (fp_text reference R11 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 270 (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 62 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 15 LIPO+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC2102F)
    (at 244.348 96.266 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F79A87D)
    (attr smd)
    (fp_text reference R10 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 47k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 GND))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 69 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC2101E)
    (at 247.396 100.33 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F7D9405)
    (attr smd)
    (fp_text reference R9 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 270 (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 61 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 15 LIPO+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC2100D)
    (at 221.234 96.266)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F791D01)
    (attr smd)
    (fp_text reference R8 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 68 "Net-(Q2-Pad1)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC20FFC)
    (at 224.282 100.33 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F7FA2F0)
    (attr smd)
    (fp_text reference R7 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 270 (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 60 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 15 LIPO+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC20FEB)
    (at 213.868 96.266 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F795254)
    (attr smd)
    (fp_text reference R6 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 GND))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 67 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC20FDA)
    (at 216.916 100.33 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5F7E5EEC)
    (attr smd)
    (fp_text reference R5 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 270 (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 59 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 15 LIPO+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC20FC9)
    (at 186.182 83.82 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5EDD7349)
    (attr smd)
    (fp_text reference R4 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 47k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 GND))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 27 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC20FB8)
    (at 188.976 83.82 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5EDD7688)
    (attr smd)
    (fp_text reference R3 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 33k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 27 "Net-(C2-Pad2)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 15 LIPO+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC20FA7)
    (at 265.938 74.676 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5EDC9260)
    (attr smd)
    (fp_text reference R2 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 33k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 26 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC20F96)
    (at 265.938 78.74 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5EDC87BD)
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 26 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 16 SOLAR_IN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C) (tstamp 5FC20F85)
    (at 233.934 81.788 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5F819B36)
    (attr smd)
    (fp_text reference Q_PWR2 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "P-channel 50v 4A" (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 PWR_SENSORS))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 LIPO+))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(Q_PWR2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C) (tstamp 5FC20F70)
    (at 238.252 83.312 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5F765B13)
    (attr smd)
    (fp_text reference Q_PWR1 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "P-channel 50v 4A" (at 0 2.54 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 PWR_PUMP_CONVERTER))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 LIPO+))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(Q_PWR1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C) (tstamp 5FC20F0B)
    (at 229.87 81.28 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5F819B3C)
    (attr smd)
    (fp_text reference Q10 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "N-channel 30V 5A" (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(Q10-Pad3)"))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(Q10-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C) (tstamp 5FC20EF6)
    (at 246.126 83.312 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5F781665)
    (attr smd)
    (fp_text reference Q9 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "N-channel 30V 5A" (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(Q9-Pad3)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(Q9-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C) (tstamp 5FC20EE1)
    (at 259.588 100.076 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5F77EC00)
    (attr smd)
    (fp_text reference Q8 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "N-channel 30V 5A" (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 PLANT6_PUMP))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(Q8-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C) (tstamp 5FC20ECC)
    (at 236.728 100.076 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5F7702AA)
    (attr smd)
    (fp_text reference Q7 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "N-channel 30V 5A" (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 PLANT3_PUMP))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(Q7-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C) (tstamp 5FC20EB7)
    (at 196.596 92.71 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5F87CA1E)
    (attr smd)
    (fp_text reference Q6 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "N-channel 30V 5A" (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(JP3-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.5 -0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(Q6-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C) (tstamp 5FC20EA2)
    (at 252.222 100.076 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5F77DFF6)
    (attr smd)
    (fp_text reference Q5 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "N-channel 30V 5A" (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 PLANT5_PUMP))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(Q5-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C) (tstamp 5FC20E8D)
    (at 228.854 100.076 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5F779588)
    (attr smd)
    (fp_text reference Q4 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "N-channel 30V 5A" (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 PLANT2_PUMP))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C) (tstamp 5FC20E78)
    (at 244.348 100.076 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5F77CB3F)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "N-channel 30V 5A" (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 PLANT4_PUMP))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C) (tstamp 5FC20E63)
    (at 221.234 100.076 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5F77A216)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "N-channel 30V 5A" (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 PLANT1_PUMP))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C) (tstamp 5FC20E4E)
    (at 213.868 100.076 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5F77AFC2)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "N-channel 30V 5A" (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 PLANT0_PUMP))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5FC20B68)
    (at 173.736 113.792 270)
    (descr "JST EH series connector, B3B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F109CD6)
    (fp_text reference J6 (at 2.5 -2.8 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x03 (at 2.5 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 7.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 2.2) (end 7.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 8 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 2.7) (end 8 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 7.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 2.31) (end 7.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 7.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 -1.21) (end 7.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 0) (end 7.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 0.81) (end 6.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.61 0.81) (end 6.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.5 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 24 PWR_SENSORS))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 21 Temp))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 7 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Fuse:Fuse_Blade_ATO_directSolder (layer F.Cu) (tedit 5A1C8B0A) (tstamp 5FC20959)
    (at 252.73 81.534 90)
    (descr "car blade fuse direct solder")
    (tags "car blade fuse")
    (path /5F8D8528)
    (fp_text reference F1 (at 4.65 -3.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 4.6 4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.95 0) (end 4.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -5.35 -3) (end 14.65 -3) (layer F.Fab) (width 0.1))
    (fp_line (start 14.65 -3) (end 14.65 3) (layer F.Fab) (width 0.1))
    (fp_line (start 14.65 3) (end -5.35 3) (layer F.Fab) (width 0.1))
    (fp_line (start -5.35 3) (end -5.35 -3) (layer F.Fab) (width 0.1))
    (fp_line (start -4.95 -2.5) (end 14.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.25 -2.5) (end 14.25 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.25 2.5) (end -4.95 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.95 2.5) (end -4.95 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.6 -3.25) (end 14.9 -3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.6 -3.25) (end -5.6 3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 14.9 3.25) (end 14.9 -3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 14.9 3.25) (end -5.6 3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.47 -3.12) (end 14.77 -3.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.47 -3.12) (end -5.47 3.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.77 3.12) (end 14.77 -3.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.77 3.12) (end -5.47 3.12) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 4.75 -1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 9.3 0 90) (size 8 3.8) (drill oval 6 2) (layers *.Cu *.Mask)
      (net 45 VCC_BATT))
    (pad 1 thru_hole oval (at 0 0 90) (size 8 3.8) (drill oval 6 2) (layers *.Cu *.Mask)
      (net 15 LIPO+))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_Blade_ATO_directSolder.wrl
      (offset (xyz 4.571999931335449 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 5FC2060C)
    (at 199.136 119.634 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /5FAEC671)
    (attr smd)
    (fp_text reference C9 (at 0 -1.68 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.68 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 8 PLANT6_MOIST))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 5FC205FB)
    (at 196.85 119.634 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /5FAEC21A)
    (attr smd)
    (fp_text reference C8 (at 0 -1.68 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.68 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 9 PLANT5_MOIST))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 5FC205EA)
    (at 194.564 119.634 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /5FAEBD5A)
    (attr smd)
    (fp_text reference C7 (at 0 -1.68 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.68 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 10 PLANT4_MOIST))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 5FC41BFF)
    (at 192.278 119.634 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /5FAEB847)
    (attr smd)
    (fp_text reference C6 (at 0 -1.68 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.68 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 11 PLANT3_MOIST))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 5FC205C8)
    (at 189.992 119.634 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /5FAEB37F)
    (attr smd)
    (fp_text reference C5 (at 0 -1.68 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.68 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 12 PLANT2_MOIST))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 5FC205B7)
    (at 187.706 119.634 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /5FAEAFAD)
    (attr smd)
    (fp_text reference C4 (at 0 -1.68 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.68 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 13 PLANT1_MOIST))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 5FC205A6)
    (at 185.42 119.634 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /5F9A17B3)
    (attr smd)
    (fp_text reference C3 (at 0 -1.68 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.68 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 25 PLANT0_MOIST))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 5FC20595)
    (at 183.134 83.82 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /5FB4725B)
    (attr smd)
    (fp_text reference C2 (at 0 -1.68 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1u (at 0 1.68 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 27 "Net-(C2-Pad2)"))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC19319)
    (at 176.276 70.358 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5FC908BA)
    (attr smd)
    (fp_text reference R53 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100 (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 44 "Net-(C10-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 45 VCC_BATT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC19308)
    (at 173.736 78.74 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5FC59C43)
    (attr smd)
    (fp_text reference R52 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 53 "Net-(IC1-Pad2)"))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC191B7)
    (at 244.094 72.136 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /600070FD)
    (attr smd)
    (fp_text reference R29 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 GND))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 58 "Net-(R21-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC19136)
    (at 246.38 72.136 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /60006701)
    (attr smd)
    (fp_text reference R21 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 18k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 58 "Net-(R21-Pad2)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 17 PUMP_PWR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE) (tstamp 5FC19125)
    (at 191.008 130.302 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (path /5FC4784F)
    (attr smd)
    (fp_text reference R20 (at 0 -1.65 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.85 0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 57 "Net-(R20-Pad2)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 52 "Net-(Hall1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductor_SMD:L_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5F68FEF0) (tstamp 5FC18BDE)
    (at 239.9935 78.74)
    (descr "Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (path /5FF33B77)
    (attr smd)
    (fp_text reference L1 (at 0 -2.28) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LQH32CN100K33L (at 0 2.28) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 1.25) (end -1.6 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -1.25) (end 1.6 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -1.25) (end 1.6 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 1.25) (end -1.6 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.602064 -1.36) (end 0.602064 -1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.602064 1.36) (end 0.602064 1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.45 1.58) (end -2.45 -1.58) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.45 -1.58) (end 2.45 -1.58) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.45 -1.58) (end 2.45 1.58) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.45 1.58) (end -2.45 1.58) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 49 "Net-(D8-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 PWR_PUMP_CONVERTER))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5A3EABFC) (tstamp 5FC18BCD)
    (at 191.77 81.534)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (path /6076B93D)
    (attr virtual)
    (fp_text reference JP6 (at 0 -1.8) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SolderJumper_2_Open (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 1) (end -1.4 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 1) (end -1.4 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.65 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 20 3_3V))
    (pad 2 smd rect (at 0.65 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 15 LIPO+))
  )

  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5A3EABFC) (tstamp 5FC18BBF)
    (at 188.722 130.302 270)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (path /6023651A)
    (attr virtual)
    (fp_text reference JP5 (at 0 -1.8 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SolderJumper_2_Open (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 1) (end -1.4 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 1) (end -1.4 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 56 "Net-(JP5-Pad1)"))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 51 "Net-(Hall1-Pad3)"))
  )

  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5A3EABFC) (tstamp 5FC18BA3)
    (at 185.166 97.282 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (path /601782AD)
    (attr virtual)
    (fp_text reference JP3 (at 0 -1.8) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SolderJumper_2_Open (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 1) (end -1.4 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 1) (end -1.4 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 54 "Net-(JP3-Pad1)"))
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 19 "Net-(J5-Pad3)"))
  )

  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5A3EABFC) (tstamp 5FC18B95)
    (at 185.166 94.234 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (path /60159E6D)
    (attr virtual)
    (fp_text reference JP2 (at 0 -1.8) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SolderJumper_2_Open (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 1) (end -1.4 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 1) (end -1.4 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 23 CUSTOM_GPIO))
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 82 "Net-(J5-Pad2)"))
  )

  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5A3EABFC) (tstamp 5FC18B87)
    (at 179.07 61.468 270)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (path /6011090E)
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SolderJumper_2_Open (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 1) (end -1.4 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 1) (end -1.4 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 43 GND_BATT))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 7 GND))
  )

  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A429) (tstamp 5F6011AA)
    (at 238.76 67.564 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (path /5F837F50)
    (fp_text reference J3 (at 0 -2.77 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 0 10.39 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -0.635) (end 1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 8.89) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.8) (end 1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 9.4) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 PUMP_PWR))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 PWR_PUMP_CONVERTER))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5FC189C2)
    (at 173.99 101.6 270)
    (descr "JST EH series connector, B3B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /6029884B)
    (fp_text reference J1 (at 2.5 -2.8 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x03_Female (at 2.5 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 7.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 2.2) (end 7.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 8 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 2.7) (end 8 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 7.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 2.31) (end 7.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 7.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 -1.21) (end 7.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 0) (end 7.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 0.81) (end 6.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.61 0.81) (end 6.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.5 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 50 "Net-(D18-Pad3)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 24 PWR_SENSORS))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC1884C)
    (at 260.731 135.128)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /6071534B)
    (attr smd)
    (fp_text reference D19 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 PLANT6_MOIST))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 3_3V))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC18837)
    (at 192.786 102.87 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /6058D950)
    (attr smd)
    (fp_text reference D18 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D18-Pad3)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 3_3V))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC187FE)
    (at 188.976 92.71 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /605F7078)
    (attr smd)
    (fp_text reference D16 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 CUSTOM_GPIO))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 3_3V))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC187E9)
    (at 253.619 135.128)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /606FC204)
    (attr smd)
    (fp_text reference D15 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 PLANT5_MOIST))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 3_3V))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC187B0)
    (at 245.999 135.128)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /606E1639)
    (attr smd)
    (fp_text reference D13 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 PLANT4_MOIST))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 3_3V))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC1879B)
    (at 238.506 135.128)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /606C8B56)
    (attr smd)
    (fp_text reference D12 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 PLANT3_MOIST))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 3_3V))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC18786)
    (at 230.886 135.128)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /606B065D)
    (attr smd)
    (fp_text reference D11 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 PLANT2_MOIST))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 3_3V))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC18771)
    (at 223.266 135.128)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /6068A851)
    (attr smd)
    (fp_text reference D10 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 PLANT1_MOIST))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 3_3V))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC2CA0F)
    (at 215.646 135.128)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /6066FB98)
    (attr smd)
    (fp_text reference D9 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 PLANT0_MOIST))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 3_3V))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_SMD:D_SOD-123F (layer F.Cu) (tedit 587F7769) (tstamp 5FC18747)
    (at 245.11 78.486 180)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (path /60005761)
    (attr smd)
    (fp_text reference D8 (at -0.127 -1.905) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "40V 1A" (at 0 2.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -1) (end -2.2 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 0.9) (end -1.4 -0.9) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.9) (end -1.4 0.9) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.9) (end 1.4 0.9) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.9) (end 1.4 -0.9) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 -1.15) (end 2.2 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.2 -1.15) (end 2.2 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.2 1.15) (end -2.2 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.15) (end -2.2 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 1) (end 1.65 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 -1) (end 1.65 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at -0.127 -1.905) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.4 0 180) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(D8-Pad2)"))
    (pad 1 smd rect (at -1.4 0 180) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 17 PUMP_PWR))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module misc_footprints:BatteryHolder_Keystone_1042_1x18650 (layer F.Cu) (tedit 5F8201AB) (tstamp 5F9429A3)
    (at 215.9 54.61 180)
    (descr "Battery holder for 18650 cylindrical cells http://www.keyelco.com/product.cfm/product_id/918")
    (tags "18650 Keystone 1042 Li-ion")
    (path /5F8D742C)
    (attr smd)
    (fp_text reference J4 (at 0 -11.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x02_Female (at 0 11.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -42.5 -4.75) (end -42.5 -7.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -43.75 -6) (end -41.25 -6) (layer F.SilkS) (width 0.12))
    (fp_line (start -39.03 3.68) (end -43.5 3.68) (layer F.CrtYd) (width 0.05))
    (fp_line (start -43.5 3.68) (end -43.5 -3.68) (layer F.CrtYd) (width 0.05))
    (fp_line (start -43.5 -3.68) (end -39.03 -3.68) (layer F.CrtYd) (width 0.05))
    (fp_line (start 43.5 -3.68) (end 39.03 -3.68) (layer F.CrtYd) (width 0.05))
    (fp_line (start 39.03 3.68) (end 43.5 3.68) (layer F.CrtYd) (width 0.05))
    (fp_line (start -39.03 -10.83) (end -39.03 -3.68) (layer F.CrtYd) (width 0.05))
    (fp_line (start -39.03 10.83) (end -39.03 3.68) (layer F.CrtYd) (width 0.05))
    (fp_line (start 39.03 -10.83) (end 39.03 -3.68) (layer F.CrtYd) (width 0.05))
    (fp_line (start -39.03 -10.83) (end 39.03 -10.83) (layer F.CrtYd) (width 0.05))
    (fp_line (start -39.03 10.83) (end 39.03 10.83) (layer F.CrtYd) (width 0.05))
    (fp_line (start 38.53 -10.33) (end 38.53 10.33) (layer F.Fab) (width 0.1))
    (fp_line (start -33.3675 -10.33) (end 38.53 -10.33) (layer F.Fab) (width 0.1))
    (fp_line (start 43.75 -6) (end 41.25 -6) (layer F.SilkS) (width 0.12))
    (fp_line (start -38.53 -5.1675) (end -38.53 10.33) (layer F.Fab) (width 0.1))
    (fp_line (start -38.53 10.33) (end 38.53 10.33) (layer F.Fab) (width 0.1))
    (fp_line (start 38.64 -3.44) (end 38.64 -10.42) (layer F.SilkS) (width 0.12))
    (fp_line (start 38.64 -10.44) (end -38.64 -10.44) (layer F.SilkS) (width 0.12))
    (fp_line (start -38.64 -10.44) (end -38.64 -3.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 38.64 3.44) (end 38.64 10.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 38.64 10.44) (end -38.64 10.44) (layer F.SilkS) (width 0.12))
    (fp_line (start -38.64 10.44) (end -38.64 3.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 39.03 10.83) (end 39.03 3.68) (layer F.CrtYd) (width 0.05))
    (fp_line (start 43.5 3.68) (end 43.5 -3.68) (layer F.CrtYd) (width 0.05))
    (fp_line (start -38.64 -3.44) (end -43 -3.44) (layer F.SilkS) (width 0.12))
    (fp_line (start -33.3675 -10.33) (end -38.53 -5.1675) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at -39.33 0 180) (size 7.34 6.35) (drill 2) (layers *.Cu *.Mask)
      (net 45 VCC_BATT))
    (pad 2 thru_hole rect (at 39.33 0 180) (size 7.34 6.35) (drill 2) (layers *.Cu *.Mask)
      (net 43 GND_BATT))
    (pad "" np_thru_hole circle (at 27.6 -8 180) (size 3.45 3.45) (drill 3.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -27.6 8 180) (size 3.45 3.45) (drill 3.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -35.93 -8 180) (size 2.39 2.39) (drill 2.39) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Keystone_1042_1x18650.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157) (tstamp 5F601710)
    (at 215.138 41.783)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (path /5F02FBC0)
    (fp_text reference U1 (at -2.54 0.127) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DS18B20 (at 1.27 2.79) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 1.75) (end 3 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.46 -2.73) (end 4 -2.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4 2.01) (end 4 -2.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4 2.01) (end -1.46 2.01) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 1.27 0) (end 1.27 -2.6) (angle 135) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 1.27 -2.48) (angle -135) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end 1.27 -2.6) (angle -135) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 1.27 -2.48) (angle 135) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 24 PWR_SENSORS))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 21 Temp))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F6016FE)
    (at 260.35 129.54 90)
    (descr "JST EH series connector, B3B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F6A8678)
    (fp_text reference S6 (at -1.27 -2.794 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x03_Male (at 2.5 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 7.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 2.2) (end 7.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 8 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 2.7) (end 8 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 7.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 2.31) (end 7.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 7.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 -1.21) (end 7.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 0) (end 7.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 0.81) (end 6.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.61 0.81) (end 6.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.5 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 3 thru_hole oval (at 5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 24 PWR_SENSORS))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 40 "Net-(R49-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 7 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F6016DD)
    (at 252.73 129.54 90)
    (descr "JST EH series connector, B3B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F6A0EA1)
    (fp_text reference S5 (at -1.27 -2.794 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x03_Male (at 2.5 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 7.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 2.2) (end 7.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 8 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 2.7) (end 8 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 7.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 2.31) (end 7.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 7.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 -1.21) (end 7.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 0) (end 7.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 0.81) (end 6.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.61 0.81) (end 6.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.5 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 3 thru_hole oval (at 5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 24 PWR_SENSORS))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 38 "Net-(R45-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 7 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F6016BC)
    (at 245.11 129.54 90)
    (descr "JST EH series connector, B3B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F695628)
    (fp_text reference S4 (at -1.524 -2.794 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x03_Male (at 2.5 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 7.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 2.2) (end 7.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 8 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 2.7) (end 8 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 7.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 2.31) (end 7.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 7.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 -1.21) (end 7.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 0) (end 7.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 0.81) (end 6.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.61 0.81) (end 6.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.5 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 3 thru_hole oval (at 5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 24 PWR_SENSORS))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 36 "Net-(R43-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 7 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F60169B)
    (at 237.49 129.54 90)
    (descr "JST EH series connector, B3B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F68ACC2)
    (fp_text reference S3 (at -1.524 -2.8 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x03_Male (at 2.5 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 7.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 2.2) (end 7.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 8 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 2.7) (end 8 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 7.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 2.31) (end 7.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 7.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 -1.21) (end 7.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 0) (end 7.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 0.81) (end 6.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.61 0.81) (end 6.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.5 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 3 thru_hole oval (at 5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 24 PWR_SENSORS))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 34 "Net-(R41-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 7 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F63AEC1)
    (at 229.87 129.54 90)
    (descr "JST EH series connector, B3B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F68A563)
    (fp_text reference S2 (at -1.27 -3.048 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x03_Male (at 2.5 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 7.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 2.2) (end 7.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 8 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 2.7) (end 8 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 7.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 2.31) (end 7.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 7.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 -1.21) (end 7.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 0) (end 7.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 0.81) (end 6.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.61 0.81) (end 6.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.5 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 3 thru_hole oval (at 5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 24 PWR_SENSORS))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 32 "Net-(R39-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 7 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F601659)
    (at 222.25 129.54 90)
    (descr "JST EH series connector, B3B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F6870CB)
    (fp_text reference S1 (at -1.778 -2.794 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x03_Male (at 2.5 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 7.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 2.2) (end 7.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 8 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 2.7) (end 8 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 7.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 2.31) (end 7.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 7.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 -1.21) (end 7.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 0) (end 7.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 0.81) (end 6.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.61 0.81) (end 6.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.5 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 3 thru_hole oval (at 5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 24 PWR_SENSORS))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 30 "Net-(R37-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 7 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F63AF8A)
    (at 214.63 129.54 90)
    (descr "JST EH series connector, B3B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F6785CE)
    (fp_text reference S0 (at -1.778 -2.921 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x03_Male (at 2.5 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 7.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 2.2) (end 7.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 7.5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 8 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 2.7) (end 8 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 7.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 2.31) (end 7.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 7.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 -1.21) (end 7.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 0) (end 7.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.61 0.81) (end 6.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.61 0.81) (end 6.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.5 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 3 thru_hole oval (at 5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 24 PWR_SENSORS))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 28 "Net-(R35-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 7 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B3B-EH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F6012E3)
    (at 260.35 113.03 90)
    (descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F6C56E4)
    (fp_text reference PUMP6 (at 1.25 -2.8 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x02_Female (at 1.25 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 5 2.2) (end 5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 5.5 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.5 2.7) (end 5.5 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.5 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 5.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 2.31) (end 5.11 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 4.61 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.61 -1.21) (end 4.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.61 0) (end 5.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 0.81) (end 4.11 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.11 0.81) (end 4.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 PLANT6_PUMP))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 17 PUMP_PWR))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F6012C3)
    (at 252.73 113.03 90)
    (descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F6C50F5)
    (fp_text reference PUMP5 (at 1.25 -2.8 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x02_Female (at 1.25 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 5 2.2) (end 5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 5.5 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.5 2.7) (end 5.5 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.5 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 5.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 2.31) (end 5.11 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 4.61 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.61 -1.21) (end 4.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.61 0) (end 5.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 0.81) (end 4.11 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.11 0.81) (end 4.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 PLANT5_PUMP))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 17 PUMP_PWR))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F6012A3)
    (at 245.11 113.03 90)
    (descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F6C4B8E)
    (fp_text reference PUMP4 (at 1.25 -2.8 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x02_Female (at 1.25 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 5 2.2) (end 5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 5.5 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.5 2.7) (end 5.5 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.5 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 5.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 2.31) (end 5.11 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 4.61 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.61 -1.21) (end 4.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.61 0) (end 5.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 0.81) (end 4.11 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.11 0.81) (end 4.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 PLANT4_PUMP))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 17 PUMP_PWR))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F601283)
    (at 237.49 113.03 90)
    (descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F6C4568)
    (fp_text reference PUMP3 (at 1.25 -2.8 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x02_Female (at 1.25 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 5 2.2) (end 5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 5.5 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.5 2.7) (end 5.5 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.5 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 5.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 2.31) (end 5.11 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 4.61 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.61 -1.21) (end 4.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.61 0) (end 5.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 0.81) (end 4.11 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.11 0.81) (end 4.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 PLANT3_PUMP))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 17 PUMP_PWR))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F601263)
    (at 229.87 113.03 90)
    (descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F6C3F83)
    (fp_text reference PUMP2 (at 1.25 -2.8 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x02_Female (at 1.25 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 5 2.2) (end 5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 5.5 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.5 2.7) (end 5.5 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.5 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 5.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 2.31) (end 5.11 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 4.61 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.61 -1.21) (end 4.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.61 0) (end 5.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 0.81) (end 4.11 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.11 0.81) (end 4.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 PLANT2_PUMP))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 17 PUMP_PWR))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F601243)
    (at 222.25 113.03 90)
    (descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F6C393A)
    (fp_text reference PUMP1 (at 1.25 -2.8 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x02_Female (at 1.25 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 5 2.2) (end 5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 5.5 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.5 2.7) (end 5.5 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.5 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 5.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 2.31) (end 5.11 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 4.61 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.61 -1.21) (end 4.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.61 0) (end 5.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 0.81) (end 4.11 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.11 0.81) (end 4.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 PLANT1_PUMP))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 17 PUMP_PWR))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F60D6DB)
    (at 214.63 113.03 90)
    (descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F6C304F)
    (fp_text reference PUMP0 (at 1.25 -2.8 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x02_Female (at 1.25 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 5 2.2) (end 5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 5 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 5.5 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.5 2.7) (end 5.5 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.5 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 5.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 2.31) (end 5.11 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 4.61 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.61 -1.21) (end 4.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.61 0) (end 5.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.11 0.81) (end 4.11 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.11 0.81) (end 4.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 PLANT0_PUMP))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 17 PUMP_PWR))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C) (tstamp 5F6011E2)
    (at 173.99 86.36 270)
    (descr "JST EH series connector, B4B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (path /5F8A6800)
    (fp_text reference J5 (at 3.75 -2.8 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 3.75 3.4 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -1.6) (end -2.5 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.2) (end 10 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 10 2.2) (end 10 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 10 -1.6) (end -2.5 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3 -2.1) (end -3 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3 2.7) (end 10.5 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.5 2.7) (end 10.5 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.5 -2.1) (end -3 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.61 -1.71) (end -2.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 2.31) (end 10.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.11 2.31) (end 10.11 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.11 -1.71) (end -2.61 -1.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0) (end -2.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 0) (end -2.11 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.11 -1.21) (end 9.61 -1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.61 -1.21) (end 9.61 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.61 0) (end 10.11 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.61 0.81) (end -1.61 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 0.81) (end -1.61 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.11 0.81) (end 9.11 0.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.11 0.81) (end 9.11 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.91 0.11) (end -2.91 2.61) (layer F.Fab) (width 0.1))
    (fp_line (start -2.91 2.61) (end -0.41 2.61) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 3.75 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 19 "Net-(J5-Pad3)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 82 "Net-(J5-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 15 LIPO+))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical (layer B.Cu) (tedit 5C28146C) (tstamp 5F939E8D)
    (at 242.57 61.722)
    (descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (path /5FAFCD50)
    (fp_text reference J7 (at 1.25 3.55) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Conn_01x02 (at 1.25 -4.6) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.45 2.35) (end -2.45 -3.4) (layer B.Fab) (width 0.1))
    (fp_line (start -2.45 -3.4) (end 4.95 -3.4) (layer B.Fab) (width 0.1))
    (fp_line (start 4.95 -3.4) (end 4.95 2.35) (layer B.Fab) (width 0.1))
    (fp_line (start 4.95 2.35) (end -2.45 2.35) (layer B.Fab) (width 0.1))
    (fp_line (start -2.56 2.46) (end -2.56 -3.51) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.56 -3.51) (end 5.06 -3.51) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.06 -3.51) (end 5.06 2.46) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.06 2.46) (end -2.56 2.46) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.95 2.85) (end -2.95 -3.9) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.95 -3.9) (end 5.45 -3.9) (layer B.CrtYd) (width 0.05))
    (fp_line (start 5.45 -3.9) (end 5.45 2.85) (layer B.CrtYd) (width 0.05))
    (fp_line (start 5.45 2.85) (end -2.95 2.85) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.625 2.35) (end 0 1.35) (layer B.Fab) (width 0.1))
    (fp_line (start 0 1.35) (end 0.625 2.35) (layer B.Fab) (width 0.1))
    (fp_line (start 0.75 2.45) (end 0.75 1.7) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.75 1.7) (end 1.75 1.7) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.75 1.7) (end 1.75 2.45) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.75 2.45) (end 0.75 2.45) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.55 2.45) (end -2.55 1.7) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.55 1.7) (end -0.75 1.7) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.75 1.7) (end -0.75 2.45) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.75 2.45) (end -2.55 2.45) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.25 2.45) (end 3.25 1.7) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.25 1.7) (end 5.05 1.7) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.05 1.7) (end 5.05 2.45) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.05 2.45) (end 3.25 2.45) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.55 0.2) (end -1.8 0.2) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.8 0.2) (end -1.8 -2.75) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.8 -2.75) (end 1.25 -2.75) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.05 0.2) (end 4.3 0.2) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.3 0.2) (end 4.3 -2.75) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.3 -2.75) (end 1.25 -2.75) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.6 2.75) (end -2.85 2.75) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.85 2.75) (end -2.85 1.5) (layer B.SilkS) (width 0.12))
    (fp_text user %R (at 1.25 -2.7) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 2 thru_hole oval (at 2.5 0) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 PUMP_PWR))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 7 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF) (tstamp 5FAC87EB)
    (at 172.974 71.374)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (path /5FCD9EFE)
    (attr smd)
    (fp_text reference C10 (at 0 -1.68) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 0 1.68) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (pad 2 smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 44 "Net-(C10-Pad2)"))
    (pad 1 smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 43 GND_BATT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module misc_footprints:SOT95P280X135-6N (layer F.Cu) (tedit 5FAC25EE) (tstamp 5FAC8803)
    (at 172.72 74.93 90)
    (descr <b>SOT2-23-6</b><br>)
    (path /5FB36987)
    (attr smd)
    (fp_text reference IC1 (at 0 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.015)))
    )
    (fp_text value DW01 (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.015)))
    )
    (fp_line (start -2.125 -1.835) (end 2.125 -1.835) (layer F.Fab) (width 0.05))
    (fp_line (start 2.125 -1.835) (end 2.125 1.835) (layer F.Fab) (width 0.05))
    (fp_line (start 2.125 1.835) (end -2.125 1.835) (layer F.Fab) (width 0.05))
    (fp_line (start -2.125 1.835) (end -2.125 -1.835) (layer F.Fab) (width 0.05))
    (fp_line (start -0.8 -1.46) (end 0.8 -1.46) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -1.46) (end 0.8 1.46) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 1.46) (end -0.8 1.46) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 1.46) (end -0.8 -1.46) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.51) (end 0.15 -1.46) (layer F.Fab) (width 0.1))
    (fp_line (start -0.275 -1.46) (end 0.275 -1.46) (layer F.SilkS) (width 0.2))
    (fp_line (start 0.275 -1.46) (end 0.275 1.46) (layer F.SilkS) (width 0.2))
    (fp_line (start 0.275 1.46) (end -0.275 1.46) (layer F.SilkS) (width 0.2))
    (fp_line (start -0.275 1.46) (end -0.275 -1.46) (layer F.SilkS) (width 0.2))
    (fp_line (start -1.875 -1.6) (end -0.625 -1.6) (layer F.SilkS) (width 0.2))
    (pad 6 smd rect (at 1.25 -0.95 90) (size 1.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 GND_BATT))
    (pad 5 smd rect (at 1.25 0 90) (size 1.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C10-Pad2)"))
    (pad 4 smd rect (at 1.25 0.95 90) (size 1.25 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.25 0.95 90) (size 1.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 LIPO_OC))
    (pad 2 smd rect (at -1.25 0 90) (size 1.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(IC1-Pad2)"))
    (pad 1 smd rect (at -1.25 -0.95 90) (size 1.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 LIPO_OD))
  )

  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C) (tstamp 5FAC8818)
    (at 174.244 61.468 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5FB813FB)
    (attr smd)
    (fp_text reference Q11 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "N-channel 30V 5A" (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q11-Pad3)"))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 43 GND_BATT))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 46 LIPO_OD))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C) (tstamp 5FAC882D)
    (at 173.228 67.31 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5FB3ECD2)
    (attr smd)
    (fp_text reference Q12 (at 0 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "N-channel 30V 5A" (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q11-Pad3)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 47 LIPO_OC))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module SOT-23-6 (layer F.Cu) (tedit 5FBEB024) (tstamp 5FC1F8CA)
    (at 240.03 75.184 180)
    (path /5FE4C408)
    (attr smd)
    (fp_text reference U4 (at 0.076237 -0.079439 180) (layer F.SilkS)
      (effects (font (size 0.600291 0.600291) (thickness 0.015)))
    )
    (fp_text value SX1308 (at 0 0) (layer F.Fab)
      (effects (font (size 0.787402 0.787402) (thickness 0.015)))
    )
    (fp_circle (center -1.2 -1.7) (end -0.9764 -1.7) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.7 -1.5) (end 0.7 -1.5) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.7 1.5) (end -0.7 -1.5) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.7 1.5) (end -0.7 1.5) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.7 -1.5) (end 0.7 1.5) (layer F.SilkS) (width 0.1524))
    (pad 2 smd rect (at -1.35 0 180) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.35 -0.95 180) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(D8-Pad2)"))
    (pad 3 smd rect (at -1.35 0.95 180) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R21-Pad2)"))
    (pad 4 smd rect (at 1.35 0.95 180) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 PWR_PUMP_CONVERTER))
    (pad 6 smd rect (at 1.35 -0.95 180) (size 1 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.35 0 180) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 PWR_PUMP_CONVERTER))
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC2CCDF)
    (at 213.868 104.902)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /6017AD7A)
    (attr smd)
    (fp_text reference D14 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 PLANT0_PUMP))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 PUMP_PWR))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC2CCF4)
    (at 221.234 104.902)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /6026C1A4)
    (attr smd)
    (fp_text reference D17 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 PUMP_PWR))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 PLANT1_PUMP))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC2CD09)
    (at 228.854 104.902)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /602A20F5)
    (attr smd)
    (fp_text reference D20 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 PLANT2_PUMP))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 PUMP_PWR))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC2CD1E)
    (at 236.728 104.902)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /602C1348)
    (attr smd)
    (fp_text reference D21 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 PLANT3_PUMP))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 PUMP_PWR))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC2CD33)
    (at 244.348 104.902)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /60303415)
    (attr smd)
    (fp_text reference D22 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 PUMP_PWR))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 PLANT4_PUMP))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC2CD48)
    (at 252.222 104.902)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /603230D8)
    (attr smd)
    (fp_text reference D23 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 PUMP_PWR))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 PLANT5_PUMP))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57) (tstamp 5FC2CD5D)
    (at 259.588 104.902)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /603441E6)
    (attr smd)
    (fp_text reference D24 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40-04 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 PUMP_PWR))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 PLANT6_PUMP))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_D12.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1) (tstamp 5FE0BA4C)
    (at 217.2208 85.1916)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (path /6014F76F)
    (fp_text reference C14 (at 2.5 -7.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100u (at 2.5 7.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 2.5 0) (end 8.75 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 8.87 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.5 0) (end 9 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.866489 -2.7375) (end -1.616489 -2.7375) (layer F.Fab) (width 0.1))
    (fp_line (start -2.241489 -3.3625) (end -2.241489 -2.1125) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 -6.33) (end 2.5 6.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.54 -6.33) (end 2.54 6.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.58 -6.33) (end 2.58 6.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.62 -6.329) (end 2.62 6.329) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.66 -6.328) (end 2.66 6.328) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.7 -6.327) (end 2.7 6.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.74 -6.326) (end 2.74 6.326) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.78 -6.324) (end 2.78 6.324) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.82 -6.322) (end 2.82 6.322) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.86 -6.32) (end 2.86 6.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.9 -6.318) (end 2.9 6.318) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.94 -6.315) (end 2.94 6.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.98 -6.312) (end 2.98 6.312) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.02 -6.309) (end 3.02 6.309) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.06 -6.306) (end 3.06 6.306) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.1 -6.302) (end 3.1 6.302) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.14 -6.298) (end 3.14 6.298) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.18 -6.294) (end 3.18 6.294) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.221 -6.29) (end 3.221 6.29) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.261 -6.285) (end 3.261 6.285) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.301 -6.28) (end 3.301 6.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.341 -6.275) (end 3.341 6.275) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.381 -6.269) (end 3.381 6.269) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.421 -6.264) (end 3.421 6.264) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.461 -6.258) (end 3.461 6.258) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.501 -6.252) (end 3.501 6.252) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.541 -6.245) (end 3.541 6.245) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.581 -6.238) (end 3.581 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.581 1.44) (end 3.581 6.238) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.621 -6.231) (end 3.621 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.621 1.44) (end 3.621 6.231) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.661 -6.224) (end 3.661 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.661 1.44) (end 3.661 6.224) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.701 -6.216) (end 3.701 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.701 1.44) (end 3.701 6.216) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.741 -6.209) (end 3.741 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.741 1.44) (end 3.741 6.209) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.781 -6.201) (end 3.781 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.781 1.44) (end 3.781 6.201) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.821 -6.192) (end 3.821 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.821 1.44) (end 3.821 6.192) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.861 -6.184) (end 3.861 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.861 1.44) (end 3.861 6.184) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.901 -6.175) (end 3.901 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.901 1.44) (end 3.901 6.175) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.941 -6.166) (end 3.941 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.941 1.44) (end 3.941 6.166) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.981 -6.156) (end 3.981 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.981 1.44) (end 3.981 6.156) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.021 -6.146) (end 4.021 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.021 1.44) (end 4.021 6.146) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.061 -6.137) (end 4.061 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.061 1.44) (end 4.061 6.137) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.101 -6.126) (end 4.101 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.101 1.44) (end 4.101 6.126) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.141 -6.116) (end 4.141 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.141 1.44) (end 4.141 6.116) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.181 -6.105) (end 4.181 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.181 1.44) (end 4.181 6.105) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.221 -6.094) (end 4.221 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.221 1.44) (end 4.221 6.094) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.261 -6.083) (end 4.261 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.261 1.44) (end 4.261 6.083) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.301 -6.071) (end 4.301 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.301 1.44) (end 4.301 6.071) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.341 -6.059) (end 4.341 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.341 1.44) (end 4.341 6.059) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.381 -6.047) (end 4.381 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.381 1.44) (end 4.381 6.047) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.421 -6.034) (end 4.421 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.421 1.44) (end 4.421 6.034) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.461 -6.021) (end 4.461 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.461 1.44) (end 4.461 6.021) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.501 -6.008) (end 4.501 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.501 1.44) (end 4.501 6.008) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.541 -5.995) (end 4.541 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.541 1.44) (end 4.541 5.995) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.581 -5.981) (end 4.581 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.581 1.44) (end 4.581 5.981) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.621 -5.967) (end 4.621 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.621 1.44) (end 4.621 5.967) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.661 -5.953) (end 4.661 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.661 1.44) (end 4.661 5.953) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.701 -5.939) (end 4.701 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.701 1.44) (end 4.701 5.939) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.741 -5.924) (end 4.741 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.741 1.44) (end 4.741 5.924) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.781 -5.908) (end 4.781 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.781 1.44) (end 4.781 5.908) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.821 -5.893) (end 4.821 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.821 1.44) (end 4.821 5.893) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.861 -5.877) (end 4.861 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.861 1.44) (end 4.861 5.877) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.901 -5.861) (end 4.901 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.901 1.44) (end 4.901 5.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.941 -5.845) (end 4.941 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.941 1.44) (end 4.941 5.845) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.981 -5.828) (end 4.981 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.981 1.44) (end 4.981 5.828) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.021 -5.811) (end 5.021 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.021 1.44) (end 5.021 5.811) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.061 -5.793) (end 5.061 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.061 1.44) (end 5.061 5.793) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.101 -5.776) (end 5.101 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.101 1.44) (end 5.101 5.776) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.141 -5.758) (end 5.141 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.141 1.44) (end 5.141 5.758) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.181 -5.739) (end 5.181 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.181 1.44) (end 5.181 5.739) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.221 -5.721) (end 5.221 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.221 1.44) (end 5.221 5.721) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.261 -5.702) (end 5.261 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.261 1.44) (end 5.261 5.702) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.301 -5.682) (end 5.301 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.301 1.44) (end 5.301 5.682) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.341 -5.662) (end 5.341 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.341 1.44) (end 5.341 5.662) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.381 -5.642) (end 5.381 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.381 1.44) (end 5.381 5.642) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.421 -5.622) (end 5.421 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.421 1.44) (end 5.421 5.622) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.461 -5.601) (end 5.461 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.461 1.44) (end 5.461 5.601) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.501 -5.58) (end 5.501 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.501 1.44) (end 5.501 5.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.541 -5.558) (end 5.541 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.541 1.44) (end 5.541 5.558) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.581 -5.536) (end 5.581 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.581 1.44) (end 5.581 5.536) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.621 -5.514) (end 5.621 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.621 1.44) (end 5.621 5.514) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.661 -5.491) (end 5.661 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.661 1.44) (end 5.661 5.491) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.701 -5.468) (end 5.701 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.701 1.44) (end 5.701 5.468) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.741 -5.445) (end 5.741 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.741 1.44) (end 5.741 5.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.781 -5.421) (end 5.781 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.781 1.44) (end 5.781 5.421) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.821 -5.397) (end 5.821 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.821 1.44) (end 5.821 5.397) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.861 -5.372) (end 5.861 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.861 1.44) (end 5.861 5.372) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.901 -5.347) (end 5.901 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.901 1.44) (end 5.901 5.347) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.941 -5.322) (end 5.941 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.941 1.44) (end 5.941 5.322) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.981 -5.296) (end 5.981 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.981 1.44) (end 5.981 5.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.021 -5.27) (end 6.021 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.021 1.44) (end 6.021 5.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.061 -5.243) (end 6.061 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.061 1.44) (end 6.061 5.243) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.101 -5.216) (end 6.101 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.101 1.44) (end 6.101 5.216) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.141 -5.188) (end 6.141 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.141 1.44) (end 6.141 5.188) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.181 -5.16) (end 6.181 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.181 1.44) (end 6.181 5.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.221 -5.131) (end 6.221 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.221 1.44) (end 6.221 5.131) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.261 -5.102) (end 6.261 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.261 1.44) (end 6.261 5.102) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.301 -5.073) (end 6.301 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.301 1.44) (end 6.301 5.073) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.341 -5.043) (end 6.341 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.341 1.44) (end 6.341 5.043) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.381 -5.012) (end 6.381 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.381 1.44) (end 6.381 5.012) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.421 -4.982) (end 6.421 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.421 1.44) (end 6.421 4.982) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.461 -4.95) (end 6.461 4.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.501 -4.918) (end 6.501 4.918) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.541 -4.885) (end 6.541 4.885) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.581 -4.852) (end 6.581 4.852) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.621 -4.819) (end 6.621 4.819) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.661 -4.785) (end 6.661 4.785) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.701 -4.75) (end 6.701 4.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.741 -4.714) (end 6.741 4.714) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.781 -4.678) (end 6.781 4.678) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.821 -4.642) (end 6.821 4.642) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.861 -4.605) (end 6.861 4.605) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.901 -4.567) (end 6.901 4.567) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.941 -4.528) (end 6.941 4.528) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.981 -4.489) (end 6.981 4.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.021 -4.449) (end 7.021 4.449) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.061 -4.408) (end 7.061 4.408) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.101 -4.367) (end 7.101 4.367) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.141 -4.325) (end 7.141 4.325) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.181 -4.282) (end 7.181 4.282) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.221 -4.238) (end 7.221 4.238) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.261 -4.194) (end 7.261 4.194) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.301 -4.148) (end 7.301 4.148) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.341 -4.102) (end 7.341 4.102) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.381 -4.055) (end 7.381 4.055) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.421 -4.007) (end 7.421 4.007) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.461 -3.957) (end 7.461 3.957) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.501 -3.907) (end 7.501 3.907) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.541 -3.856) (end 7.541 3.856) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.581 -3.804) (end 7.581 3.804) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.621 -3.75) (end 7.621 3.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.661 -3.696) (end 7.661 3.696) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.701 -3.64) (end 7.701 3.64) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.741 -3.583) (end 7.741 3.583) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.781 -3.524) (end 7.781 3.524) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.821 -3.464) (end 7.821 3.464) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.861 -3.402) (end 7.861 3.402) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.901 -3.339) (end 7.901 3.339) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.941 -3.275) (end 7.941 3.275) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.981 -3.208) (end 7.981 3.208) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.021 -3.14) (end 8.021 3.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.061 -3.069) (end 8.061 3.069) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.101 -2.996) (end 8.101 2.996) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.141 -2.921) (end 8.141 2.921) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.181 -2.844) (end 8.181 2.844) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.221 -2.764) (end 8.221 2.764) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.261 -2.681) (end 8.261 2.681) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.301 -2.594) (end 8.301 2.594) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.341 -2.504) (end 8.341 2.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.381 -2.41) (end 8.381 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.421 -2.312) (end 8.421 2.312) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.461 -2.209) (end 8.461 2.209) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.501 -2.1) (end 8.501 2.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.541 -1.984) (end 8.541 1.984) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.581 -1.861) (end 8.581 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.621 -1.728) (end 8.621 1.728) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.661 -1.583) (end 8.661 1.583) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.701 -1.422) (end 8.701 1.422) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.741 -1.241) (end 8.741 1.241) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.781 -1.028) (end 8.781 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.821 -0.757) (end 8.821 0.757) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.861 -0.317) (end 8.861 0.317) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.317082 -3.575) (end -3.067082 -3.575) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.692082 -4.2) (end -3.692082 -2.95) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 3_3V))
    (pad 2 thru_hole circle (at 5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (dimension 26.173095 (width 0.15) (layer Cmts.User)
    (gr_text "26.173 mm" (at 277.257459 88.035181 -88.33166255) (layer Cmts.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (feature1 (pts (xy 268.986 75.184) (xy 276.163182 74.974956)))
    (feature2 (pts (xy 269.748 101.346) (xy 276.925182 101.136956)))
    (crossbar (pts (xy 276.33901 101.154029) (xy 275.57701 74.992029)))
    (arrow1a (pts (xy 275.57701 74.992029) (xy 276.195979 76.100982)))
    (arrow1b (pts (xy 275.57701 74.992029) (xy 275.023635 76.135128)))
    (arrow2a (pts (xy 276.33901 101.154029) (xy 276.892385 100.01093)))
    (arrow2b (pts (xy 276.33901 101.154029) (xy 275.720041 100.045076)))
  )
  (dimension 52.075575 (width 0.15) (layer Cmts.User)
    (gr_text "52.076 mm" (at 282.597337 75.031893 -89.16158503) (layer Cmts.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (feature1 (pts (xy 263.144 49.276) (xy 281.502834 49.007334)))
    (feature2 (pts (xy 263.906 101.346) (xy 282.264834 101.077334)))
    (crossbar (pts (xy 281.678476 101.085915) (xy 280.916476 49.015915)))
    (arrow1a (pts (xy 280.916476 49.015915) (xy 281.519318 50.133717)))
    (arrow1b (pts (xy 280.916476 49.015915) (xy 280.346602 50.150879)))
    (arrow2a (pts (xy 281.678476 101.085915) (xy 282.24835 99.950951)))
    (arrow2b (pts (xy 281.678476 101.085915) (xy 281.075634 99.968113)))
  )
  (dimension 10.163175 (width 0.15) (layer Cmts.User)
    (gr_text "10.163 mm" (at 263.867164 73.503565 1.432096184) (layer Cmts.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (feature1 (pts (xy 259.08 85.344) (xy 258.804998 74.343921)))
    (feature2 (pts (xy 269.24 85.09) (xy 268.964998 74.089921)))
    (crossbar (pts (xy 268.979654 74.676159) (xy 258.819654 74.930159)))
    (arrow1a (pts (xy 258.819654 74.930159) (xy 259.93115 74.315768)))
    (arrow1b (pts (xy 258.819654 74.930159) (xy 259.960462 75.488243)))
    (arrow2a (pts (xy 268.979654 74.676159) (xy 267.838846 74.118075)))
    (arrow2b (pts (xy 268.979654 74.676159) (xy 267.868158 75.29055)))
  )
  (gr_text "PlantCtrl V0.5" (at 215.4936 48.514) (layer B.SilkS) (tstamp 5F9CBCD8)
    (effects (font (size 4 4) (thickness 0.5)) (justify mirror))
  )
  (gr_text "PlantCtrl V0.5\n" (at 246.4308 90.3732) (layer F.SilkS) (tstamp 5F9CBCD5)
    (effects (font (size 4 4) (thickness 0.5)))
  )
  (gr_line (start 170.18 40.64) (end 269.24 40.64) (layer Edge.Cuts) (width 0.05) (tstamp 5F61C1CA))
  (gr_line (start 170.18 43.18) (end 170.18 40.64) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.18 139.7) (end 170.18 43.18) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 269.24 139.7) (end 269.24 40.64) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.18 139.7) (end 269.24 139.7) (layer Edge.Cuts) (width 0.05))

  (via (at 173.99 135.636) (size 4) (drill 3) (layers F.Cu B.Cu) (net 0))
  (via (at 265.43 135.636) (size 4) (drill 3) (layers F.Cu B.Cu) (net 0))
  (via (at 173.99 44.45) (size 4) (drill 3) (layers F.Cu B.Cu) (net 0))
  (via (at 265.43 44.45) (size 4) (drill 3) (layers F.Cu B.Cu) (net 0) (tstamp 5FC2218F))
  (segment (start 223.685 106.353) (end 222.234 104.902) (width 0.2) (layer F.Cu) (net 1) (status 30))
  (segment (start 224.282 106.353) (end 223.685 106.353) (width 0.2) (layer F.Cu) (net 1) (status 30))
  (segment (start 222.25 104.918) (end 222.234 104.902) (width 1) (layer F.Cu) (net 1) (status 30))
  (segment (start 222.25 110.53) (end 222.25 104.918) (width 1) (layer F.Cu) (net 1) (status 30))
  (segment (start 222.234 102.576) (end 221.234 101.576) (width 1) (layer F.Cu) (net 1) (status 20))
  (segment (start 222.234 104.902) (end 222.234 102.576) (width 1) (layer F.Cu) (net 1) (status 10))
  (segment (start 229.87 104.918) (end 229.854 104.902) (width 1) (layer F.Cu) (net 2) (status 30))
  (segment (start 229.87 110.53) (end 229.87 104.918) (width 1) (layer F.Cu) (net 2) (status 30))
  (segment (start 229.854 102.576) (end 229.854 104.902) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 228.854 101.576) (end 229.854 102.576) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 231.305 106.353) (end 229.854 104.902) (width 0.2) (layer F.Cu) (net 2) (status 30))
  (segment (start 231.902 106.353) (end 231.305 106.353) (width 0.2) (layer F.Cu) (net 2) (status 30))
  (segment (start 239.179 106.353) (end 237.728 104.902) (width 0.2) (layer F.Cu) (net 3) (status 30))
  (segment (start 239.776 106.353) (end 239.179 106.353) (width 0.2) (layer F.Cu) (net 3) (status 30))
  (segment (start 237.49 102.338) (end 237.49 110.53) (width 1) (layer F.Cu) (net 3) (status 20))
  (segment (start 236.728 101.576) (end 237.49 102.338) (width 1) (layer F.Cu) (net 3) (status 10))
  (segment (start 246.8355 106.3895) (end 245.348 104.902) (width 0.2) (layer F.Cu) (net 4) (status 30))
  (segment (start 247.396 106.3895) (end 246.8355 106.3895) (width 0.2) (layer F.Cu) (net 4) (status 30))
  (segment (start 245.348 102.576) (end 245.348 104.902) (width 1) (layer F.Cu) (net 4) (status 20))
  (segment (start 244.348 101.576) (end 245.348 102.576) (width 1) (layer F.Cu) (net 4) (status 10))
  (segment (start 245.348 110.292) (end 245.11 110.53) (width 1) (layer F.Cu) (net 4) (status 30))
  (segment (start 245.348 104.902) (end 245.348 110.292) (width 1) (layer F.Cu) (net 4) (status 30))
  (segment (start 252.73 105.394) (end 253.222 104.902) (width 1) (layer F.Cu) (net 5) (status 20))
  (segment (start 252.73 110.53) (end 252.73 105.394) (width 1) (layer F.Cu) (net 5) (status 10))
  (segment (start 253.222 102.576) (end 253.222 104.902) (width 1) (layer F.Cu) (net 5) (status 20))
  (segment (start 252.222 101.576) (end 253.222 102.576) (width 1) (layer F.Cu) (net 5) (status 10))
  (segment (start 253.7825 104.902) (end 255.27 106.3895) (width 0.2) (layer F.Cu) (net 5) (status 20))
  (segment (start 253.222 104.902) (end 253.7825 104.902) (width 0.2) (layer F.Cu) (net 5) (status 10))
  (segment (start 261.1485 104.902) (end 262.636 106.3895) (width 0.2) (layer F.Cu) (net 6) (status 20))
  (segment (start 260.588 104.902) (end 261.1485 104.902) (width 0.2) (layer F.Cu) (net 6) (status 10))
  (segment (start 260.588 102.576) (end 260.588 104.902) (width 1) (layer F.Cu) (net 6) (status 20))
  (segment (start 259.588 101.576) (end 260.588 102.576) (width 1) (layer F.Cu) (net 6) (status 10))
  (segment (start 260.588 110.292) (end 260.35 110.53) (width 1) (layer F.Cu) (net 6) (status 30))
  (segment (start 260.588 104.902) (end 260.588 110.292) (width 1) (layer F.Cu) (net 6) (status 30))
  (segment (start 260.255 129.635) (end 260.35 129.54) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (via (at 213.106 92.202) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 7))
  (segment (start 212.918 92.39) (end 213.106 92.202) (width 1) (layer F.Cu) (net 7))
  (segment (start 212.918 98.576) (end 212.918 92.39) (width 1) (layer F.Cu) (net 7) (status 10))
  (segment (start 212.918 103.902) (end 212.868 103.952) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 212.918 98.576) (end 212.918 103.902) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 220.284 103.902) (end 220.234 103.952) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 220.284 98.576) (end 220.284 103.902) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 227.904 103.902) (end 227.854 103.952) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 227.904 98.576) (end 227.904 103.902) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 235.778 103.902) (end 235.728 103.952) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 235.778 98.576) (end 235.778 103.902) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 243.398 103.902) (end 243.348 103.952) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 243.398 98.576) (end 243.398 103.902) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 220.284 98.576) (end 220.284 92.268) (width 1) (layer F.Cu) (net 7) (status 10))
  (via (at 220.284 92.268) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 7))
  (segment (start 220.218 92.202) (end 220.284 92.268) (width 1) (layer B.Cu) (net 7))
  (segment (start 213.106 92.202) (end 220.218 92.202) (width 1) (layer B.Cu) (net 7))
  (segment (start 258.588 98.626) (end 258.638 98.576) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 258.588 103.952) (end 258.588 98.626) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 227.904 96.332) (end 227.838 96.266) (width 1) (layer F.Cu) (net 7) (status 30))
  (segment (start 227.904 98.576) (end 227.904 96.332) (width 1) (layer F.Cu) (net 7) (status 30))
  (via (at 257.744 92.268) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 7))
  (segment (start 257.744 92.268) (end 258.572 93.096) (width 1) (layer F.Cu) (net 7))
  (segment (start 258.572 93.096) (end 258.572 96.266) (width 1) (layer F.Cu) (net 7) (status 20))
  (segment (start 258.572 98.51) (end 258.638 98.576) (width 1) (layer F.Cu) (net 7) (status 30))
  (segment (start 258.572 96.266) (end 258.572 98.51) (width 1) (layer F.Cu) (net 7) (status 30))
  (segment (start 251.272 96.316) (end 251.222 96.266) (width 1) (layer F.Cu) (net 7) (status 30))
  (segment (start 251.272 98.576) (end 251.272 96.316) (width 1) (layer F.Cu) (net 7) (status 30))
  (segment (start 251.222 92.604) (end 250.886 92.268) (width 1) (layer F.Cu) (net 7))
  (via (at 250.886 92.268) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 7))
  (segment (start 251.222 96.266) (end 251.222 92.604) (width 1) (layer F.Cu) (net 7) (status 10))
  (segment (start 243.398 96.316) (end 243.348 96.266) (width 1) (layer F.Cu) (net 7) (status 30))
  (segment (start 243.398 98.576) (end 243.398 96.316) (width 1) (layer F.Cu) (net 7) (status 30))
  (via (at 242.25 92.268) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 7))
  (segment (start 243.348 96.266) (end 243.348 93.366) (width 1) (layer F.Cu) (net 7) (status 10))
  (segment (start 242.25 92.268) (end 250.886 92.268) (width 1) (layer B.Cu) (net 7))
  (segment (start 243.348 93.366) (end 242.25 92.268) (width 1) (layer F.Cu) (net 7))
  (via (at 235.016 92.268) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 7))
  (segment (start 235.778 93.03) (end 235.016 92.268) (width 1) (layer F.Cu) (net 7))
  (segment (start 235.778 98.576) (end 235.778 93.03) (width 1) (layer F.Cu) (net 7) (status 10))
  (segment (start 235.016 92.268) (end 242.25 92.268) (width 1) (layer B.Cu) (net 7))
  (via (at 227.396 92.268) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 7))
  (segment (start 227.838 92.71) (end 227.396 92.268) (width 1) (layer F.Cu) (net 7))
  (segment (start 227.838 96.266) (end 227.838 92.71) (width 1) (layer F.Cu) (net 7) (status 10))
  (segment (start 227.396 92.268) (end 235.016 92.268) (width 1) (layer B.Cu) (net 7))
  (segment (start 220.284 92.268) (end 227.396 92.268) (width 1) (layer B.Cu) (net 7))
  (segment (start 251.222 98.626) (end 251.272 98.576) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 251.222 103.952) (end 251.222 98.626) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 214.63 129.54) (end 260.35 129.54) (width 1) (layer B.Cu) (net 7) (status 30))
  (segment (start 214.63 134.162) (end 214.646 134.178) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 214.63 129.54) (end 214.63 134.162) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 222.25 134.162) (end 222.266 134.178) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 222.25 129.54) (end 222.25 134.162) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 229.87 129.54) (end 229.87 133.858) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 229.886 133.874) (end 229.886 134.178) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 229.87 133.858) (end 229.886 133.874) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 237.49 134.162) (end 237.506 134.178) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 237.49 129.54) (end 237.49 134.162) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 245.11 134.067) (end 244.999 134.178) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 245.11 129.54) (end 245.11 134.067) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 252.73 134.067) (end 252.619 134.178) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 252.73 129.54) (end 252.73 134.067) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 260.35 133.559) (end 259.731 134.178) (width 0.2) (layer F.Cu) (net 7) (status 20))
  (segment (start 260.35 129.54) (end 260.35 133.559) (width 0.2) (layer F.Cu) (net 7) (status 10))
  (via (at 176.276 66.548) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 7))
  (segment (start 174.178 68.646) (end 176.276 66.548) (width 1.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 174.178 68.81) (end 174.178 68.646) (width 1.2) (layer F.Cu) (net 7) (status 30))
  (via (at 175.26 76.454) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 7))
  (segment (start 174.736 76.978) (end 175.26 76.454) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 174.736 78.74) (end 174.736 76.978) (width 0.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 179.07 63.754) (end 176.276 66.548) (width 1.2) (layer F.Cu) (net 7))
  (segment (start 179.07 63.754) (end 179.07 62.118) (width 1) (layer F.Cu) (net 7) (status 20))
  (segment (start 212.486 131.684) (end 214.63 129.54) (width 0.2) (layer F.Cu) (net 7) (status 20))
  (segment (start 211.328 131.684) (end 212.486 131.684) (width 0.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 259.478676 118.96699) (end 259.07499 119.370676) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 259.07499 119.370676) (end 259.07499 128.26499) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 261.96899 118.96699) (end 259.478676 118.96699) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 259.07499 128.26499) (end 260.35 129.54) (width 0.2) (layer F.Cu) (net 7) (status 20))
  (segment (start 263.144 120.142) (end 261.96899 118.96699) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 185.42 118.5965) (end 199.136 118.5965) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 173.788 113.792) (end 179.705 107.875) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 173.736 113.792) (end 173.788 113.792) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 178.43 106.6) (end 179.705 107.875) (width 0.2) (layer F.Cu) (net 7) (status 20))
  (segment (start 173.99 106.6) (end 178.43 106.6) (width 0.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 240.744998 75.184) (end 240.03 74.469002) (width 0.5) (layer F.Cu) (net 7))
  (segment (start 241.38 75.184) (end 240.744998 75.184) (width 0.5) (layer F.Cu) (net 7) (status 10))
  (segment (start 240.03 73.432) (end 241.58 71.882) (width 0.5) (layer F.Cu) (net 7) (status 20))
  (segment (start 240.03 74.469002) (end 240.03 73.432) (width 0.5) (layer F.Cu) (net 7))
  (segment (start 244.094 74.904) (end 243.56 75.438) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 244.094 73.136) (end 244.094 74.904) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 241.58 67.844) (end 241.3 67.564) (width 1.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 241.58 71.882) (end 241.58 67.844) (width 1.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 241.3 67.564) (end 243.84 67.564) (width 1.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 245.825999 86.062001) (end 247.076 84.812) (width 0.2) (layer F.Cu) (net 7) (status 20))
  (segment (start 242.542001 86.062001) (end 245.825999 86.062001) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 241.316 84.836) (end 242.542001 86.062001) (width 0.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 244.560001 78.063195) (end 244.560001 76.438001) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 244.560001 76.438001) (end 243.56 75.438) (width 0.2) (layer F.Cu) (net 7) (status 20))
  (segment (start 247.076 80.579194) (end 244.560001 78.063195) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 247.076 84.812) (end 247.076 80.579194) (width 0.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 241.3 62.992) (end 242.57 61.722) (width 1.2) (layer F.Cu) (net 7) (status 20))
  (segment (start 241.3 67.564) (end 241.3 62.992) (width 1.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 265.7 73.914) (end 265.938 73.676) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 259.842 73.914) (end 265.7 73.914) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 186.1445 84.8575) (end 186.182 84.82) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 183.134 84.8575) (end 186.1445 84.8575) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 183.134 86.868) (end 183.134 84.8575) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 212.355999 103.439999) (end 212.868 103.952) (width 0.2) (layer F.Cu) (net 7) (status 20))
  (segment (start 210.483999 103.439999) (end 212.355999 103.439999) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 209.64499 104.279008) (end 210.483999 103.439999) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 209.64499 111.81849) (end 209.64499 104.279008) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 210.82 112.9935) (end 209.64499 111.81849) (width 0.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 259.842 73.914) (end 259.842 76.454) (width 1.2) (layer B.Cu) (net 7) (status 30))
  (segment (start 259.842 76.454) (end 258.064 76.454) (width 1.2) (layer B.Cu) (net 7) (status 10))
  (segment (start 256.474 78.044) (end 256.474 92.268) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 258.064 76.454) (end 256.474 78.044) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 256.474 92.268) (end 257.744 92.268) (width 1) (layer B.Cu) (net 7))
  (segment (start 250.886 92.268) (end 256.474 92.268) (width 1) (layer B.Cu) (net 7))
  (segment (start 255.979912 43.688) (end 263.398 51.106088) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 227.584 43.688) (end 255.979912 43.688) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 261.044081 73.914) (end 259.842 73.914) (width 1.2) (layer B.Cu) (net 7) (status 20))
  (segment (start 263.398 71.560081) (end 261.044081 73.914) (width 1.2) (layer B.Cu) (net 7))
  (via (at 191.262 66.548) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 7))
  (segment (start 191.262 71.594) (end 191.262 66.548) (width 1.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 191.262 66.548) (end 204.724 66.548) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 176.276 66.548) (end 191.262 66.548) (width 1.2) (layer B.Cu) (net 7))
  (via (at 263.398 59.436) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 7))
  (segment (start 263.398 59.436) (end 263.398 71.560081) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 263.398 51.106088) (end 263.398 59.436) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 242.57 61.722) (end 242.57 60.198) (width 1.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 243.332 59.436) (end 245.872 59.436) (width 1.2) (layer F.Cu) (net 7))
  (segment (start 242.57 60.198) (end 243.332 59.436) (width 1.2) (layer F.Cu) (net 7))
  (segment (start 245.872 59.436) (end 263.398 59.436) (width 1.2) (layer F.Cu) (net 7))
  (segment (start 228.87 79.73) (end 228.92 79.78) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 228.87 77.216) (end 228.87 79.73) (width 0.2) (layer F.Cu) (net 7) (status 30))
  (via (at 227.584 87.376) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 7))
  (segment (start 227.584 81.116) (end 227.584 87.376) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 228.92 79.78) (end 227.584 81.116) (width 0.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 227.584 92.08) (end 227.396 92.268) (width 0.2) (layer B.Cu) (net 7))
  (segment (start 227.584 87.376) (end 227.584 92.08) (width 0.2) (layer B.Cu) (net 7))
  (via (at 211.455 59.817) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 7))
  (segment (start 211.455 45.466) (end 211.455 59.817) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 215.138 41.783) (end 211.455 45.466) (width 0.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 211.455 59.817) (end 227.584 43.688) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 204.724 66.548) (end 211.455 59.817) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 175.26 67.564) (end 175.26 76.454) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 176.276 66.548) (end 175.26 67.564) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 172.84 93.86) (end 173.99 93.86) (width 1.2) (layer B.Cu) (net 7) (status 20))
  (segment (start 171.704 92.724) (end 172.84 93.86) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 171.704 80.01) (end 171.704 92.724) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 175.26 76.454) (end 171.704 80.01) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 200.61 91.76) (end 200.66 91.71) (width 1.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 198.096 91.76) (end 200.61 91.76) (width 1.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 202.275 90.095) (end 200.66 91.71) (width 1.2) (layer F.Cu) (net 7) (status 20))
  (segment (start 191.262 74.73649) (end 191.262 66.548) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 195.295518 78.770008) (end 191.262 74.73649) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 205.105 90.095) (end 207.518 87.682) (width 1.2) (layer B.Cu) (net 7) (status 10))
  (segment (start 207.518 87.682) (end 207.518 75.946) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 206.427 74.855) (end 205.105 74.855) (width 1.2) (layer B.Cu) (net 7) (status 20))
  (segment (start 207.518 75.946) (end 206.427 74.855) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 258.488002 92.268) (end 257.744 92.268) (width 1) (layer B.Cu) (net 7))
  (segment (start 263.736001 97.515999) (end 258.488002 92.268) (width 1) (layer B.Cu) (net 7))
  (segment (start 263.736001 127.128999) (end 263.736001 97.515999) (width 1) (layer B.Cu) (net 7))
  (segment (start 261.325 129.54) (end 263.736001 127.128999) (width 1) (layer B.Cu) (net 7))
  (segment (start 260.35 129.54) (end 261.325 129.54) (width 1) (layer B.Cu) (net 7) (status 10))
  (segment (start 193.675 133.985) (end 211.963 133.985) (width 1) (layer F.Cu) (net 7) (status 10))
  (segment (start 214.63 131.318) (end 214.63 129.54) (width 1) (layer F.Cu) (net 7) (status 20))
  (segment (start 211.963 133.985) (end 214.63 131.318) (width 1) (layer F.Cu) (net 7))
  (segment (start 190.2335 72.6225) (end 191.262 71.594) (width 1.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 189.930006 85.72001) (end 196.880008 78.770008) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 187.08201 85.72001) (end 189.930006 85.72001) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 186.182 84.82) (end 187.08201 85.72001) (width 0.2) (layer F.Cu) (net 7) (status 10))
  (via (at 196.880008 78.770008) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 7))
  (segment (start 196.880008 78.770008) (end 195.295518 78.770008) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 194.155998 91.76) (end 198.096 91.76) (width 0.2) (layer F.Cu) (net 7) (status 20))
  (segment (start 193.305988 92.61001) (end 194.155998 91.76) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 190.82601 92.61001) (end 193.305988 92.61001) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 189.926 91.71) (end 190.82601 92.61001) (width 0.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 203.138001 90.362001) (end 202.871 90.095) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 203.138001 98.380001) (end 203.138001 90.362001) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 199.648002 101.87) (end 203.138001 98.380001) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 193.736 101.87) (end 199.648002 101.87) (width 0.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 202.871 90.095) (end 202.275 90.095) (width 1.2) (layer F.Cu) (net 7))
  (segment (start 205.105 90.095) (end 202.871 90.095) (width 1.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 173.99 106.6) (end 175.086 106.6) (width 0.2) (layer B.Cu) (net 7) (status 10))
  (segment (start 175.086 106.6) (end 176.53 105.156) (width 0.2) (layer B.Cu) (net 7))
  (segment (start 176.53 96.4) (end 173.99 93.86) (width 0.2) (layer B.Cu) (net 7) (status 20))
  (segment (start 176.53 105.156) (end 176.53 96.4) (width 0.2) (layer B.Cu) (net 7))
  (segment (start 175.514 113.792) (end 173.736 113.792) (width 0.2) (layer F.Cu) (net 7) (status 20))
  (segment (start 177.292 115.57) (end 175.514 113.792) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 177.292 121.666) (end 177.292 115.57) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 178.308 122.682) (end 177.292 121.666) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 180.34 122.682) (end 178.308 122.682) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 184.4255 118.5965) (end 180.34 122.682) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 185.42 118.5965) (end 184.4255 118.5965) (width 0.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 190.6835 72.1725) (end 191.262 71.594) (width 1.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 228.92 80.93) (end 228.92 79.78) (width 0.2) (layer F.Cu) (net 7) (status 20))
  (segment (start 229.020001 81.030001) (end 228.92 80.93) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 231.460001 81.030001) (end 229.020001 81.030001) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 233.111 79.379002) (end 231.460001 81.030001) (width 0.2) (layer F.Cu) (net 7))
  (segment (start 233.111 77.581) (end 233.111 79.379002) (width 0.2) (layer F.Cu) (net 7) (status 10))
  (segment (start 190.221 72.635) (end 191.262 71.594) (width 1.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 186.182 72.635) (end 190.221 72.635) (width 1.2) (layer F.Cu) (net 7) (status 30))
  (segment (start 243.831 75.184) (end 244.085 75.438) (width 0.5) (layer F.Cu) (net 7) (status 30))
  (segment (start 241.38 75.184) (end 243.831 75.184) (width 0.5) (layer F.Cu) (net 7) (status 30))
  (segment (start 205.105 74.855) (end 201.189992 78.770008) (width 1.2) (layer B.Cu) (net 7) (status 10))
  (segment (start 201.189992 78.770008) (end 196.880008 78.770008) (width 1.2) (layer B.Cu) (net 7))
  (segment (start 265.28701 131.57199) (end 261.731 135.128) (width 0.2) (layer F.Cu) (net 8) (status 20))
  (segment (start 265.28701 126.23801) (end 265.28701 131.57199) (width 0.2) (layer F.Cu) (net 8))
  (segment (start 264.287 125.238) (end 265.28701 126.23801) (width 0.2) (layer F.Cu) (net 8) (status 10))
  (via (at 199.136 122.428) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 8))
  (segment (start 199.136 120.6715) (end 199.136 122.428) (width 0.2) (layer F.Cu) (net 8) (status 10))
  (segment (start 263.434314 118.56698) (end 264.287 119.419666) (width 0.2) (layer F.Cu) (net 8))
  (segment (start 255.82902 118.56698) (end 263.434314 118.56698) (width 0.2) (layer F.Cu) (net 8))
  (segment (start 253.60606 120.78994) (end 255.82902 118.56698) (width 0.2) (layer F.Cu) (net 8))
  (segment (start 264.287 119.419666) (end 264.287 125.238) (width 0.2) (layer F.Cu) (net 8) (status 20))
  (segment (start 208.64806 120.78994) (end 253.60606 120.78994) (width 0.2) (layer F.Cu) (net 8))
  (segment (start 207.01 122.428) (end 208.64806 120.78994) (width 0.2) (layer F.Cu) (net 8))
  (segment (start 199.136 122.428) (end 207.01 122.428) (width 0.2) (layer F.Cu) (net 8))
  (segment (start 199.136 122.428) (end 187.92805 111.22005) (width 0.2) (layer B.Cu) (net 8))
  (segment (start 187.92805 111.22005) (end 187.92805 106.117774) (width 0.2) (layer B.Cu) (net 8))
  (segment (start 187.92805 106.117774) (end 182.626 100.815724) (width 0.2) (layer B.Cu) (net 8))
  (segment (start 182.626 93.016) (end 179.705 90.095) (width 0.2) (layer B.Cu) (net 8) (status 20))
  (segment (start 182.626 100.815724) (end 182.626 93.016) (width 0.2) (layer B.Cu) (net 8))
  (segment (start 257.79401 126.36501) (end 256.794 125.365) (width 0.2) (layer F.Cu) (net 9) (status 20))
  (segment (start 257.79401 131.95299) (end 257.79401 126.36501) (width 0.2) (layer F.Cu) (net 9))
  (segment (start 254.619 135.128) (end 257.79401 131.95299) (width 0.2) (layer F.Cu) (net 9) (status 10))
  (segment (start 252.61895 121.18995) (end 212.531559 121.18995) (width 0.2) (layer F.Cu) (net 9))
  (segment (start 256.794 125.365) (end 252.61895 121.18995) (width 0.2) (layer F.Cu) (net 9) (status 10))
  (segment (start 212.531557 121.189952) (end 212.531554 121.189952) (width 0.2) (layer F.Cu) (net 9))
  (segment (start 212.531559 121.18995) (end 212.531557 121.189952) (width 0.2) (layer F.Cu) (net 9))
  (via (at 196.85 122.428) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 9))
  (segment (start 196.85 120.6715) (end 196.85 122.428) (width 0.2) (layer F.Cu) (net 9) (status 10))
  (segment (start 197.550001 123.128001) (end 206.878798 123.128001) (width 0.2) (layer F.Cu) (net 9))
  (segment (start 196.85 122.428) (end 197.550001 123.128001) (width 0.2) (layer F.Cu) (net 9))
  (segment (start 208.816847 121.189952) (end 210.597952 121.189952) (width 0.2) (layer F.Cu) (net 9))
  (segment (start 206.878798 123.128001) (end 208.816847 121.189952) (width 0.2) (layer F.Cu) (net 9))
  (segment (start 210.597952 121.189952) (end 212.531557 121.189952) (width 0.2) (layer F.Cu) (net 9))
  (segment (start 210.363627 121.189952) (end 210.597952 121.189952) (width 0.2) (layer F.Cu) (net 9))
  (segment (start 179.705 92.635) (end 182.158869 95.088869) (width 0.2) (layer B.Cu) (net 9) (status 10))
  (segment (start 182.158869 101.011774) (end 187.52804 106.380944) (width 0.2) (layer B.Cu) (net 9))
  (segment (start 182.158869 95.088869) (end 182.158869 101.011774) (width 0.2) (layer B.Cu) (net 9))
  (segment (start 187.52804 113.10604) (end 187.52804 112.95396) (width 0.2) (layer B.Cu) (net 9))
  (segment (start 196.85 122.428) (end 187.52804 113.10604) (width 0.2) (layer B.Cu) (net 9))
  (segment (start 187.52804 106.380944) (end 187.52804 112.95396) (width 0.2) (layer B.Cu) (net 9))
  (segment (start 250.17401 131.95299) (end 246.999 135.128) (width 0.2) (layer F.Cu) (net 10) (status 20))
  (segment (start 250.17401 126.36501) (end 250.17401 131.95299) (width 0.2) (layer F.Cu) (net 10))
  (segment (start 249.174 125.365) (end 250.17401 126.36501) (width 0.2) (layer F.Cu) (net 10) (status 10))
  (segment (start 249.174 125.365) (end 245.39896 121.58996) (width 0.2) (layer F.Cu) (net 10) (status 10))
  (via (at 194.564 122.428) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 10))
  (segment (start 194.564 120.6715) (end 194.564 122.428) (width 0.2) (layer F.Cu) (net 10) (status 10))
  (segment (start 208.982537 121.58996) (end 210.64204 121.58996) (width 0.2) (layer F.Cu) (net 10))
  (segment (start 207.044487 123.528011) (end 208.982537 121.58996) (width 0.2) (layer F.Cu) (net 10))
  (segment (start 195.664011 123.528011) (end 207.044487 123.528011) (width 0.2) (layer F.Cu) (net 10))
  (segment (start 194.564 122.428) (end 195.664011 123.528011) (width 0.2) (layer F.Cu) (net 10))
  (segment (start 210.64204 121.58996) (end 210.529317 121.58996) (width 0.2) (layer F.Cu) (net 10))
  (segment (start 245.39896 121.58996) (end 210.64204 121.58996) (width 0.2) (layer F.Cu) (net 10))
  (segment (start 179.705 95.175) (end 181.758859 97.228859) (width 0.2) (layer B.Cu) (net 10) (status 10))
  (segment (start 181.758859 101.177462) (end 187.12803 106.546633) (width 0.2) (layer B.Cu) (net 10))
  (segment (start 181.758859 97.228859) (end 181.758859 101.177462) (width 0.2) (layer B.Cu) (net 10))
  (segment (start 187.12803 114.99203) (end 194.564 122.428) (width 0.2) (layer B.Cu) (net 10))
  (segment (start 187.12803 106.546633) (end 187.12803 114.99203) (width 0.2) (layer B.Cu) (net 10))
  (segment (start 242.55401 132.07999) (end 239.506 135.128) (width 0.2) (layer F.Cu) (net 11) (status 20))
  (segment (start 242.55401 126.36501) (end 242.55401 132.07999) (width 0.2) (layer F.Cu) (net 11))
  (segment (start 241.554 125.365) (end 242.55401 126.36501) (width 0.2) (layer F.Cu) (net 11) (status 10))
  (segment (start 238.17897 121.98997) (end 212.862933 121.98997) (width 0.2) (layer F.Cu) (net 11))
  (segment (start 241.554 125.365) (end 238.17897 121.98997) (width 0.2) (layer F.Cu) (net 11) (status 10))
  (via (at 192.278 122.428) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 11))
  (segment (start 192.278 120.6715) (end 192.278 122.428) (width 0.2) (layer F.Cu) (net 11) (status 10))
  (segment (start 193.778021 123.928021) (end 207.210174 123.928021) (width 0.2) (layer F.Cu) (net 11))
  (segment (start 192.278 122.428) (end 193.778021 123.928021) (width 0.2) (layer F.Cu) (net 11))
  (segment (start 209.148225 121.98997) (end 210.88997 121.98997) (width 0.2) (layer F.Cu) (net 11))
  (segment (start 207.210174 123.928021) (end 209.148225 121.98997) (width 0.2) (layer F.Cu) (net 11))
  (segment (start 210.88997 121.98997) (end 210.695005 121.98997) (width 0.2) (layer F.Cu) (net 11))
  (segment (start 212.862933 121.98997) (end 210.88997 121.98997) (width 0.2) (layer F.Cu) (net 11))
  (segment (start 179.705 97.715) (end 181.358849 99.368849) (width 0.2) (layer B.Cu) (net 11) (status 10))
  (segment (start 181.358849 101.343151) (end 186.72802 106.712321) (width 0.2) (layer B.Cu) (net 11))
  (segment (start 181.358849 99.368849) (end 181.358849 101.343151) (width 0.2) (layer B.Cu) (net 11))
  (segment (start 192.278 122.428) (end 186.72802 116.87802) (width 0.2) (layer B.Cu) (net 11))
  (segment (start 186.72802 106.712321) (end 186.72802 116.87802) (width 0.2) (layer B.Cu) (net 11))
  (segment (start 235.06101 126.36501) (end 235.06101 132.22299) (width 0.2) (layer F.Cu) (net 12))
  (segment (start 234.061 125.365) (end 235.06101 126.36501) (width 0.2) (layer F.Cu) (net 12) (status 10))
  (segment (start 232.156 135.128) (end 231.886 135.128) (width 0.2) (layer F.Cu) (net 12) (status 30))
  (segment (start 235.06101 132.22299) (end 232.156 135.128) (width 0.2) (layer F.Cu) (net 12) (status 20))
  (segment (start 234.061 125.365) (end 231.08598 122.38998) (width 0.2) (layer F.Cu) (net 12) (status 10))
  (via (at 189.992 122.428) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 12))
  (segment (start 189.992 120.6715) (end 189.992 122.428) (width 0.2) (layer F.Cu) (net 12) (status 10))
  (segment (start 191.892031 124.328031) (end 207.395969 124.328031) (width 0.2) (layer F.Cu) (net 12))
  (segment (start 189.992 122.428) (end 191.892031 124.328031) (width 0.2) (layer F.Cu) (net 12))
  (segment (start 209.33402 122.38998) (end 211.03598 122.38998) (width 0.2) (layer F.Cu) (net 12))
  (segment (start 207.395969 124.328031) (end 209.33402 122.38998) (width 0.2) (layer F.Cu) (net 12))
  (segment (start 211.03598 122.38998) (end 210.860693 122.38998) (width 0.2) (layer F.Cu) (net 12))
  (segment (start 231.08598 122.38998) (end 211.03598 122.38998) (width 0.2) (layer F.Cu) (net 12))
  (segment (start 179.705 100.255) (end 186.32801 106.87801) (width 0.2) (layer B.Cu) (net 12) (status 10))
  (segment (start 186.32801 118.76401) (end 189.992 122.428) (width 0.2) (layer B.Cu) (net 12))
  (segment (start 186.32801 106.87801) (end 186.32801 118.76401) (width 0.2) (layer B.Cu) (net 12))
  (segment (start 227.44101 131.95299) (end 224.266 135.128) (width 0.2) (layer F.Cu) (net 13) (status 20))
  (segment (start 227.44101 126.34901) (end 227.44101 131.95299) (width 0.2) (layer F.Cu) (net 13))
  (segment (start 226.441 125.349) (end 227.44101 126.34901) (width 0.2) (layer F.Cu) (net 13) (status 10))
  (via (at 187.706 122.428) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 13))
  (segment (start 187.706 120.6715) (end 187.706 122.428) (width 0.2) (layer F.Cu) (net 13) (status 10))
  (segment (start 223.88199 122.78999) (end 226.441 125.349) (width 0.2) (layer F.Cu) (net 13) (status 20))
  (segment (start 209.499708 122.78999) (end 223.88199 122.78999) (width 0.2) (layer F.Cu) (net 13))
  (segment (start 207.561658 124.728041) (end 209.499708 122.78999) (width 0.2) (layer F.Cu) (net 13))
  (segment (start 190.006041 124.728041) (end 207.561658 124.728041) (width 0.2) (layer F.Cu) (net 13))
  (segment (start 187.706 122.428) (end 190.006041 124.728041) (width 0.2) (layer F.Cu) (net 13))
  (segment (start 180.808086 102.795) (end 185.928 107.914914) (width 0.2) (layer B.Cu) (net 13))
  (segment (start 179.705 102.795) (end 180.808086 102.795) (width 0.2) (layer B.Cu) (net 13) (status 10))
  (segment (start 185.928 120.65) (end 187.706 122.428) (width 0.2) (layer B.Cu) (net 13))
  (segment (start 185.928 107.914914) (end 185.928 120.65) (width 0.2) (layer B.Cu) (net 13))
  (segment (start 206.577 112.955) (end 205.105 112.955) (width 0.2) (layer F.Cu) (net 14) (status 20))
  (segment (start 210.71201 95.669689) (end 208.28 98.101699) (width 0.2) (layer F.Cu) (net 14))
  (segment (start 208.28 111.252) (end 206.577 112.955) (width 0.2) (layer F.Cu) (net 14))
  (segment (start 212.774624 91.401992) (end 210.71201 93.464605) (width 0.2) (layer F.Cu) (net 14))
  (segment (start 208.28 98.101699) (end 208.28 111.252) (width 0.2) (layer F.Cu) (net 14))
  (segment (start 214.067992 91.401992) (end 212.774624 91.401992) (width 0.2) (layer F.Cu) (net 14))
  (segment (start 210.71201 93.464605) (end 210.71201 95.669689) (width 0.2) (layer F.Cu) (net 14))
  (segment (start 216.916 94.25) (end 214.067992 91.401992) (width 0.2) (layer F.Cu) (net 14) (status 10))
  (via (at 216.916 98.044) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 15))
  (segment (start 216.916 99.33) (end 216.916 98.044) (width 0.2) (layer F.Cu) (net 15) (status 10))
  (via (at 262.636 98.044) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 15))
  (segment (start 262.636 99.314) (end 262.636 98.044) (width 0.2) (layer F.Cu) (net 15) (status 10))
  (via (at 255.27 98.044) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 15))
  (segment (start 255.27 99.33) (end 255.27 98.044) (width 0.2) (layer F.Cu) (net 15) (status 10))
  (segment (start 255.27 98.044) (end 262.636 98.044) (width 0.2) (layer B.Cu) (net 15))
  (via (at 247.396 98.044) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 15))
  (segment (start 247.396 99.33) (end 247.396 98.044) (width 0.2) (layer F.Cu) (net 15) (status 10))
  (segment (start 247.396 98.044) (end 255.27 98.044) (width 0.2) (layer B.Cu) (net 15))
  (via (at 239.776 98.044) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 15))
  (segment (start 239.776 99.346) (end 239.776 98.044) (width 0.2) (layer F.Cu) (net 15) (status 10))
  (segment (start 239.776 98.044) (end 247.396 98.044) (width 0.2) (layer B.Cu) (net 15))
  (via (at 231.902 98.044) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 15))
  (segment (start 231.902 99.346) (end 231.902 98.044) (width 0.2) (layer F.Cu) (net 15) (status 10))
  (segment (start 231.902 98.044) (end 239.776 98.044) (width 0.2) (layer B.Cu) (net 15))
  (via (at 224.282 98.044) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 15))
  (segment (start 224.282 99.33) (end 224.282 98.044) (width 0.2) (layer F.Cu) (net 15) (status 10))
  (segment (start 224.282 98.044) (end 231.902 98.044) (width 0.2) (layer B.Cu) (net 15))
  (segment (start 216.916 98.044) (end 224.282 98.044) (width 0.2) (layer B.Cu) (net 15))
  (segment (start 259.842 71.374) (end 258.064 71.374) (width 1.2) (layer F.Cu) (net 15) (status 10))
  (segment (start 258.064 71.374) (end 256.54 72.898) (width 1.2) (layer F.Cu) (net 15))
  (segment (start 256.54 77.724) (end 252.73 81.534) (width 1.2) (layer F.Cu) (net 15) (status 20))
  (segment (start 256.54 72.898) (end 256.54 77.724) (width 1.2) (layer F.Cu) (net 15))
  (segment (start 239.202 87.072) (end 239.252 87.122) (width 1.2) (layer F.Cu) (net 15) (status 30))
  (segment (start 239.202 84.812) (end 239.202 87.072) (width 1.2) (layer F.Cu) (net 15) (status 30))
  (segment (start 252.73 82.55) (end 252.73 81.534) (width 1.2) (layer F.Cu) (net 15) (status 30))
  (segment (start 248.158 87.122) (end 252.73 82.55) (width 1.2) (layer F.Cu) (net 15) (status 20))
  (segment (start 193.547 78.364) (end 193.547 79.674) (width 0.2) (layer F.Cu) (net 15) (status 10))
  (segment (start 192.42 79.491) (end 193.547 78.364) (width 1) (layer F.Cu) (net 15) (status 20))
  (segment (start 192.42 81.534) (end 192.42 79.491) (width 1) (layer F.Cu) (net 15) (status 10))
  (segment (start 192.42 82.076) (end 192.42 81.534) (width 0.2) (layer F.Cu) (net 15) (status 30))
  (segment (start 189.676 84.82) (end 192.42 82.076) (width 0.2) (layer F.Cu) (net 15) (status 20))
  (segment (start 188.976 84.82) (end 189.676 84.82) (width 0.2) (layer F.Cu) (net 15) (status 10))
  (segment (start 194.441 77.47) (end 193.547 78.364) (width 1) (layer F.Cu) (net 15) (status 20))
  (segment (start 200.914 72.39) (end 200.533 72.771) (width 1) (layer B.Cu) (net 15))
  (segment (start 261.366 51.054) (end 261.366 69.85) (width 1.2) (layer B.Cu) (net 15))
  (segment (start 259.447001 49.135001) (end 261.366 51.054) (width 1.2) (layer B.Cu) (net 15))
  (segment (start 224.168999 49.135001) (end 259.447001 49.135001) (width 1.2) (layer B.Cu) (net 15))
  (segment (start 261.366 69.85) (end 259.842 71.374) (width 1.2) (layer B.Cu) (net 15) (status 20))
  (via (at 241.3 87.122) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 15))
  (segment (start 241.3 87.122) (end 248.158 87.122) (width 1.2) (layer F.Cu) (net 15))
  (segment (start 239.252 87.122) (end 241.3 87.122) (width 1.2) (layer F.Cu) (net 15) (status 10))
  (segment (start 265.213834 71.374) (end 259.842 71.374) (width 0.2) (layer F.Cu) (net 15) (status 20))
  (segment (start 267.33802 73.498186) (end 265.213834 71.374) (width 0.2) (layer F.Cu) (net 15))
  (segment (start 267.33802 93.34198) (end 267.33802 73.498186) (width 0.2) (layer F.Cu) (net 15))
  (segment (start 262.636 98.044) (end 267.33802 93.34198) (width 0.2) (layer F.Cu) (net 15))
  (segment (start 238.25199 88.12201) (end 239.252 87.122) (width 0.2) (layer F.Cu) (net 15) (status 20))
  (segment (start 236.674176 88.12201) (end 238.25199 88.12201) (width 0.2) (layer F.Cu) (net 15))
  (segment (start 236.35199 87.799824) (end 236.674176 88.12201) (width 0.2) (layer F.Cu) (net 15))
  (segment (start 236.35199 86.41599) (end 236.35199 87.799824) (width 0.2) (layer F.Cu) (net 15))
  (segment (start 235.534 85.598) (end 236.35199 86.41599) (width 0.2) (layer F.Cu) (net 15))
  (segment (start 234.934 85.598) (end 235.534 85.598) (width 0.2) (layer F.Cu) (net 15) (status 10))
  (segment (start 234.934 83.338) (end 234.884 83.288) (width 0.2) (layer F.Cu) (net 15) (status 30))
  (segment (start 234.934 85.598) (end 234.934 83.338) (width 0.2) (layer F.Cu) (net 15) (status 30))
  (segment (start 174.965 86.36) (end 177.292 84.033) (width 1.2) (layer F.Cu) (net 15))
  (segment (start 173.99 86.36) (end 174.965 86.36) (width 1.2) (layer F.Cu) (net 15) (status 10))
  (segment (start 177.292 73.830806) (end 179.07 72.052806) (width 1.2) (layer F.Cu) (net 15))
  (segment (start 177.292 84.033) (end 177.292 73.830806) (width 1.2) (layer F.Cu) (net 15))
  (via (at 208.28 65.024) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 15))
  (segment (start 190.331998 65.024) (end 208.28 65.024) (width 1.2) (layer F.Cu) (net 15))
  (segment (start 183.303192 72.052806) (end 190.331998 65.024) (width 1.2) (layer F.Cu) (net 15))
  (segment (start 179.07 72.052806) (end 183.303192 72.052806) (width 1.2) (layer F.Cu) (net 15))
  (segment (start 208.28 65.024) (end 224.168999 49.135001) (width 1.2) (layer B.Cu) (net 15))
  (segment (start 200.533 72.771) (end 208.28 65.024) (width 1.2) (layer B.Cu) (net 15))
  (segment (start 235.484 83.288) (end 234.884 83.288) (width 0.2) (layer F.Cu) (net 15) (status 20))
  (segment (start 237.174001 81.597999) (end 235.484 83.288) (width 0.2) (layer F.Cu) (net 15))
  (segment (start 235.611 77.581) (end 237.174001 79.144001) (width 0.2) (layer F.Cu) (net 15))
  (segment (start 237.174001 79.144001) (end 237.174001 81.597999) (width 0.2) (layer F.Cu) (net 15))
  (segment (start 235.011 77.581) (end 235.611 77.581) (width 0.2) (layer F.Cu) (net 15) (status 10))
  (segment (start 194.441 77.47) (end 194.5132 77.47) (width 1) (layer F.Cu) (net 15))
  (via (at 200.533 72.771) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 15))
  (segment (start 199.2122 72.771) (end 200.533 72.771) (width 1) (layer F.Cu) (net 15))
  (segment (start 194.5132 77.47) (end 199.2122 72.771) (width 1) (layer F.Cu) (net 15))
  (segment (start 260.588 79.74) (end 259.842 78.994) (width 0.2) (layer F.Cu) (net 16) (status 20))
  (segment (start 265.938 79.74) (end 260.588 79.74) (width 0.2) (layer F.Cu) (net 16) (status 10))
  (segment (start 212.868 111.268) (end 214.63 113.03) (width 0.2) (layer F.Cu) (net 17) (status 20))
  (segment (start 212.868 105.852) (end 212.868 111.268) (width 0.2) (layer F.Cu) (net 17) (status 10))
  (segment (start 220.234 111.014) (end 222.25 113.03) (width 0.2) (layer F.Cu) (net 17) (status 20))
  (segment (start 220.234 105.852) (end 220.234 111.014) (width 0.2) (layer F.Cu) (net 17) (status 10))
  (segment (start 227.854 111.014) (end 229.87 113.03) (width 0.2) (layer F.Cu) (net 17) (status 20))
  (segment (start 227.854 105.852) (end 227.854 111.014) (width 0.2) (layer F.Cu) (net 17) (status 10))
  (segment (start 235.728 111.268) (end 237.49 113.03) (width 0.2) (layer F.Cu) (net 17) (status 20))
  (segment (start 235.728 105.852) (end 235.728 111.268) (width 0.2) (layer F.Cu) (net 17) (status 10))
  (segment (start 243.348 111.268) (end 245.11 113.03) (width 0.2) (layer F.Cu) (net 17) (status 20))
  (segment (start 243.348 105.852) (end 243.348 111.268) (width 0.2) (layer F.Cu) (net 17) (status 10))
  (segment (start 214.63 113.03) (end 260.35 113.03) (width 1) (layer F.Cu) (net 17) (status 30))
  (segment (start 258.588 111.268) (end 260.35 113.03) (width 0.2) (layer F.Cu) (net 17) (status 20))
  (segment (start 258.588 105.852) (end 258.588 111.268) (width 0.2) (layer F.Cu) (net 17) (status 10))
  (segment (start 251.222 111.522) (end 252.73 113.03) (width 0.2) (layer F.Cu) (net 17) (status 20))
  (segment (start 251.222 105.852) (end 251.222 111.522) (width 0.2) (layer F.Cu) (net 17) (status 10))
  (segment (start 246.38 75.158) (end 246.66 75.438) (width 0.2) (layer F.Cu) (net 17) (status 30))
  (segment (start 246.38 73.136) (end 246.38 75.158) (width 0.2) (layer F.Cu) (net 17) (status 30))
  (segment (start 247.88001 74.21799) (end 246.66 75.438) (width 1.2) (layer F.Cu) (net 17) (status 20))
  (segment (start 247.88001 69.06401) (end 247.88001 74.21799) (width 1.2) (layer F.Cu) (net 17))
  (segment (start 246.38 67.564) (end 247.88001 69.06401) (width 1.2) (layer F.Cu) (net 17) (status 10))
  (segment (start 246.51 75.588) (end 246.66 75.438) (width 1.2) (layer F.Cu) (net 17) (status 30))
  (segment (start 246.51 78.486) (end 246.51 75.588) (width 1.2) (layer F.Cu) (net 17) (status 30))
  (segment (start 262.128 113.03) (end 268.41499 106.74301) (width 1.2) (layer F.Cu) (net 17))
  (segment (start 260.35 113.03) (end 262.128 113.03) (width 1.2) (layer F.Cu) (net 17) (status 10))
  (segment (start 268.41499 106.74301) (end 268.41499 66.73899) (width 1.2) (layer F.Cu) (net 17))
  (segment (start 268.41499 66.73899) (end 266.954 65.278) (width 1.2) (layer F.Cu) (net 17))
  (segment (start 248.666 65.278) (end 246.38 67.564) (width 1.2) (layer F.Cu) (net 17) (status 20))
  (segment (start 266.954 65.278) (end 248.666 65.278) (width 1.2) (layer F.Cu) (net 17))
  (segment (start 245.11 61.722) (end 248.666 65.278) (width 1.2) (layer F.Cu) (net 17) (status 10))
  (segment (start 245.07 61.722) (end 245.11 61.722) (width 1.2) (layer F.Cu) (net 17) (status 30))
  (segment (start 238.68 75.184) (end 238.68 74.234) (width 0.5) (layer F.Cu) (net 18) (status 30))
  (segment (start 238.506 81.558) (end 238.252 81.812) (width 1.2) (layer F.Cu) (net 18) (status 30))
  (segment (start 238.506 78.74) (end 238.506 81.558) (width 1.2) (layer F.Cu) (net 18) (status 30))
  (segment (start 237.379999 77.613999) (end 238.506 78.74) (width 1.2) (layer F.Cu) (net 18) (status 20))
  (segment (start 238.364998 74.234) (end 237.379999 75.218999) (width 1.2) (layer F.Cu) (net 18) (status 10))
  (segment (start 238.68 74.234) (end 238.364998 74.234) (width 1.2) (layer F.Cu) (net 18) (status 30))
  (segment (start 238.48 74.034) (end 238.68 74.234) (width 1.2) (layer F.Cu) (net 18) (status 30))
  (segment (start 238.48 67.844) (end 238.76 67.564) (width 1.2) (layer F.Cu) (net 18) (status 30))
  (via (at 210.82 104.14) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 18))
  (segment (start 210.82 105.934) (end 210.82 104.14) (width 0.2) (layer F.Cu) (net 18) (status 10))
  (segment (start 210.82 89.662) (end 213.36 87.122) (width 0.2) (layer B.Cu) (net 18))
  (segment (start 210.82 104.14) (end 210.82 89.662) (width 0.2) (layer B.Cu) (net 18))
  (segment (start 238.252 81.812) (end 238.228 81.812) (width 0.2) (layer F.Cu) (net 18) (status 30))
  (segment (start 213.36 87.122) (end 226.06 87.122) (width 0.2) (layer B.Cu) (net 18))
  (via (at 237.379999 76.343999) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 18))
  (segment (start 236.838001 76.343999) (end 237.379999 76.343999) (width 0.2) (layer B.Cu) (net 18))
  (segment (start 226.06 87.122) (end 236.838001 76.343999) (width 0.2) (layer B.Cu) (net 18))
  (segment (start 237.379999 76.343999) (end 237.379999 77.613999) (width 1.2) (layer F.Cu) (net 18))
  (segment (start 237.379999 75.218999) (end 237.379999 76.343999) (width 1.2) (layer F.Cu) (net 18))
  (segment (start 238.68 72.207) (end 239.005 71.882) (width 1.2) (layer F.Cu) (net 18) (status 30))
  (segment (start 238.68 74.234) (end 238.68 72.207) (width 1.2) (layer F.Cu) (net 18) (status 30))
  (segment (start 239.005 67.809) (end 238.76 67.564) (width 1.2) (layer F.Cu) (net 18) (status 30))
  (segment (start 239.005 71.882) (end 239.005 67.809) (width 1.2) (layer F.Cu) (net 18) (status 30))
  (segment (start 173.99 91.36) (end 177.292 88.058) (width 1.2) (layer B.Cu) (net 19) (status 10))
  (segment (start 177.292 88.058) (end 177.292 73.406) (width 1.2) (layer B.Cu) (net 19))
  (segment (start 177.292 73.406) (end 178.816 71.882) (width 1.2) (layer B.Cu) (net 19))
  (segment (start 178.816 71.882) (end 180.594 71.882) (width 1.2) (layer B.Cu) (net 19))
  (via (at 184.404 99.568) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 19))
  (segment (start 184.404 75.692) (end 184.404 99.568) (width 1.2) (layer B.Cu) (net 19))
  (segment (start 180.594 71.882) (end 184.404 75.692) (width 1.2) (layer B.Cu) (net 19))
  (segment (start 184.404 97.394) (end 184.516 97.282) (width 1.2) (layer F.Cu) (net 19) (status 30))
  (segment (start 184.404 99.568) (end 184.404 97.394) (width 1.2) (layer F.Cu) (net 19) (status 20))
  (segment (start 259.731 136.078) (end 214.646 136.078) (width 0.2) (layer F.Cu) (net 20) (status 30))
  (segment (start 188.977 77.734) (end 188.977 78.364) (width 1) (layer F.Cu) (net 20) (status 30))
  (segment (start 179.705 74.855) (end 179.92301 74.63699) (width 1) (layer F.Cu) (net 20) (status 30))
  (segment (start 188.977 78.364) (end 188.977 79.391) (width 1) (layer F.Cu) (net 20) (status 30))
  (segment (start 188.776001 90.959999) (end 188.026 91.71) (width 0.2) (layer F.Cu) (net 20) (status 20))
  (segment (start 191.527999 90.959999) (end 188.776001 90.959999) (width 0.2) (layer F.Cu) (net 20))
  (segment (start 192.278 91.71) (end 191.527999 90.959999) (width 0.2) (layer F.Cu) (net 20) (status 10))
  (via (at 192.278 88.9) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 20))
  (segment (start 192.278 91.71) (end 192.278 88.9) (width 0.2) (layer F.Cu) (net 20) (status 10))
  (via (at 189.794 80.208) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 20))
  (segment (start 192.278 82.692) (end 189.794 80.208) (width 0.2) (layer B.Cu) (net 20))
  (segment (start 192.278 88.9) (end 192.278 82.692) (width 0.2) (layer B.Cu) (net 20))
  (segment (start 189.794 80.208) (end 191.12 81.534) (width 1) (layer F.Cu) (net 20) (status 20))
  (segment (start 188.977 79.391) (end 189.794 80.208) (width 1) (layer F.Cu) (net 20) (status 10))
  (via (at 192.024 99.822) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 20))
  (segment (start 191.836 100.01) (end 192.024 99.822) (width 0.2) (layer F.Cu) (net 20))
  (segment (start 191.836 101.87) (end 191.836 100.01) (width 0.2) (layer F.Cu) (net 20) (status 10))
  (segment (start 192.024 89.154) (end 192.278 88.9) (width 0.2) (layer B.Cu) (net 20))
  (segment (start 192.024 99.822) (end 192.024 89.154) (width 0.2) (layer B.Cu) (net 20))
  (via (at 197.612 135.636) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 20))
  (segment (start 198.054 136.078) (end 197.612 135.636) (width 0.2) (layer F.Cu) (net 20))
  (segment (start 214.646 136.078) (end 198.054 136.078) (width 0.2) (layer F.Cu) (net 20) (status 10))
  (segment (start 197.612 135.636) (end 197.612 129.024594) (width 0.2) (layer B.Cu) (net 20))
  (segment (start 197.612 129.024594) (end 202.50797 124.128624) (width 0.2) (layer B.Cu) (net 20))
  (segment (start 202.50797 124.128624) (end 202.50797 104.435065) (width 0.2) (layer B.Cu) (net 20))
  (segment (start 197.894905 99.822) (end 192.024 99.822) (width 0.2) (layer B.Cu) (net 20))
  (segment (start 202.50797 104.435065) (end 197.894905 99.822) (width 0.2) (layer B.Cu) (net 20))
  (segment (start 179.705 74.855) (end 185.8895 74.855) (width 1.2) (layer F.Cu) (net 20) (status 30))
  (segment (start 188.977 77.48) (end 186.182 74.685) (width 1.2) (layer F.Cu) (net 20) (status 30))
  (segment (start 188.977 78.364) (end 188.977 77.48) (width 1.2) (layer F.Cu) (net 20) (status 30))
  (segment (start 217.2208 85.1916) (end 215.7984 83.7692) (width 1) (layer B.Cu) (net 20))
  (segment (start 215.7984 83.7692) (end 210.6676 83.7692) (width 1) (layer B.Cu) (net 20))
  (segment (start 210.6676 83.7692) (end 210.2104 83.7692) (width 1) (layer B.Cu) (net 20))
  (segment (start 210.2104 83.7692) (end 209.0928 82.6516) (width 1) (layer B.Cu) (net 20))
  (segment (start 209.0928 82.6516) (end 209.0928 74.5236) (width 1) (layer B.Cu) (net 20))
  (segment (start 209.0928 74.5236) (end 206.7052 72.136) (width 1) (layer B.Cu) (net 20))
  (segment (start 203.00649 72.136) (end 198.4756 76.66689) (width 1) (layer B.Cu) (net 20))
  (segment (start 206.7052 72.136) (end 203.00649 72.136) (width 1) (layer B.Cu) (net 20))
  (via (at 198.4756 76.66689) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 20))
  (segment (start 189.794 80.208) (end 198.3688 80.208) (width 1) (layer B.Cu) (net 20))
  (via (at 198.3688 80.208) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 20))
  (segment (start 198.4756 80.1012) (end 198.3688 80.208) (width 1) (layer F.Cu) (net 20))
  (segment (start 198.4756 76.66689) (end 198.4756 80.1012) (width 1) (layer F.Cu) (net 20))
  (via (at 201.93 127) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 21))
  (segment (start 203.47 127) (end 201.93 127) (width 0.2) (layer F.Cu) (net 21) (status 10))
  (segment (start 209.419999 106.100001) (end 209.419999 98.428001) (width 0.2) (layer B.Cu) (net 21))
  (segment (start 205.105 110.415) (end 209.419999 106.100001) (width 0.2) (layer B.Cu) (net 21) (status 10))
  (via (at 212.32002 85.598) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 21))
  (segment (start 209.419999 88.498021) (end 212.32002 85.598) (width 0.2) (layer B.Cu) (net 21))
  (segment (start 209.419999 98.428001) (end 209.419999 88.498021) (width 0.2) (layer B.Cu) (net 21))
  (segment (start 212.32002 85.598) (end 212.32002 50.56998) (width 0.2) (layer F.Cu) (net 21))
  (segment (start 216.408 46.482) (end 216.408 41.783) (width 0.2) (layer F.Cu) (net 21) (status 20))
  (segment (start 212.32002 50.56998) (end 216.408 46.482) (width 0.2) (layer F.Cu) (net 21))
  (segment (start 198.12 136.652) (end 201.93 132.842) (width 0.2) (layer B.Cu) (net 21))
  (segment (start 201.93 132.842) (end 201.93 127) (width 0.2) (layer B.Cu) (net 21))
  (segment (start 183.388 136.652) (end 198.12 136.652) (width 0.2) (layer B.Cu) (net 21))
  (segment (start 176.784 130.048) (end 183.388 136.652) (width 0.2) (layer B.Cu) (net 21))
  (segment (start 176.784 119.34) (end 176.784 130.048) (width 0.2) (layer B.Cu) (net 21))
  (segment (start 173.736 116.292) (end 176.784 119.34) (width 0.2) (layer B.Cu) (net 21) (status 10))
  (segment (start 205.105 110.415) (end 203.708 111.812) (width 0.2) (layer B.Cu) (net 21) (status 10))
  (segment (start 203.708 125.222) (end 201.93 127) (width 0.2) (layer B.Cu) (net 21))
  (segment (start 203.708 111.812) (end 203.708 125.222) (width 0.2) (layer B.Cu) (net 21))
  (segment (start 214.868 102.576) (end 214.868 104.902) (width 1) (layer F.Cu) (net 22) (status 20))
  (segment (start 213.868 101.576) (end 214.868 102.576) (width 1) (layer F.Cu) (net 22) (status 10))
  (segment (start 214.868 110.292) (end 214.63 110.53) (width 1) (layer F.Cu) (net 22) (status 30))
  (segment (start 214.868 104.902) (end 214.868 110.292) (width 1) (layer F.Cu) (net 22) (status 30))
  (segment (start 216.3555 106.3895) (end 214.868 104.902) (width 0.2) (layer F.Cu) (net 22) (status 30))
  (segment (start 216.916 106.3895) (end 216.3555 106.3895) (width 0.2) (layer F.Cu) (net 22) (status 30))
  (segment (start 188.452 94.234) (end 188.976 93.71) (width 0.2) (layer F.Cu) (net 23) (status 20))
  (segment (start 185.816 94.234) (end 188.452 94.234) (width 0.2) (layer F.Cu) (net 23) (status 10))
  (via (at 202.438 98.044) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 23))
  (segment (start 202.438 102.668) (end 202.438 98.044) (width 0.2) (layer B.Cu) (net 23))
  (segment (start 205.105 105.335) (end 202.438 102.668) (width 0.2) (layer B.Cu) (net 23) (status 10))
  (segment (start 198.644 98.044) (end 198.374 97.774) (width 0.2) (layer F.Cu) (net 23) (status 30))
  (segment (start 202.438 98.044) (end 198.644 98.044) (width 0.2) (layer F.Cu) (net 23) (status 20))
  (via (at 188.976 95.504) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 23))
  (segment (start 188.976 93.71) (end 188.976 95.504) (width 0.2) (layer F.Cu) (net 23) (status 10))
  (via (at 188.976 98.552) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 23))
  (segment (start 197.596 98.552) (end 188.976 98.552) (width 0.2) (layer F.Cu) (net 23))
  (segment (start 198.374 97.774) (end 197.596 98.552) (width 0.2) (layer F.Cu) (net 23) (status 10))
  (segment (start 188.976 98.552) (end 188.976 95.504) (width 0.2) (layer B.Cu) (net 23))
  (segment (start 260.35 124.54) (end 214.63 124.54) (width 0.2) (layer B.Cu) (net 24) (status 30))
  (segment (start 260.169 124.359) (end 260.35 124.54) (width 0.2) (layer F.Cu) (net 24) (status 30))
  (segment (start 260.169 120.142) (end 260.169 124.359) (width 0.2) (layer F.Cu) (net 24) (status 20))
  (segment (start 173.736 121.666) (end 186.055 133.985) (width 0.2) (layer F.Cu) (net 24) (status 20))
  (segment (start 173.736 118.792) (end 173.736 121.666) (width 0.2) (layer F.Cu) (net 24) (status 10))
  (segment (start 172.46099 117.51699) (end 173.736 118.792) (width 0.2) (layer F.Cu) (net 24) (status 20))
  (segment (start 172.46099 102.15401) (end 172.46099 117.51699) (width 0.2) (layer F.Cu) (net 24))
  (segment (start 173.015 101.6) (end 172.46099 102.15401) (width 0.2) (layer F.Cu) (net 24) (status 10))
  (segment (start 173.99 101.6) (end 173.015 101.6) (width 0.2) (layer F.Cu) (net 24) (status 30))
  (segment (start 186.055 133.985) (end 186.055 127.941061) (width 0.2) (layer F.Cu) (net 24) (status 10))
  (segment (start 186.055 127.941061) (end 188.468 125.528061) (width 0.2) (layer F.Cu) (net 24))
  (segment (start 207.893036 125.528061) (end 208.127357 125.293738) (width 0.2) (layer F.Cu) (net 24))
  (segment (start 208.127357 125.293738) (end 209.723095 123.698) (width 0.2) (layer F.Cu) (net 24))
  (segment (start 213.788 123.698) (end 214.63 124.54) (width 0.2) (layer F.Cu) (net 24) (status 20))
  (segment (start 209.723095 123.698) (end 213.788 123.698) (width 0.2) (layer F.Cu) (net 24))
  (segment (start 206.808061 126.782061) (end 206.808061 125.528061) (width 0.2) (layer F.Cu) (net 24))
  (segment (start 208.788 128.762) (end 206.808061 126.782061) (width 0.2) (layer F.Cu) (net 24) (status 10))
  (segment (start 206.808061 125.528061) (end 207.893036 125.528061) (width 0.2) (layer F.Cu) (net 24))
  (segment (start 188.468 125.528061) (end 206.808061 125.528061) (width 0.2) (layer F.Cu) (net 24))
  (segment (start 206.590122 127) (end 206.808061 126.782061) (width 0.2) (layer F.Cu) (net 24))
  (segment (start 205.47 127) (end 206.590122 127) (width 0.2) (layer F.Cu) (net 24) (status 10))
  (segment (start 217.678 41.783) (end 225.171 41.783) (width 0.2) (layer F.Cu) (net 24) (status 10))
  (segment (start 233.934 50.546) (end 233.807 50.419) (width 0.2) (layer F.Cu) (net 24))
  (segment (start 225.171 41.783) (end 233.807 50.419) (width 0.2) (layer F.Cu) (net 24))
  (via (at 236.474 80.01) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 24))
  (segment (start 234.212 80.01) (end 233.934 80.288) (width 0.2) (layer F.Cu) (net 24) (status 30))
  (segment (start 236.474 80.01) (end 234.212 80.01) (width 0.2) (layer F.Cu) (net 24) (status 20))
  (segment (start 213.455 124.54) (end 214.63 124.54) (width 0.2) (layer B.Cu) (net 24) (status 20))
  (segment (start 212.30599 123.39099) (end 213.455 124.54) (width 0.2) (layer B.Cu) (net 24))
  (segment (start 212.30599 91.40199) (end 212.30599 123.39099) (width 0.2) (layer B.Cu) (net 24))
  (segment (start 223.031688 90.71601) (end 212.99197 90.71601) (width 0.2) (layer B.Cu) (net 24))
  (segment (start 233.737698 80.01) (end 223.031688 90.71601) (width 0.2) (layer B.Cu) (net 24))
  (segment (start 212.99197 90.71601) (end 212.30599 91.40199) (width 0.2) (layer B.Cu) (net 24))
  (segment (start 236.474 80.01) (end 233.737698 80.01) (width 0.2) (layer B.Cu) (net 24))
  (segment (start 234.061 75.581) (end 234.061 75.565) (width 0.2) (layer F.Cu) (net 24) (status 30))
  (segment (start 233.934 80.288) (end 233.934 75.438) (width 0.2) (layer F.Cu) (net 24) (status 30))
  (segment (start 234.061 75.565) (end 233.934 75.438) (width 0.2) (layer F.Cu) (net 24) (status 30))
  (segment (start 233.934 75.438) (end 233.934 50.546) (width 0.2) (layer F.Cu) (net 24) (status 10))
  (segment (start 219.69401 126.34901) (end 218.694 125.349) (width 0.2) (layer F.Cu) (net 25) (status 20))
  (segment (start 219.69401 132.07999) (end 219.69401 126.34901) (width 0.2) (layer F.Cu) (net 25))
  (segment (start 216.646 135.128) (end 219.69401 132.07999) (width 0.2) (layer F.Cu) (net 25) (status 10))
  (segment (start 218.694 125.349) (end 218.35299 125.69001) (width 0.2) (layer F.Cu) (net 25) (status 30))
  (segment (start 218.694 125.349) (end 216.535 123.19) (width 0.2) (layer F.Cu) (net 25) (status 10))
  (via (at 185.42 122.428) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 25))
  (segment (start 185.42 120.6715) (end 185.42 122.428) (width 0.2) (layer F.Cu) (net 25) (status 10))
  (segment (start 207.727347 125.128051) (end 209.665396 123.19) (width 0.2) (layer F.Cu) (net 25))
  (segment (start 188.120051 125.128051) (end 207.727347 125.128051) (width 0.2) (layer F.Cu) (net 25))
  (segment (start 185.42 122.428) (end 188.120051 125.128051) (width 0.2) (layer F.Cu) (net 25))
  (segment (start 211.328 123.19) (end 211.192069 123.19) (width 0.2) (layer F.Cu) (net 25))
  (segment (start 209.665396 123.19) (end 211.328 123.19) (width 0.2) (layer F.Cu) (net 25))
  (segment (start 216.535 123.19) (end 211.328 123.19) (width 0.2) (layer F.Cu) (net 25))
  (segment (start 179.705 105.335) (end 182.551 105.335) (width 0.2) (layer B.Cu) (net 25) (status 10))
  (segment (start 185.42 108.204) (end 185.42 122.428) (width 0.2) (layer B.Cu) (net 25))
  (segment (start 182.551 105.335) (end 185.42 108.204) (width 0.2) (layer B.Cu) (net 25))
  (segment (start 265.938 75.676) (end 265.938 77.74) (width 0.2) (layer F.Cu) (net 26) (status 30))
  (segment (start 266.93801 78.74001) (end 266.93801 80.317824) (width 0.2) (layer F.Cu) (net 26))
  (segment (start 266.93801 80.317824) (end 258.653912 88.601922) (width 0.2) (layer F.Cu) (net 26))
  (segment (start 265.938 77.74) (end 266.93801 78.74001) (width 0.2) (layer F.Cu) (net 26) (status 10))
  (segment (start 212.553922 88.601922) (end 211.62002 87.66802) (width 0.2) (layer F.Cu) (net 26))
  (segment (start 211.62002 87.66802) (end 211.62002 78.77802) (width 0.2) (layer F.Cu) (net 26))
  (segment (start 211.62002 78.77802) (end 205.994 73.152) (width 0.2) (layer F.Cu) (net 26))
  (segment (start 258.653912 88.601922) (end 212.553922 88.601922) (width 0.2) (layer F.Cu) (net 26))
  (segment (start 179.7585 87.6085) (end 179.705 87.555) (width 0.2) (layer F.Cu) (net 26) (status 30))
  (segment (start 181.093 88.943) (end 179.705 87.555) (width 0.2) (layer F.Cu) (net 26) (status 20))
  (segment (start 183.134 88.943) (end 181.093 88.943) (width 0.2) (layer F.Cu) (net 26) (status 10))
  (segment (start 183.134 88.943) (end 183.890834 88.943) (width 0.2) (layer F.Cu) (net 26) (status 10))
  (segment (start 203.3016 74.2188) (end 204.3176 73.2028) (width 0.2) (layer F.Cu) (net 26))
  (segment (start 191.7192 87.1728) (end 199.9996 87.1728) (width 0.2) (layer F.Cu) (net 26))
  (segment (start 189.949 88.943) (end 191.7192 87.1728) (width 0.2) (layer F.Cu) (net 26))
  (segment (start 203.3016 83.8708) (end 203.3016 74.2188) (width 0.2) (layer F.Cu) (net 26))
  (segment (start 183.134 88.943) (end 189.949 88.943) (width 0.2) (layer F.Cu) (net 26))
  (segment (start 199.9996 87.1728) (end 203.3016 83.8708) (width 0.2) (layer F.Cu) (net 26))
  (segment (start 205.994 73.152) (end 204.3176 73.2028) (width 0.2) (layer F.Cu) (net 26))
  (segment (start 183.1715 82.82) (end 183.134 82.7825) (width 0.2) (layer F.Cu) (net 27) (status 30))
  (segment (start 186.182 82.82) (end 183.1715 82.82) (width 0.2) (layer F.Cu) (net 27) (status 30))
  (segment (start 188.436 82.82) (end 188.468 82.788) (width 0.2) (layer F.Cu) (net 27) (status 30))
  (segment (start 181.9375 82.7825) (end 179.705 85.015) (width 0.2) (layer F.Cu) (net 27) (status 20))
  (segment (start 183.134 82.7825) (end 181.9375 82.7825) (width 0.2) (layer F.Cu) (net 27) (status 10))
  (segment (start 186.182 82.82) (end 188.976 82.82) (width 0.2) (layer F.Cu) (net 27) (status 30))
  (segment (start 218.385 127.04) (end 218.694 127.349) (width 0.2) (layer F.Cu) (net 28) (status 30))
  (segment (start 214.63 127.04) (end 218.385 127.04) (width 0.2) (layer F.Cu) (net 28) (status 30))
  (segment (start 212.608935 91.001982) (end 210.312 93.298917) (width 0.2) (layer F.Cu) (net 29))
  (segment (start 221.017982 91.001982) (end 212.608935 91.001982) (width 0.2) (layer F.Cu) (net 29))
  (segment (start 224.282 94.266) (end 221.017982 91.001982) (width 0.2) (layer F.Cu) (net 29) (status 10))
  (segment (start 210.312 93.298917) (end 210.312 95.504) (width 0.2) (layer F.Cu) (net 29))
  (segment (start 208.101 97.715) (end 205.105 97.715) (width 0.2) (layer F.Cu) (net 29) (status 20))
  (segment (start 210.312 95.504) (end 208.101 97.715) (width 0.2) (layer F.Cu) (net 29))
  (segment (start 226.132 127.04) (end 226.441 127.349) (width 0.2) (layer F.Cu) (net 30) (status 30))
  (segment (start 222.25 127.04) (end 226.132 127.04) (width 0.2) (layer F.Cu) (net 30) (status 30))
  (segment (start 207.870219 95.175) (end 205.105 95.175) (width 0.2) (layer F.Cu) (net 31) (status 20))
  (segment (start 212.443246 90.601972) (end 207.870219 95.175) (width 0.2) (layer F.Cu) (net 31))
  (segment (start 228.237972 90.601972) (end 212.443246 90.601972) (width 0.2) (layer F.Cu) (net 31))
  (segment (start 231.902 94.266) (end 228.237972 90.601972) (width 0.2) (layer F.Cu) (net 31) (status 10))
  (segment (start 233.736 127.04) (end 234.061 127.365) (width 0.2) (layer F.Cu) (net 32) (status 30))
  (segment (start 229.87 127.04) (end 233.736 127.04) (width 0.2) (layer F.Cu) (net 32) (status 30))
  (segment (start 212.277557 90.201962) (end 211.582 90.897521) (width 0.2) (layer F.Cu) (net 33))
  (segment (start 235.711962 90.201962) (end 212.277557 90.201962) (width 0.2) (layer F.Cu) (net 33))
  (segment (start 239.776 94.266) (end 235.711962 90.201962) (width 0.2) (layer F.Cu) (net 33) (status 10))
  (segment (start 209.844521 92.635) (end 205.105 92.635) (width 0.2) (layer F.Cu) (net 33) (status 20))
  (segment (start 211.582 90.897521) (end 209.844521 92.635) (width 0.2) (layer F.Cu) (net 33))
  (segment (start 241.229 127.04) (end 241.554 127.365) (width 0.2) (layer F.Cu) (net 34) (status 30))
  (segment (start 237.49 127.04) (end 241.229 127.04) (width 0.2) (layer F.Cu) (net 34) (status 30))
  (segment (start 242.947952 89.801952) (end 211.975952 89.801952) (width 0.2) (layer F.Cu) (net 35))
  (segment (start 247.396 94.25) (end 242.947952 89.801952) (width 0.2) (layer F.Cu) (net 35) (status 10))
  (segment (start 209.729 87.555) (end 205.105 87.555) (width 0.2) (layer F.Cu) (net 35) (status 20))
  (segment (start 211.975952 89.801952) (end 209.729 87.555) (width 0.2) (layer F.Cu) (net 35))
  (segment (start 248.849 127.04) (end 249.174 127.365) (width 0.2) (layer F.Cu) (net 36) (status 30))
  (segment (start 245.11 127.04) (end 248.849 127.04) (width 0.2) (layer F.Cu) (net 36) (status 30))
  (segment (start 255.27 94.25) (end 250.421942 89.401942) (width 0.2) (layer F.Cu) (net 37) (status 10))
  (segment (start 250.421942 89.401942) (end 212.14164 89.401942) (width 0.2) (layer F.Cu) (net 37))
  (segment (start 212.14164 89.401942) (end 210.82 88.080302) (width 0.2) (layer F.Cu) (net 37))
  (segment (start 210.82 88.080302) (end 210.82 82.55) (width 0.2) (layer F.Cu) (net 37))
  (segment (start 208.205 79.935) (end 205.105 79.935) (width 0.2) (layer F.Cu) (net 37) (status 20))
  (segment (start 210.82 82.55) (end 208.205 79.935) (width 0.2) (layer F.Cu) (net 37))
  (segment (start 256.469 127.04) (end 256.794 127.365) (width 0.2) (layer F.Cu) (net 38) (status 30))
  (segment (start 252.73 127.04) (end 256.469 127.04) (width 0.2) (layer F.Cu) (net 38) (status 30))
  (segment (start 262.636 94.25) (end 257.387932 89.001932) (width 0.2) (layer F.Cu) (net 39) (status 10))
  (segment (start 257.387932 89.001932) (end 212.307328 89.001932) (width 0.2) (layer F.Cu) (net 39))
  (segment (start 212.307328 89.001932) (end 211.22001 87.914614) (width 0.2) (layer F.Cu) (net 39))
  (segment (start 206.230699 77.395) (end 205.105 77.395) (width 0.2) (layer F.Cu) (net 39) (status 20))
  (segment (start 211.22001 82.384311) (end 206.230699 77.395) (width 0.2) (layer F.Cu) (net 39))
  (segment (start 211.22001 87.914614) (end 211.22001 82.384311) (width 0.2) (layer F.Cu) (net 39))
  (segment (start 264.089 127.04) (end 264.287 127.238) (width 0.2) (layer F.Cu) (net 40) (status 30))
  (segment (start 260.35 127.04) (end 264.089 127.04) (width 0.2) (layer F.Cu) (net 40) (status 30))
  (segment (start 179.884 110.236) (end 179.705 110.415) (width 0.2) (layer F.Cu) (net 41) (status 30))
  (segment (start 181.896 110.236) (end 179.884 110.236) (width 0.2) (layer F.Cu) (net 41) (status 30))
  (via (at 226.822 85.09) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 42))
  (segment (start 226.822 76.978) (end 226.822 85.09) (width 0.2) (layer F.Cu) (net 42))
  (segment (start 228.87 74.93) (end 226.822 76.978) (width 0.2) (layer F.Cu) (net 42) (status 10))
  (segment (start 226.822 85.09) (end 226.822 85.794302) (width 0.2) (layer B.Cu) (net 42))
  (segment (start 226.822 85.794302) (end 225.894312 86.72199) (width 0.2) (layer B.Cu) (net 42))
  (segment (start 225.894312 86.72199) (end 215.75399 86.72199) (width 0.2) (layer B.Cu) (net 42))
  (segment (start 213.929999 84.897999) (end 211.520001 84.897999) (width 0.2) (layer B.Cu) (net 42))
  (segment (start 215.75399 86.72199) (end 213.929999 84.897999) (width 0.2) (layer B.Cu) (net 42))
  (segment (start 211.520001 84.897999) (end 209.019989 87.398011) (width 0.2) (layer B.Cu) (net 42))
  (segment (start 209.019989 87.398011) (end 209.019989 100.860011) (width 0.2) (layer B.Cu) (net 42))
  (segment (start 207.085 102.795) (end 205.105 102.795) (width 0.2) (layer B.Cu) (net 42) (status 20))
  (segment (start 209.019989 100.860011) (end 207.085 102.795) (width 0.2) (layer B.Cu) (net 42))
  (segment (start 173.294 57.886) (end 176.57 54.61) (width 1.2) (layer F.Cu) (net 43) (status 20))
  (segment (start 173.294 59.968) (end 173.294 57.886) (width 1.2) (layer F.Cu) (net 43) (status 10))
  (segment (start 171.9365 73.5135) (end 171.77 73.68) (width 0.2) (layer F.Cu) (net 43) (status 30))
  (segment (start 171.9365 71.374) (end 171.9365 73.5135) (width 0.2) (layer F.Cu) (net 43) (status 30))
  (segment (start 171.577999 61.684001) (end 173.294 59.968) (width 0.2) (layer F.Cu) (net 43) (status 20))
  (segment (start 171.577999 71.015499) (end 171.577999 61.684001) (width 0.2) (layer F.Cu) (net 43) (status 10))
  (segment (start 171.9365 71.374) (end 171.577999 71.015499) (width 0.2) (layer F.Cu) (net 43) (status 30))
  (segment (start 179.07 57.11) (end 179.07 60.71799) (width 1.2) (layer F.Cu) (net 43) (status 30))
  (segment (start 176.57 54.61) (end 179.07 57.11) (width 1.2) (layer F.Cu) (net 43) (status 30))
  (segment (start 172.72 72.6655) (end 174.0115 71.374) (width 0.2) (layer F.Cu) (net 44) (status 20))
  (segment (start 172.72 73.68) (end 172.72 72.6655) (width 0.2) (layer F.Cu) (net 44) (status 10))
  (segment (start 176.26 71.374) (end 176.276 71.358) (width 0.2) (layer F.Cu) (net 44) (status 30))
  (segment (start 174.0115 71.374) (end 176.26 71.374) (width 0.2) (layer F.Cu) (net 44) (status 30))
  (segment (start 255.23 69.734) (end 255.23 54.61) (width 1.2) (layer B.Cu) (net 45) (status 20))
  (segment (start 252.73 72.234) (end 255.23 69.734) (width 1.2) (layer B.Cu) (net 45) (status 10))
  (segment (start 176.276 69.342) (end 176.276 69.358) (width 0.2) (layer F.Cu) (net 45) (status 30))
  (segment (start 191.008 54.61) (end 176.276 69.342) (width 0.2) (layer F.Cu) (net 45) (status 20))
  (via (at 221.234 54.61) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 45))
  (segment (start 255.23 54.61) (end 221.234 54.61) (width 0.2) (layer B.Cu) (net 45) (status 10))
  (via (at 214.122 54.356) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 45))
  (segment (start 214.376 54.61) (end 214.122 54.356) (width 0.2) (layer F.Cu) (net 45))
  (segment (start 221.234 54.61) (end 214.376 54.61) (width 0.2) (layer F.Cu) (net 45))
  (via (at 191.008 54.61) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 45))
  (segment (start 191.262 54.356) (end 191.008 54.61) (width 0.2) (layer B.Cu) (net 45))
  (segment (start 214.122 54.356) (end 191.262 54.356) (width 0.2) (layer B.Cu) (net 45))
  (via (at 171.45 77.724) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 46))
  (segment (start 171.77 77.404) (end 171.45 77.724) (width 0.2) (layer F.Cu) (net 46))
  (segment (start 171.77 76.18) (end 171.77 77.404) (width 0.2) (layer F.Cu) (net 46) (status 10))
  (segment (start 171.45 77.724) (end 171.45 62.484) (width 0.2) (layer B.Cu) (net 46))
  (segment (start 171.45 62.484) (end 172.466 61.468) (width 0.2) (layer B.Cu) (net 46))
  (via (at 176.784 59.944) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 46))
  (segment (start 173.99 59.944) (end 176.784 59.944) (width 0.2) (layer B.Cu) (net 46))
  (segment (start 172.466 61.468) (end 173.99 59.944) (width 0.2) (layer B.Cu) (net 46))
  (segment (start 175.218 59.944) (end 175.194 59.968) (width 0.2) (layer F.Cu) (net 46) (status 30))
  (segment (start 176.784 59.944) (end 175.218 59.944) (width 0.2) (layer F.Cu) (net 46) (status 20))
  (segment (start 173.72601 70.25801) (end 172.278 68.81) (width 0.2) (layer F.Cu) (net 47) (status 20))
  (segment (start 176.953824 70.25801) (end 173.72601 70.25801) (width 0.2) (layer F.Cu) (net 47))
  (segment (start 177.27601 70.580196) (end 176.953824 70.25801) (width 0.2) (layer F.Cu) (net 47))
  (segment (start 177.27601 72.57399) (end 177.27601 70.580196) (width 0.2) (layer F.Cu) (net 47))
  (segment (start 173.67 76.18) (end 177.27601 72.57399) (width 0.2) (layer F.Cu) (net 47) (status 10))
  (segment (start 173.228 63.984) (end 174.244 62.968) (width 1.2) (layer F.Cu) (net 48) (status 20))
  (segment (start 173.228 65.81) (end 173.228 63.984) (width 1.2) (layer F.Cu) (net 48) (status 10))
  (segment (start 241.38 78.639) (end 241.481 78.74) (width 0.5) (layer F.Cu) (net 49) (status 30))
  (segment (start 241.38 76.134) (end 241.38 78.639) (width 0.5) (layer F.Cu) (net 49) (status 30))
  (segment (start 243.456 78.74) (end 243.71 78.486) (width 1.2) (layer F.Cu) (net 49) (status 30))
  (segment (start 241.481 78.74) (end 243.456 78.74) (width 1.2) (layer F.Cu) (net 49) (status 30))
  (segment (start 201.26 104.1) (end 205.105 100.255) (width 0.2) (layer F.Cu) (net 50) (status 20))
  (segment (start 192.786 103.87) (end 192.786 104.06) (width 0.2) (layer F.Cu) (net 50) (status 30))
  (segment (start 192.746 104.1) (end 201.26 104.1) (width 0.2) (layer F.Cu) (net 50) (status 10))
  (segment (start 192.786 104.06) (end 192.746 104.1) (width 0.2) (layer F.Cu) (net 50) (status 30))
  (segment (start 173.99 104.1) (end 192.746 104.1) (width 0.2) (layer F.Cu) (net 50) (status 30))
  (segment (start 188.722 133.858) (end 188.595 133.985) (width 0.2) (layer F.Cu) (net 51) (status 30))
  (segment (start 188.722 130.952) (end 188.722 133.858) (width 0.2) (layer F.Cu) (net 51) (status 30))
  (segment (start 191.008 133.858) (end 191.135 133.985) (width 0.2) (layer F.Cu) (net 52) (status 30))
  (segment (start 191.008 131.302) (end 191.008 133.858) (width 0.2) (layer F.Cu) (net 52) (status 30))
  (segment (start 172.72 78.724) (end 172.736 78.74) (width 0.2) (layer F.Cu) (net 53) (status 30))
  (segment (start 172.72 76.18) (end 172.72 78.724) (width 0.2) (layer F.Cu) (net 53) (status 30))
  (segment (start 195.096 92.71) (end 195.096 95.226) (width 1.2) (layer F.Cu) (net 54) (status 10))
  (segment (start 193.04 97.282) (end 185.916009 97.282) (width 1.2) (layer F.Cu) (net 54) (status 20))
  (segment (start 195.096 95.226) (end 193.04 97.282) (width 1.2) (layer F.Cu) (net 54))
  (segment (start 194.096 93.71) (end 195.096 92.71) (width 0.2) (layer F.Cu) (net 54) (status 20))
  (segment (start 192.278 93.71) (end 194.096 93.71) (width 0.2) (layer F.Cu) (net 54) (status 10))
  (segment (start 211.3645 129.54) (end 210.82 128.9955) (width 0.2) (layer F.Cu) (net 55) (status 20))
  (segment (start 210.028 130.0415) (end 210.028 131.684) (width 0.2) (layer F.Cu) (net 55) (status 20))
  (segment (start 211.074 128.9955) (end 210.028 130.0415) (width 0.2) (layer F.Cu) (net 55) (status 10))
  (segment (start 205.105 82.475) (end 203.05399 84.52601) (width 0.2) (layer B.Cu) (net 56) (status 10))
  (segment (start 203.05399 95.846312) (end 201.337989 97.562312) (width 0.2) (layer B.Cu) (net 56))
  (segment (start 203.05399 84.52601) (end 203.05399 95.846312) (width 0.2) (layer B.Cu) (net 56))
  (segment (start 201.337989 102.699386) (end 202.90798 104.269377) (width 0.2) (layer B.Cu) (net 56))
  (segment (start 201.337989 97.562312) (end 201.337989 102.699386) (width 0.2) (layer B.Cu) (net 56))
  (segment (start 202.90798 104.269377) (end 202.90798 124.294312) (width 0.2) (layer B.Cu) (net 56))
  (via (at 200.214 128.016) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 56))
  (segment (start 200.214 126.988292) (end 200.214 128.016) (width 0.2) (layer B.Cu) (net 56))
  (segment (start 202.90798 124.294312) (end 200.214 126.988292) (width 0.2) (layer B.Cu) (net 56))
  (segment (start 200.214 128.016) (end 189.484 128.016) (width 0.2) (layer F.Cu) (net 56))
  (segment (start 188.722 128.778) (end 188.722 129.652) (width 0.2) (layer F.Cu) (net 56) (status 20))
  (segment (start 189.484 128.016) (end 188.722 128.778) (width 0.2) (layer F.Cu) (net 56))
  (via (at 200.914 129.286) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 57))
  (segment (start 200.898 129.302) (end 200.914 129.286) (width 0.2) (layer F.Cu) (net 57))
  (segment (start 191.008 129.302) (end 200.898 129.302) (width 0.2) (layer F.Cu) (net 57) (status 10))
  (segment (start 200.914 129.286) (end 200.914 126.85399) (width 0.2) (layer B.Cu) (net 57))
  (segment (start 200.914 126.85399) (end 203.30799 124.46) (width 0.2) (layer B.Cu) (net 57))
  (segment (start 201.737999 102.533697) (end 201.737999 97.728001) (width 0.2) (layer B.Cu) (net 57))
  (segment (start 203.30799 104.103688) (end 201.737999 102.533697) (width 0.2) (layer B.Cu) (net 57))
  (segment (start 203.30799 124.46) (end 203.30799 104.103688) (width 0.2) (layer B.Cu) (net 57))
  (segment (start 201.737999 97.728001) (end 203.454 96.012) (width 0.2) (layer B.Cu) (net 57))
  (segment (start 203.454 86.666) (end 205.105 85.015) (width 0.2) (layer B.Cu) (net 57) (status 20))
  (segment (start 203.454 96.012) (end 203.454 86.666) (width 0.2) (layer B.Cu) (net 57))
  (segment (start 241.7 73.914) (end 241.38 74.234) (width 0.2) (layer F.Cu) (net 58) (status 20))
  (segment (start 246.38 71.136) (end 244.094 71.136) (width 0.2) (layer F.Cu) (net 58) (status 30))
  (segment (start 244.094 71.136) (end 242.824 72.406) (width 0.2) (layer F.Cu) (net 58) (status 10))
  (segment (start 242.824 72.79) (end 241.38 74.234) (width 0.2) (layer F.Cu) (net 58) (status 20))
  (segment (start 242.824 72.406) (end 242.824 72.79) (width 0.2) (layer F.Cu) (net 58))
  (segment (start 216.916 103.4145) (end 216.916 101.33) (width 0.2) (layer F.Cu) (net 59) (status 30))
  (segment (start 224.282 101.33) (end 224.282 103.378) (width 0.2) (layer F.Cu) (net 60) (status 30))
  (segment (start 247.396 103.4145) (end 247.396 101.33) (width 0.2) (layer F.Cu) (net 61) (status 30))
  (segment (start 231.902 103.378) (end 231.902 101.346) (width 0.2) (layer F.Cu) (net 62) (status 30))
  (segment (start 255.27 101.33) (end 255.27 103.4145) (width 0.2) (layer F.Cu) (net 63) (status 30))
  (segment (start 239.776 101.346) (end 239.776 103.378) (width 0.2) (layer F.Cu) (net 64) (status 30))
  (segment (start 262.636 101.314) (end 262.636 103.4145) (width 0.2) (layer F.Cu) (net 65) (status 30))
  (segment (start 210.82 107.934) (end 210.82 110.0185) (width 0.2) (layer F.Cu) (net 66) (status 30))
  (segment (start 214.818 96.316) (end 214.868 96.266) (width 0.2) (layer F.Cu) (net 67) (status 30))
  (segment (start 214.818 98.576) (end 214.818 96.316) (width 0.2) (layer F.Cu) (net 67) (status 30))
  (segment (start 216.9 96.266) (end 216.916 96.25) (width 0.2) (layer F.Cu) (net 67) (status 30))
  (segment (start 214.868 96.266) (end 216.9 96.266) (width 0.2) (layer F.Cu) (net 67) (status 30))
  (segment (start 222.184 96.316) (end 222.234 96.266) (width 0.2) (layer F.Cu) (net 68) (status 30))
  (segment (start 222.184 98.576) (end 222.184 96.316) (width 0.2) (layer F.Cu) (net 68) (status 30))
  (segment (start 222.234 96.266) (end 224.282 96.266) (width 0.2) (layer F.Cu) (net 68) (status 30))
  (segment (start 245.348 98.526) (end 245.298 98.576) (width 0.2) (layer F.Cu) (net 69) (status 30))
  (segment (start 245.348 96.266) (end 245.348 98.526) (width 0.2) (layer F.Cu) (net 69) (status 30))
  (segment (start 247.38 96.266) (end 247.396 96.25) (width 0.2) (layer F.Cu) (net 69) (status 30))
  (segment (start 245.348 96.266) (end 247.38 96.266) (width 0.2) (layer F.Cu) (net 69) (status 30))
  (segment (start 229.838 96.266) (end 231.902 96.266) (width 0.2) (layer F.Cu) (net 70) (status 30))
  (segment (start 229.838 98.542) (end 229.804 98.576) (width 0.2) (layer F.Cu) (net 70) (status 30))
  (segment (start 229.838 96.266) (end 229.838 98.542) (width 0.2) (layer F.Cu) (net 70) (status 30))
  (segment (start 253.172 96.316) (end 253.222 96.266) (width 0.2) (layer F.Cu) (net 71) (status 30))
  (segment (start 253.172 98.576) (end 253.172 96.316) (width 0.2) (layer F.Cu) (net 71) (status 30))
  (segment (start 255.254 96.266) (end 255.27 96.25) (width 0.2) (layer F.Cu) (net 71) (status 30))
  (segment (start 253.222 96.266) (end 255.254 96.266) (width 0.2) (layer F.Cu) (net 71) (status 30))
  (segment (start 200.61 93.66) (end 200.66 93.71) (width 0.2) (layer F.Cu) (net 72) (status 30))
  (segment (start 198.096 93.66) (end 200.61 93.66) (width 0.2) (layer F.Cu) (net 72) (status 30))
  (segment (start 198.096 95.496) (end 198.374 95.774) (width 0.2) (layer F.Cu) (net 72) (status 30))
  (segment (start 198.096 93.66) (end 198.096 95.496) (width 0.2) (layer F.Cu) (net 72) (status 30))
  (segment (start 237.712 96.266) (end 239.776 96.266) (width 0.2) (layer F.Cu) (net 73) (status 30))
  (segment (start 237.712 98.542) (end 237.678 98.576) (width 0.2) (layer F.Cu) (net 73) (status 30))
  (segment (start 237.712 96.266) (end 237.712 98.542) (width 0.2) (layer F.Cu) (net 73) (status 30))
  (segment (start 262.62 96.266) (end 262.636 96.25) (width 0.2) (layer F.Cu) (net 74) (status 30))
  (segment (start 260.572 96.266) (end 262.62 96.266) (width 0.2) (layer F.Cu) (net 74) (status 30))
  (segment (start 260.572 98.542) (end 260.538 98.576) (width 0.2) (layer F.Cu) (net 74) (status 30))
  (segment (start 260.572 96.266) (end 260.572 98.542) (width 0.2) (layer F.Cu) (net 74) (status 30))
  (segment (start 245.848 81.534) (end 246.126 81.812) (width 0.2) (layer F.Cu) (net 75) (status 30))
  (segment (start 243.316 81.534) (end 245.848 81.534) (width 0.2) (layer F.Cu) (net 75) (status 30))
  (segment (start 245.126 84.862) (end 245.176 84.812) (width 0.2) (layer F.Cu) (net 76) (status 30))
  (segment (start 245.152 84.836) (end 245.176 84.812) (width 0.2) (layer F.Cu) (net 76) (status 30))
  (segment (start 243.316 84.836) (end 245.152 84.836) (width 0.2) (layer F.Cu) (net 76) (status 30))
  (via (at 242.316 83.058) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 76))
  (segment (start 243.316 84.058) (end 242.316 83.058) (width 0.2) (layer F.Cu) (net 76))
  (segment (start 243.316 84.836) (end 243.316 84.058) (width 0.2) (layer F.Cu) (net 76) (status 10))
  (segment (start 235.596009 88.022009) (end 235.204 87.63) (width 0.2) (layer B.Cu) (net 76))
  (segment (start 241.672797 88.022009) (end 235.596009 88.022009) (width 0.2) (layer B.Cu) (net 76))
  (via (at 235.204 87.63) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 76))
  (segment (start 242.316 87.378806) (end 241.672797 88.022009) (width 0.2) (layer B.Cu) (net 76))
  (segment (start 242.316 83.058) (end 242.316 87.378806) (width 0.2) (layer B.Cu) (net 76))
  (segment (start 235.204 87.63) (end 234.696 88.138) (width 0.2) (layer F.Cu) (net 76))
  (via (at 212.344 87.122) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 76))
  (segment (start 213.36 88.138) (end 212.344 87.122) (width 0.2) (layer F.Cu) (net 76))
  (segment (start 234.696 88.138) (end 213.36 88.138) (width 0.2) (layer F.Cu) (net 76))
  (via (at 210.12 102.616) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 76))
  (segment (start 210.12 89.346) (end 210.12 102.616) (width 0.2) (layer B.Cu) (net 76))
  (segment (start 212.344 87.122) (end 210.12 89.346) (width 0.2) (layer B.Cu) (net 76))
  (segment (start 206.844312 122.02799) (end 203.30799 122.02799) (width 0.2) (layer F.Cu) (net 76))
  (segment (start 209.24498 119.627322) (end 206.844312 122.02799) (width 0.2) (layer F.Cu) (net 76))
  (segment (start 209.24498 103.49102) (end 209.24498 119.627322) (width 0.2) (layer F.Cu) (net 76))
  (segment (start 203.30799 122.02799) (end 201.93 120.65) (width 0.2) (layer F.Cu) (net 76))
  (segment (start 210.12 102.616) (end 209.24498 103.49102) (width 0.2) (layer F.Cu) (net 76))
  (segment (start 183.896 110.236) (end 183.896 114.3) (width 0.2) (layer F.Cu) (net 76) (status 10))
  (segment (start 183.896 114.3) (end 186.436 116.84) (width 0.2) (layer F.Cu) (net 76))
  (segment (start 186.436 116.84) (end 199.644 116.84) (width 0.2) (layer F.Cu) (net 76))
  (segment (start 199.644 116.84) (end 201.93 119.126) (width 0.2) (layer F.Cu) (net 76))
  (segment (start 201.93 120.65) (end 201.93 119.126) (width 0.2) (layer F.Cu) (net 76))
  (segment (start 228.87 83.78) (end 229.87 82.78) (width 0.2) (layer F.Cu) (net 77) (status 20))
  (segment (start 228.87 85.598) (end 228.87 83.78) (width 0.2) (layer F.Cu) (net 77) (status 10))
  (segment (start 230.87 79.73) (end 230.82 79.78) (width 0.2) (layer F.Cu) (net 78) (status 30))
  (segment (start 230.87 74.93) (end 230.87 79.73) (width 0.2) (layer F.Cu) (net 78) (status 30))
  (segment (start 237.302 87.072) (end 237.252 87.122) (width 1.2) (layer F.Cu) (net 79) (status 30))
  (segment (start 237.252 84.862) (end 237.302 84.812) (width 0.2) (layer F.Cu) (net 79) (status 30))
  (segment (start 237.252 87.122) (end 237.252 84.862) (width 0.2) (layer F.Cu) (net 79) (status 30))
  (segment (start 240.58 81.534) (end 241.316 81.534) (width 0.2) (layer F.Cu) (net 79) (status 20))
  (segment (start 237.302 84.812) (end 240.58 81.534) (width 0.2) (layer F.Cu) (net 79) (status 10))
  (segment (start 232.984 85.548) (end 232.934 85.598) (width 0.2) (layer F.Cu) (net 80) (status 30))
  (segment (start 232.984 83.288) (end 232.984 85.548) (width 0.2) (layer F.Cu) (net 80) (status 30))
  (segment (start 232.934 85.598) (end 230.87 85.598) (width 0.2) (layer F.Cu) (net 80) (status 30))
  (segment (start 210.3325 126.762) (end 211.074 126.0205) (width 0.2) (layer F.Cu) (net 81) (status 20))
  (segment (start 208.788 126.762) (end 210.3325 126.762) (width 0.2) (layer F.Cu) (net 81) (status 10))
  (segment (start 173.99 88.86) (end 176.57 91.44) (width 0.2) (layer F.Cu) (net 82) (status 10))
  (segment (start 181.722 91.44) (end 184.516 94.234) (width 0.2) (layer F.Cu) (net 82) (status 20))
  (segment (start 176.57 91.44) (end 181.722 91.44) (width 0.2) (layer F.Cu) (net 82))

  (zone (net 7) (net_name GND) (layer F.Cu) (tstamp 5FC46F5C) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 273.812 159.512) (xy 153.67 151.384) (xy 166.116 32.258) (xy 275.336 27.94)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer B.Cu) (tstamp 5FC46F59) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 279.654 153.67) (xy 135.382 153.162) (xy 150.876 35.052) (xy 278.638 31.496)
      )
    )
  )
)
