(module 4056E_LiIon_loader_SMT (layer F.Cu) (tedit 569E2953)
  (fp_text reference M1 (at -1.266 1.13) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 4056E_Loader_prot (at 0.66 -3.46) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -13.29 8.5) (end 12.7 8.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -13.3 -8.5) (end 12.7 -8.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -13.87 3.26) (end -13.87 -3.29) (layer F.SilkS) (width 0.15))
  (fp_text user microUSB (at -9.538 -0.014 180) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -13.856 3.288) (end -13.348 3.288) (layer F.SilkS) (width 0.15))
  (fp_line (start -13.348 3.288) (end -13.094 2.78) (layer F.SilkS) (width 0.15))
  (fp_line (start -13.094 2.78) (end -12.84 2.78) (layer F.SilkS) (width 0.15))
  (fp_line (start -13.856 -3.316) (end -13.348 -3.316) (layer F.SilkS) (width 0.15))
  (fp_line (start -13.348 -3.316) (end -13.094 -2.808) (layer F.SilkS) (width 0.15))
  (fp_line (start -13.094 -2.808) (end -8.268 -2.808) (layer F.SilkS) (width 0.15))
  (fp_line (start -8.268 -2.808) (end -8.268 2.78) (layer F.SilkS) (width 0.15))
  (fp_line (start -8.268 2.78) (end -12.84 2.78) (layer F.SilkS) (width 0.15))
  (fp_text user B- (at 10.674 1.29) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user B+ (at 10.674 -2.012) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user OUT- (at 7.19 6.556) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user OUT+ (at 6.87 -6.348) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user IN- (at -6.9 6.76) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user IN+ (at -7.43 -6.13) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -13.296 8.5) (end -13.296 -8.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.706 -8.5) (end 12.706 8.5) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -11 -6.75) (size 3 3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -11 6.75) (size 3 3) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 11 7) (size 3 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 11 -7) (size 3 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 11 -3.75) (size 3 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 11 3.75) (size 3 2.5) (layers F.Cu F.Paste F.Mask))
)
