(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "CN61CN33" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "CN61CN33" (at 5.08 10.16 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (at 7.62 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm809.pdf" (at 7.62 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "reset supervisor" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microprocessor Reset (active-low) Circuit, SOT-23" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "CN61CN33_0_1"
      (rectangle (start 5.08 7.62) (end -5.08 -7.62)
        (stroke (width 0.254) (type solid))
        (fill (type background))
      )
    )
    (symbol "CN61CN33_1_1"
      (pin output line (at 0 -10.16 90) (length 2.54)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 0 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 10.16 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "DS2438" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "DS2438" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "DS2438_0_1"
      (rectangle (start -11.43 -2.54) (end 12.7 -30.48)
        (stroke (width 0) (type solid))
        (fill (type background))
      )
    )
    (symbol "DS2438_1_1"
      (pin power_in line (at -13.97 -6.35 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at -13.97 -12.7 0) (length 2.54)
        (name "Vsens+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at -13.97 -19.05 0) (length 2.54)
        (name "Vsense-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 -25.4 0) (length 2.54)
        (name "Vad" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 15.24 -25.4 180) (length 2.54)
        (name "Vdd" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 15.24 -19.05 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 15.24 -12.7 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -6.35 180) (length 2.54)
        (name "DQ" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "DW01" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "IC" (at 21.59 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "DW01" (at 21.59 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "SOT95P280X135-6N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "HEIGHT" "1.35mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "DESCRIPTION" "ic" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MANUFACTURER_PART_NUMBER" "DW01" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MANUFACTURER_NAME" "Slkor" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "DW01_0_0"
      (polyline
        (pts
          (xy 5.08 2.54)
          (xy 5.08 -7.62)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 2.54)
          (xy 20.32 2.54)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 20.32 -7.62)
          (xy 5.08 -7.62)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 20.32 -7.62)
          (xy 20.32 2.54)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (pin bidirectional line (at 0 0 0) (length 5.08)
        (name "OD" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 0 -2.54 0) (length 5.08)
        (name "CSI" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 0 -5.08 0) (length 5.08)
        (name "OC" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -5.08 180) (length 5.08)
        (name "TD" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -2.54 180) (length 5.08)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 0 180) (length 5.08)
        (name "VSS" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
