(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "ESP32-C6-WROOM-1-N8"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 23.622 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "ESP32-C6-WROOM-1-N8"
			(at -15.24 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "ESP32-C6-WROOM-1-N8:XCVR_ESP32-C6-WROOM-1-N8"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "MF" "Espressif Systems"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.25mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "Package" "None"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "Price" "None"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/ESP32-C6-WROOM-1-N8/Espressif+Systems/view-part/?ref=eda"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "PARTREV" "1.0"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/ESP32-C6-WROOM-1-N8/Espressif+Systems/view-part/?ref=snap"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "MP" "ESP32-C6-WROOM-1-N8"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=12616380&manufacturer=Espressif Systems&part_name=ESP32-C6-WROOM-1-N8&search_term=None"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "Description_1" "\nMultiprotocol Modules ESP32-C6 module, Wi-Fi 6 in 2.4 GHz band, Bluetooth 5, Zigbee 3.0 and Thread. ESP34-WROOM Compatible - ENGINEERING SAMPLE\n"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "MANUFACTURER" "Espressif Systems"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(symbol "ESP32-C6-WROOM-1-N8_0_0"
			(rectangle
				(start -15.24 -22.86)
				(end 15.24 22.86)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "IO8"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "IO10"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "IO11"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "IO12"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "IO13"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "IO9"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "IO18"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "IO19"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "IO20"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "IO21"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "3V3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "IO22"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "IO23"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin no_connect line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "NC"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "IO15"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "RXD0/GPIO17"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "TXD0/GPIO16"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "IO3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "IO2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "29_1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "29_2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "29_3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "29_4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "29_5"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "29_6"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "29_7"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "29_8"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "29_9"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "EN"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "IO4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "IO5"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "IO6"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "IO7"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "IO0"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "IO1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
		)
		(symbol "ESP32-C6-WROOM-1-N8_1_0"
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "30_1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "30_10"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "30_11"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "30_12"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "30_2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "30_3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "30_4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "30_5"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "30_6"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "30_7"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "30_8"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "30_9"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
		)
	)
)
