(footprint "AMASS_XT30UPB+DATA-M_1x02_P5.0mm_Vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Connector XT30 Vertical PCB Male, https://www.tme.eu/en/Document/4acc913878197f8c2e30d4b8cdc47230/XT30UPB%20SPEC.pdf")
	(tags "RC Connector XT30")
	(property "Reference" "REF**"
		(at 2.5 -4 0)
		(layer "F.SilkS")
		(uuid "f7510d54-dcb1-4c3b-b842-cd250a98370c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "AMASS_XT30UPB+DATA-M_1x02_P5.0mm_Vertical"
		(at 2.5 4 0)
		(layer "F.Fab")
		(uuid "c5a8a60c-4ea1-4401-a30c-34d36be61c07")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8fb27306-c085-4316-b554-4ba9be794054")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "74b71861-05d2-4229-8e81-25952aaaef7e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a1d16ecc-7e64-48c4-b772-a9255380960d")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -2.71 -1.41)
		(end -2.71 1.41)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e96c6ad2-9ca6-4df1-b35b-76e090d7ff4e")
	)
	(fp_line
		(start -2.71 -1.41)
		(end -1.01 -2.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0784d204-0a48-4a2b-8085-50e1ff7a1493")
	)
	(fp_line
		(start -2.71 1.41)
		(end -1.01 2.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "db750970-e424-4a8e-a882-20a90baabffc")
	)
	(fp_line
		(start -1.01 -2.71)
		(end 7.71 -2.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9f23420e-db87-438c-a708-676a0616966e")
	)
	(fp_line
		(start -1.01 2.71)
		(end 7.71 2.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2ba574e3-9de5-4d7d-9777-e19e6fa702e7")
	)
	(fp_line
		(start 7.71 -2.71)
		(end 7.71 2.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2018cc6b-6115-4763-8b7c-54b60affbda7")
	)
	(fp_rect
		(start -6.3 -2.71)
		(end 7.71 2.7)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "11aac399-c862-4b67-9828-087abeea5b1b")
	)
	(fp_line
		(start -3.1 -1.8)
		(end -3.1 1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "06ae69d8-1372-4524-8b1a-27a2f062f1c5")
	)
	(fp_line
		(start -3.1 -1.8)
		(end -1.4 -3.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ae869a92-c688-4f2b-82ca-0578106a035a")
	)
	(fp_line
		(start -3.1 1.8)
		(end -1.4 3.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "cac6d927-6ba1-4095-825b-f94ee0d7abe9")
	)
	(fp_line
		(start -1.4 -3.1)
		(end 8.1 -3.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fb4fa373-5492-4717-a9fe-7b69f4c53ba0")
	)
	(fp_line
		(start -1.4 3.1)
		(end 8.1 3.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "70296c77-546d-44a2-b5d3-e6dc58cf713b")
	)
	(fp_line
		(start 8.1 -3.1)
		(end 8.1 3.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "64764a09-de32-4f35-b54a-17e44810370f")
	)
	(fp_line
		(start -2.6 -1.3)
		(end -2.6 1.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8d7ee7cb-5dda-453f-aa9a-6420c87f1b8e")
	)
	(fp_line
		(start -2.6 -1.3)
		(end -0.9 -2.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2fa3ad90-36bb-4374-95ed-e44e50c7e385")
	)
	(fp_line
		(start -2.6 1.3)
		(end -0.9 2.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2e4f8556-ffc2-4791-91da-e68c3513337e")
	)
	(fp_line
		(start -0.9 -2.6)
		(end 7.6 -2.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cb9cd8af-1997-41db-b9fe-8982960ac6db")
	)
	(fp_line
		(start -0.9 2.6)
		(end 7.6 2.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ea8a6c02-e974-4677-a854-a0891c323245")
	)
	(fp_line
		(start 7.6 -2.6)
		(end 7.6 2.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c66f305c-0d56-4591-bc02-23252ad20321")
	)
	(fp_text user "-"
		(at -4 0 0)
		(layer "F.SilkS")
		(uuid "c119570a-6846-48dc-9422-0b5665ab2df6")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "+"
		(at 9 0 0)
		(layer "F.SilkS")
		(uuid "d6ab678c-47f7-47e0-869b-ef3b9dbd1ba9")
		(effects
			(font
				(size 1.5 1.5)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 2.5 0 0)
		(layer "F.Fab")
		(uuid "a70efd12-1491-4664-ae98-5b2b7f52a502")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3a0f3b23-814b-4df9-a02c-3d9fed9e23c9")
	)
	(pad "2" thru_hole circle
		(at 5 0)
		(size 3 3)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d897d74a-a13b-47cf-9806-eb8a75fe8d08")
	)
	(pad "3" thru_hole circle
		(at -3.9 -1)
		(size 1.524 1.524)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "02a8c3fc-d75c-47a4-a907-f9191ff19e2c")
	)
	(pad "4" thru_hole circle
		(at -3.9 1)
		(size 1.524 1.524)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2000b5b8-f7c9-40a8-9010-65c16d2aefce")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_AMASS.3dshapes/AMASS_XT30UPB-M_1x02_P5.0mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
