(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "SX1308" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -17.78 20.32 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "SX1308" (at -17.8054 17.8054 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "SOT-23-6" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "SX1308_0_0"
      (polyline
        (pts
          (xy -17.78 -7.62)
          (xy -17.78 15.24)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -17.78 15.24)
          (xy 0 15.24)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -13.7922 0.1778)
          (xy -11.2522 0.1778)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -11.303 1.6764)
          (xy -8.763 1.6764)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -11.2522 0.1778)
          (xy -11.303 1.6764)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -7.62)
          (xy -17.78 -7.62)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 15.24)
          (xy 0 -7.62)
        )
        (stroke (width 0.254) (type solid))
        (fill (type none))
      )
      (text "ON/OFF" (at -10.8712 -0.0508 0)
        (effects (font (size 0.8128 0.8128)) (justify left bottom))
      )
      (pin bidirectional line (at 5.08 12.7 180) (length 5.08)
        (name "SW" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 -5.08 0) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 5.08 -2.54 180) (length 5.08)
        (name "FB" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 2.54 0) (length 5.08)
        (name "EN" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 12.7 0) (length 5.08)
        (name "IN" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 5.08 5.08 180) (length 5.08)
        (name "N/C" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
